GENERAL REMARKS

1)MONITORING SUBSYSTEM IS NOW A SEPERATE ASSEMBLY CONSISTING OF 3 SUBASSEMBLIES (MCAMM, MCALM, MCADM)
2)THE BUSSES IN ALL MODULES THAT CONNECT COMPONENTS TO THE SWITCHES IN THE MCA SUBASSEMBLIES
ARE NAMED MCA_SWITCH_BUS.




DRIVER MODULE

1)REMOVED POTENSIOMETER R1 10K. CLOCK FIXED TO 1MHz.
2)REMOVED POTENSIOMETER R86 10K. CLOCK FIXED TO 1MHz.



LOGIC MODULE

1) -


MEMORY MODULE

1) -


INTERFACE MODULE / DSKY

1)ADDED PRO KEY (SW19 & R1 1K) CONNECTED TO CON18 PIN 19
2)ADDED THE FOLLOWING CAUTION & STATUS INDICATORS:

TEMP
AUTO
GIMBAL LOCK
HOLD
FREE
RESTART
NO ATT
TRACKER

3)CHANGED THE +/- LOGIC IN DISPLAY (DSP) #11. REMOVED U25x HEX INVERTERS,
REPLACED 74LS02 WITH 74LS32 AND RECONFIGURED THE CONNECTIONS SO THAT WHEN
+ IS PRESSED ALL M,S,U,P SEGMENTS ARE LIT WHILE WHEN - IS PRESSED ONLY U,P
SEGMENTS ARE LIT (PSA05-12GWA)
4)CHANGED THE VALUE OF R55x CURRENT LIMITING RESISTORS FROM 330 Ohm TO 1 Ohm. 
