(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (title_block
    (title "Solid-state circuit breaker with definite-time overcurrent trip")
    (date "2022-10-14")
    (rev "0")
  )
  (lib_symbols
    (symbol "4xxx:4011" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 1.27 0))
      (property "Value" "4011" (at 0 -1.27 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "CMOS Nand2" (at 0 0 0))
      (property "ki_description" "Quad Nand 2 inputs" (at 0 0 0))
      (property "ki_fp_filters" "DIP?14*" (at 0 0 0))
      (symbol "4011_1_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "4011_1_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "1")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "2")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "4011_2_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "4011_2_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "5")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "6")
        )
      )
      (symbol "4011_3_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "4011_3_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "8")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "9")
        )
      )
      (symbol "4011_4_1"
        (arc (start 0 -3.81) (mid 3.7934 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "4011_4_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1842 -2.5851) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1915 2.5936) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "12")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "13")
        )
      )
      (symbol "4011_5_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VDD")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "VSS")
          (number "7")
        )
      )
      (symbol "4011_5_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "Comparator:LM339" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.08 0))
      (property "Value" "LM339" (at 0 -5.08 0))
      (property "Footprint" "" (at -1.27 2.54 0))
      (property "Datasheet" "https://www.st.com/resource/en/datasheet/lm139.pdf" (at 1.27 5.08 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_keywords" "cmp open collector" (at 0 0 0))
      (property "ki_description" "Quad Differential Comparators, SOIC-14/TSSOP-14" (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*" (at 0 0 0))
      (symbol "LM339_1_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy 3.302 -0.508)
            (xy 2.794 -0.508)
            (xy 3.302 0)
            (xy 2.794 0.508)
            (xy 2.286 0)
            (xy 2.794 -0.508)
            (xy 2.286 -0.508)
          )
          (fill (type none))
        )
        (pin open_collector line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "4")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "5")
        )
      )
      (symbol "LM339_2_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy 3.302 -0.508)
            (xy 2.794 -0.508)
            (xy 3.302 0)
            (xy 2.794 0.508)
            (xy 2.286 0)
            (xy 2.794 -0.508)
            (xy 2.286 -0.508)
          )
          (fill (type none))
        )
        (pin open_collector line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "6")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "7")
        )
      )
      (symbol "LM339_3_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy 3.302 -0.508)
            (xy 2.794 -0.508)
            (xy 3.302 0)
            (xy 2.794 0.508)
            (xy 2.286 0)
            (xy 2.794 -0.508)
            (xy 2.286 -0.508)
          )
          (fill (type none))
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "10")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "11")
        )
        (pin open_collector line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "13")
        )
      )
      (symbol "LM339_4_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy 3.302 -0.508)
            (xy 2.794 -0.508)
            (xy 3.302 0)
            (xy 2.794 0.508)
            (xy 2.286 0)
            (xy 2.794 -0.508)
            (xy 2.286 -0.508)
          )
          (fill (type none))
        )
        (pin open_collector line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "14")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "8")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "9")
        )
      )
      (symbol "LM339_5_1"
        (pin power_in line (at -2.54 -7.62 90) (length 3.81)
          (name "V-")
          (number "12")
        )
        (pin power_in line (at -2.54 7.62 270) (length 3.81)
          (name "V+")
          (number "3")
        )
      )
    )
    (symbol "Connector_Generic:Conn_01x01" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 2.54 0))
      (property "Value" "Conn_01x01" (at 0 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "connector" (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)" (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (at 0 0 0))
      (symbol "Conn_01x01_1_1"
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 1.27) (end 1.27 -1.27)
          (fill (type background))
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.254 1.778 0))
      (property "Value" "C_Small" (at 0.254 -2.032 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Potentiometer_US" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RV" (at -4.445 0 90))
      (property "Value" "R_Potentiometer_US" (at -2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "resistor variable" (at 0 0 0))
      (property "ki_description" "Potentiometer, US symbol" (at 0 0 0))
      (property "ki_fp_filters" "Potentiometer*" (at 0 0 0))
      (symbol "R_Potentiometer_US_0_1"
        (polyline
          (pts
            (xy 0 -2.286)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.524 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.143 0)
            (xy 2.286 0.508)
            (xy 2.286 -0.508)
            (xy 1.143 0)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 1.016 -1.143)
            (xy 0 -1.524)
            (xy -1.016 -1.905)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 1.016 0.381)
            (xy 0 0)
            (xy -1.016 -0.381)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 1.016 1.905)
            (xy 0 1.524)
            (xy -1.016 1.143)
            (xy 0 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "R_Potentiometer_US_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "3")
          (number "3")
        )
      )
    )
    (symbol "Device:R_US" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.54 0 90))
      (property "Value" "R_US" (at -2.54 0 90))
      (property "Footprint" "" (at 1.016 -0.254 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor, US symbol" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_US_0_1"
        (polyline
          (pts
            (xy 0 -2.286)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 1.016 -1.143)
            (xy 0 -1.524)
            (xy -1.016 -1.905)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 1.016 0.381)
            (xy 0 0)
            (xy -1.016 -0.381)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 1.016 1.905)
            (xy 0 1.524)
            (xy -1.016 1.143)
            (xy 0 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "R_US_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "LED:CQY99" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (at 0.508 1.778 0))
      (property "Value" "CQY99" (at -1.016 -2.794 0))
      (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (at 0 4.445 0))
      (property "Datasheet" "https://www.prtice.info/IMG/pdf/CQY99.pdf" (at -1.27 0 0))
      (property "ki_keywords" "IR LED" (at 0 0 0))
      (property "ki_description" "950nm IR-LED, 5mm" (at 0 0 0))
      (property "ki_fp_filters" "LED*5.0mm*IRGrey*" (at 0 0 0))
      (symbol "CQY99_0_1"
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.381 3.175)
            (xy -0.127 3.175)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.143 1.651)
            (xy 0.381 3.175)
            (xy 0.381 2.667)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -1.27)
            (xy -2.54 0)
            (xy 0 1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.413 1.651)
            (xy -0.889 3.175)
            (xy -0.889 2.667)
            (xy -0.889 3.175)
            (xy -1.397 3.175)
          )
          (fill (type none))
        )
      )
      (symbol "CQY99_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Power_MOSFET_FDA59N30:FDA59N30" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 20.32 10.16 0))
      (property "Value" "FDA59N30" (at 20.32 7.62 0))
      (property "Footprint" "TO-3PN_20P10X16P20_ONS" (at 20.32 6.096 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_locked" "" (at 0 0 0))
      (property "ki_fp_filters" "TO-3PN_20P10X16P20_ONS" (at 0 0 0))
      (symbol "FDA59N30_1_1"
        (polyline
          (pts
            (xy 7.62 -7.62)
            (xy 33.02 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 5.08)
            (xy 7.62 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 33.02 -7.62)
            (xy 33.02 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 33.02 5.08)
            (xy 7.62 5.08)
          )
          (fill (type none))
        )
        (pin unspecified line (at 0 0 0) (length 7.62)
          (name "G")
          (number "1")
        )
        (pin unspecified line (at 40.64 -2.54 180) (length 7.62)
          (name "D")
          (number "2")
        )
        (pin unspecified line (at 40.64 0 180) (length 7.62)
          (name "S")
          (number "3")
        )
      )
    )
    (symbol "Regulator_Linear:L7805" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -3.81 3.175 0))
      (property "Value" "L7805" (at 0 3.175 0))
      (property "Footprint" "" (at 0.635 -3.81 0))
      (property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf" (at 0 -1.27 0))
      (property "ki_keywords" "Voltage Regulator 1.5A Positive" (at 0 0 0))
      (property "ki_description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252" (at 0 0 0))
      (property "ki_fp_filters" "TO?252* TO?263* TO?220*" (at 0 0 0))
      (symbol "L7805_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "L7805_1_1"
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "IN")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "OUT")
          (number "3")
        )
      )
    )
    (symbol "Switch:SW_Push" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 1.27 2.54 0))
      (property "Value" "SW_Push" (at 0 -1.524 0))
      (property "Footprint" "" (at 0 5.08 0))
      (property "Datasheet" "~" (at 0 5.08 0))
      (property "ki_keywords" "switch normally-open pushbutton push-button" (at 0 0 0))
      (property "ki_description" "Push button switch, generic, two pins" (at 0 0 0))
      (symbol "SW_Push_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:+9V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+9V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+9V\"" (at 0 0 0))
      (symbol "+9V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+9V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+9V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 66.04 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 109.22 151.13) (diameter 0) (color 0 0 0 0))
  (junction (at 39.37 144.78) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 38.1) (diameter 0) (color 0 0 0 0))
  (junction (at 24.13 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 212.09 91.44) (diameter 0) (color 0 0 0 0))
  (junction (at 77.47 92.71) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 74.93) (diameter 0) (color 0 0 0 0))
  (junction (at 83.82 35.56) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 149.86) (diameter 0) (color 0 0 0 0))
  (junction (at 66.04 162.56) (diameter 0) (color 0 0 0 0))
  (junction (at 105.41 160.02) (diameter 0) (color 0 0 0 0))
  (junction (at 39.37 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 82.55 41.91) (diameter 0) (color 0 0 0 0))
  (junction (at 139.7 57.15) (diameter 0) (color 0 0 0 0))
  (junction (at 166.37 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 101.6 35.56) (diameter 0) (color 0 0 0 0))
  (junction (at 93.98 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 146.05 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 139.7) (diameter 0) (color 0 0 0 0))
  (junction (at 27.94 72.39) (diameter 0) (color 0 0 0 0))
  (junction (at 120.65 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 49.53 72.39) (diameter 0) (color 0 0 0 0))
  (no_connect (at 91.44 83.82))
  (no_connect (at 101.6 45.72))
  (wire (pts (xy 109.22 151.13) (xy 120.65 151.13)))
  (wire (pts (xy 91.44 81.28) (xy 91.44 87.63)))
  (wire (pts (xy 83.82 25.4) (xy 83.82 35.56)))
  (wire (pts (xy 106.68 81.28) (xy 91.44 81.28)))
  (wire (pts (xy 120.65 87.63) (xy 120.65 92.71)))
  (wire (pts (xy 142.24 35.56) (xy 172.72 35.56)))
  (wire (pts (xy 220.98 99.06) (xy 224.79 99.06)))
  (wire (pts (xy 97.79 129.54) (xy 105.41 129.54)))
  (wire (pts (xy 161.29 90.17) (xy 166.37 90.17)))
  (wire (pts (xy 101.6 57.15) (xy 106.68 57.15)))
  (wire (pts (xy 166.37 77.47) (xy 166.37 80.01)))
  (wire (pts (xy 57.15 166.37) (xy 57.15 170.18)))
  (wire (pts (xy 106.68 87.63) (xy 120.65 87.63)))
  (wire (pts (xy 127 154.94) (xy 127 161.29)))
  (wire (pts (xy 166.37 100.33) (xy 166.37 102.87)))
  (wire (pts (xy 66.04 127) (xy 71.12 127)))
  (wire (pts (xy 24.13 87.63) (xy 24.13 80.01)))
  (wire (pts (xy 60.96 162.56) (xy 66.04 162.56)))
  (wire (pts (xy 109.22 149.86) (xy 109.22 151.13)))
  (wire (pts (xy 88.9 139.7) (xy 95.25 139.7)))
  (wire (pts (xy 57.15 153.67) (xy 57.15 158.75)))
  (wire (pts (xy 101.6 35.56) (xy 101.6 57.15)))
  (wire (pts (xy 72.39 92.71) (xy 77.47 92.71)))
  (wire (pts (xy 27.94 144.78) (xy 39.37 144.78)))
  (wire (pts (xy 86.36 160.02) (xy 105.41 160.02)))
  (wire (pts (xy 124.46 59.69) (xy 124.46 57.15)))
  (wire (pts (xy 83.82 35.56) (xy 82.55 35.56)))
  (wire (pts (xy 77.47 92.71) (xy 91.44 92.71)))
  (wire (pts (xy 93.98 35.56) (xy 93.98 45.72)))
  (wire (pts (xy 24.13 87.63) (xy 24.13 99.06)))
  (wire (pts (xy 82.55 41.91) (xy 85.09 41.91)))
  (wire (pts (xy 212.09 90.17) (xy 212.09 91.44)))
  (wire (pts (xy 142.24 38.1) (xy 142.24 41.91)))
  (wire (pts (xy 87.63 25.4) (xy 83.82 25.4)))
  (wire (pts (xy 82.55 38.1) (xy 82.55 41.91)))
  (wire (pts (xy 49.53 72.39) (xy 49.53 74.93)))
  (wire (pts (xy 27.94 72.39) (xy 31.75 72.39)))
  (wire (pts (xy 146.05 87.63) (xy 146.05 90.17)))
  (wire (pts (xy 257.81 81.28) (xy 257.81 83.82)))
  (wire (pts (xy 39.37 161.29) (xy 39.37 165.1)))
  (wire (pts (xy 24.13 72.39) (xy 27.94 72.39)))
  (wire (pts (xy 212.09 91.44) (xy 224.79 91.44)))
  (wire (pts (xy 142.24 163.83) (xy 146.05 163.83)))
  (wire (pts (xy 71.12 132.08) (xy 71.12 139.7)))
  (wire (pts (xy 86.36 35.56) (xy 83.82 35.56)))
  (wire (pts (xy 88.9 83.82) (xy 88.9 77.47)))
  (wire (pts (xy 105.41 158.75) (xy 105.41 160.02)))
  (wire (pts (xy 57.15 142.24) (xy 57.15 146.05)))
  (wire (pts (xy 120.65 158.75) (xy 120.65 160.02)))
  (wire (pts (xy 82.55 41.91) (xy 82.55 48.26)))
  (wire (pts (xy 27.94 147.32) (xy 27.94 144.78)))
  (wire (pts (xy 71.12 139.7) (xy 71.12 149.86)))
  (wire (pts (xy 71.12 139.7) (xy 83.82 139.7)))
  (wire (pts (xy 66.04 162.56) (xy 71.12 162.56)))
  (wire (pts (xy 257.81 91.44) (xy 257.81 93.98)))
  (wire (pts (xy 240.03 93.98) (xy 242.57 93.98)))
  (wire (pts (xy 106.68 57.15) (xy 106.68 74.93)))
  (wire (pts (xy 39.37 144.78) (xy 39.37 146.05)))
  (wire (pts (xy 124.46 57.15) (xy 139.7 57.15)))
  (wire (pts (xy 41.91 35.56) (xy 41.91 21.59)))
  (wire (pts (xy 212.09 91.44) (xy 212.09 92.71)))
  (wire (pts (xy 66.04 127) (xy 66.04 162.56)))
  (wire (pts (xy 71.12 149.86) (xy 71.12 157.48)))
  (wire (pts (xy 142.24 38.1) (xy 147.32 38.1)))
  (wire (pts (xy 105.41 160.02) (xy 105.41 162.56)))
  (wire (pts (xy 124.46 64.77) (xy 124.46 68.58)))
  (wire (pts (xy 172.72 45.72) (xy 172.72 35.56)))
  (wire (pts (xy 115.57 166.37) (xy 127 166.37)))
  (wire (pts (xy 166.37 90.17) (xy 166.37 92.71)))
  (wire (pts (xy 66.04 92.71) (xy 66.04 72.39)))
  (wire (pts (xy 105.41 167.64) (xy 105.41 171.45)))
  (wire (pts (xy 166.37 110.49) (xy 166.37 113.03)))
  (wire (pts (xy 212.09 100.33) (xy 212.09 102.87)))
  (wire (pts (xy 27.94 152.4) (xy 27.94 156.21)))
  (wire (pts (xy 41.91 21.59) (xy 101.6 21.59)))
  (wire (pts (xy 106.68 74.93) (xy 106.68 81.28)))
  (wire (pts (xy 93.98 45.72) (xy 172.72 45.72)))
  (wire (pts (xy 105.41 116.84) (xy 105.41 119.38)))
  (wire (pts (xy 106.68 87.63) (xy 106.68 83.82)))
  (wire (pts (xy 166.37 67.31) (xy 166.37 69.85)))
  (wire (pts (xy 88.9 77.47) (xy 91.44 77.47)))
  (wire (pts (xy 72.39 87.63) (xy 72.39 92.71)))
  (wire (pts (xy 86.36 129.54) (xy 90.17 129.54)))
  (wire (pts (xy 124.46 154.94) (xy 127 154.94)))
  (wire (pts (xy 66.04 72.39) (xy 91.44 72.39)))
  (wire (pts (xy 24.13 80.01) (xy 39.37 80.01)))
  (wire (pts (xy 166.37 87.63) (xy 166.37 90.17)))
  (wire (pts (xy 101.6 21.59) (xy 101.6 35.56)))
  (wire (pts (xy 135.89 90.17) (xy 146.05 90.17)))
  (wire (pts (xy 46.99 72.39) (xy 49.53 72.39)))
  (wire (pts (xy 105.41 127) (xy 105.41 129.54)))
  (wire (pts (xy 106.68 83.82) (xy 88.9 83.82)))
  (wire (pts (xy 105.41 160.02) (xy 115.57 160.02)))
  (wire (pts (xy 49.53 80.01) (xy 49.53 82.55)))
  (wire (pts (xy 146.05 90.17) (xy 146.05 92.71)))
  (wire (pts (xy 92.71 149.86) (xy 90.17 149.86)))
  (wire (pts (xy 71.12 149.86) (xy 82.55 149.86)))
  (wire (pts (xy 115.57 160.02) (xy 115.57 166.37)))
  (wire (pts (xy 212.09 78.74) (xy 212.09 82.55)))
  (wire (pts (xy 106.68 90.17) (xy 106.68 87.63)))
  (wire (pts (xy 224.79 96.52) (xy 224.79 99.06)))
  (wire (pts (xy 39.37 142.24) (xy 39.37 144.78)))
  (wire (pts (xy 250.19 93.98) (xy 257.81 93.98)))
  (wire (pts (xy 105.41 151.13) (xy 109.22 151.13)))
  (global_label "SENSE" (shape input) (at 87.63 25.4 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 96.0907 25.3206 0))
  )
  (global_label "TRIP" (shape input) (at 146.05 163.83 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 152.5755 163.7506 0))
  )
  (global_label "LINE" (shape input) (at 85.09 41.91 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 91.6155 41.8306 0))
  )
  (global_label "TRIP" (shape input) (at 72.39 87.63 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 72.3106 81.1045 90))
  )
  (global_label "SENSE" (shape input) (at 92.71 149.86 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 101.1707 149.7806 0))
  )
  (global_label "LOAD" (shape input) (at 142.24 41.91 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 149.3702 41.8306 0))
  )
  (symbol (lib_id "Device:C_Small") (at 105.41 165.1 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C1" (at 107.95 163.8362 0))
    (property "Value" "2u2" (at 107.95 166.3762 0))
    (property "Footprint" "Capacitor_THT:C_Axial_L17.0mm_D7.0mm_P25.00mm_Horizontal" (at 105.41 165.1 0))
    (property "Datasheet" "~" (at 105.41 165.1 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 139.7 82.55 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0105" (at 139.7 88.9 0))
    (property "Value" "GND" (at 139.7 87.63 0))
    (property "Footprint" "" (at 139.7 82.55 0))
    (property "Datasheet" "" (at 139.7 82.55 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0105") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 49.53 82.55 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0125" (at 49.53 88.9 0))
    (property "Value" "GND" (at 49.53 87.63 0))
    (property "Footprint" "" (at 49.53 82.55 0))
    (property "Datasheet" "" (at 49.53 82.55 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0125") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "4xxx:4011") (at 153.67 90.17 0) (unit 4)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 153.67 81.28 0))
    (property "Value" "4011" (at 153.67 83.82 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 153.67 90.17 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf" (at 153.67 90.17 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U1") (unit 4)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 166.37 106.68 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R10" (at 168.91 105.4099 0))
    (property "Value" "10k" (at 168.91 107.9499 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 167.386 106.934 90))
    (property "Datasheet" "~" (at 166.37 106.68 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 86.36 149.86 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R11" (at 86.36 143.51 90))
    (property "Value" "10k" (at 86.36 146.05 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 86.106 150.876 90))
    (property "Datasheet" "~" (at 86.36 149.86 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R11") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 95.25 139.7 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0126" (at 95.25 146.05 0))
    (property "Value" "GND" (at 95.25 144.78 0))
    (property "Footprint" "" (at 95.25 139.7 0))
    (property "Datasheet" "" (at 95.25 139.7 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0126") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Comparator:LM339") (at 78.74 129.54 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U5" (at 78.74 119.38 0))
    (property "Value" "LM339" (at 78.74 121.92 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 77.47 127 0))
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/lm139.pdf" (at 80.01 124.46 0))
    (pin "2")
    (pin "4")
    (pin "5")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "11")
    (pin "13")
    (pin "14")
    (pin "8")
    (pin "9")
    (pin "12")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 212.09 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R6" (at 214.63 85.0899 0))
    (property "Value" "4k7" (at 214.63 87.6299 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 213.106 86.614 90))
    (property "Datasheet" "~" (at 212.09 86.36 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Comparator:LM339") (at 232.41 93.98 0) (unit 3)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U5" (at 232.41 83.82 0))
    (property "Value" "LM339" (at 232.41 86.36 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 231.14 91.44 0))
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/lm139.pdf" (at 233.68 88.9 0))
    (pin "2")
    (pin "4")
    (pin "5")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "11")
    (pin "13")
    (pin "14")
    (pin "8")
    (pin "9")
    (pin "12")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U5") (unit 3)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 166.37 73.66 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R9" (at 168.91 72.3899 0))
    (property "Value" "10k" (at 168.91 74.9299 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 167.386 73.914 90))
    (property "Datasheet" "~" (at 166.37 73.66 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 57.15 170.18 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0103" (at 57.15 176.53 0))
    (property "Value" "GND" (at 57.15 175.26 0))
    (property "Footprint" "" (at 57.15 170.18 0))
    (property "Datasheet" "" (at 57.15 170.18 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0103") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 212.09 78.74 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0115" (at 212.09 82.55 0))
    (property "Value" "+9V" (at 212.09 73.66 0))
    (property "Footprint" "" (at 212.09 78.74 0))
    (property "Datasheet" "" (at 212.09 78.74 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0115") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 105.41 116.84 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0111" (at 105.41 120.65 0))
    (property "Value" "+9V" (at 105.41 111.76 0))
    (property "Footprint" "" (at 105.41 116.84 0))
    (property "Datasheet" "" (at 105.41 116.84 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0111") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 39.37 142.24 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0101" (at 39.37 146.05 0))
    (property "Value" "+9V" (at 39.37 137.16 0))
    (property "Footprint" "" (at 39.37 142.24 0))
    (property "Datasheet" "" (at 39.37 142.24 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0101") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 105.41 171.45 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0108" (at 105.41 177.8 0))
    (property "Value" "GND" (at 105.41 176.53 0))
    (property "Footprint" "" (at 105.41 171.45 0))
    (property "Datasheet" "" (at 105.41 171.45 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0108") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 109.22 149.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR0109" (at 109.22 153.67 0))
    (property "Value" "+5V" (at 109.22 144.78 0))
    (property "Footprint" "" (at 109.22 149.86 0))
    (property "Datasheet" "" (at 109.22 149.86 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0109") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 57.15 142.24 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR0102" (at 57.15 146.05 0))
    (property "Value" "+5V" (at 57.15 137.16 0))
    (property "Footprint" "" (at 57.15 142.24 0))
    (property "Datasheet" "" (at 57.15 142.24 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0102") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Potentiometer_US") (at 57.15 162.56 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "RV1" (at 54.61 161.2899 0))
    (property "Value" "10k" (at 54.61 163.8299 0))
    (property "Footprint" "Potentiometer_THT:Potentiometer_Bourns_3266Y_Vertical" (at 57.15 162.56 0))
    (property "Datasheet" "~" (at 57.15 162.56 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "RV1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 257.81 87.63 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 260.35 86.3599 0))
    (property "Value" "10k" (at 260.35 88.8999 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 258.826 87.884 90))
    (property "Datasheet" "~" (at 257.81 87.63 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 57.15 149.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R3" (at 59.69 148.5899 0))
    (property "Value" "47k" (at 59.69 151.1299 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 58.166 150.114 90))
    (property "Datasheet" "~" (at 57.15 149.86 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 66.04 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R1" (at 68.58 67.3099 0))
    (property "Value" "10k" (at 68.58 69.8499 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 67.056 68.834 90))
    (property "Datasheet" "~" (at 66.04 68.58 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 49.53 77.47 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C2" (at 52.07 76.2062 0))
    (property "Value" "0u1" (at 52.07 78.7462 0))
    (property "Footprint" "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (at 49.53 77.47 0))
    (property "Datasheet" "~" (at 49.53 77.47 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "C2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "4xxx:4011") (at 99.06 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 99.06 66.04 0))
    (property "Value" "4011" (at 99.06 68.58 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 99.06 74.93 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf" (at 99.06 74.93 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 90.17 35.56 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R_shunt1" (at 90.17 29.21 90))
    (property "Value" "1" (at 90.17 31.75 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 90.424 34.544 90))
    (property "Datasheet" "~" (at 90.17 35.56 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R_shunt1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 86.36 139.7 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C3" (at 86.3536 133.35 90))
    (property "Value" "1u" (at 86.3536 135.89 90))
    (property "Footprint" "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (at 86.36 139.7 0))
    (property "Datasheet" "~" (at 86.36 139.7 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "C3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:CQY99") (at 247.65 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D2" (at 246.507 85.09 0))
    (property "Value" "Low Batt" (at 246.507 87.63 0))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (at 247.65 89.535 0))
    (property "Datasheet" "https://www.prtice.info/IMG/pdf/CQY99.pdf" (at 246.38 93.98 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "D2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "4xxx:4011") (at 128.27 90.17 0) (unit 3)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 128.27 81.28 0))
    (property "Value" "4011" (at 128.27 83.82 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 128.27 90.17 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf" (at 128.27 90.17 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U1") (unit 3)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 39.37 165.1 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0104" (at 39.37 171.45 0))
    (property "Value" "GND" (at 39.37 170.18 0))
    (property "Footprint" "" (at 39.37 165.1 0))
    (property "Datasheet" "" (at 39.37 165.1 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0104") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "4xxx:4011") (at 139.7 69.85 0) (unit 5)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 146.05 68.5799 0))
    (property "Value" "4011" (at 146.05 71.1199 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 139.7 69.85 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf" (at 139.7 69.85 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U1") (unit 5)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 19.05 87.63 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "-PS1" (at 19.05 81.28 0))
    (property "Value" "Ground" (at 19.05 83.82 0))
    (property "Footprint" "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (at 19.05 87.63 0))
    (property "Datasheet" "~" (at 19.05 87.63 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "-PS1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 139.7 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0106" (at 139.7 60.96 0))
    (property "Value" "+9V" (at 139.7 52.07 0))
    (property "Footprint" "" (at 139.7 57.15 0))
    (property "Datasheet" "" (at 139.7 57.15 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0106") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:CQY99") (at 95.25 129.54 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D1" (at 94.107 120.65 0))
    (property "Value" "Pick-up" (at 94.107 123.19 0))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (at 95.25 125.095 0))
    (property "Datasheet" "https://www.prtice.info/IMG/pdf/CQY99.pdf" (at 93.98 129.54 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "D1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 77.47 88.9 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R2" (at 80.01 87.6299 0))
    (property "Value" "10k" (at 80.01 90.1699 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 78.486 89.154 90))
    (property "Datasheet" "~" (at 77.47 88.9 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 49.53 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR0121" (at 49.53 76.2 0))
    (property "Value" "+5V" (at 49.53 67.31 0))
    (property "Footprint" "" (at 49.53 72.39 0))
    (property "Datasheet" "" (at 49.53 72.39 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0121") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 19.05 72.39 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "+PS1" (at 19.05 66.04 0))
    (property "Value" "+9 Volts" (at 19.05 68.58 0))
    (property "Footprint" "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (at 19.05 72.39 0))
    (property "Datasheet" "~" (at 19.05 72.39 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "+PS1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 77.47 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0117" (at 77.47 88.9 0))
    (property "Value" "+9V" (at 77.47 80.01 0))
    (property "Footprint" "" (at 77.47 85.09 0))
    (property "Datasheet" "" (at 77.47 85.09 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0117") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 257.81 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0113" (at 257.81 85.09 0))
    (property "Value" "+9V" (at 257.81 76.2 0))
    (property "Footprint" "" (at 257.81 81.28 0))
    (property "Datasheet" "" (at 257.81 81.28 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0113") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 124.46 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0127" (at 124.46 74.93 0))
    (property "Value" "GND" (at 124.46 73.66 0))
    (property "Footprint" "" (at 124.46 68.58 0))
    (property "Datasheet" "" (at 124.46 68.58 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0127") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Comparator:LM339") (at 41.91 153.67 0) (unit 5)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U5" (at 40.64 152.3999 0))
    (property "Value" "LM339" (at 40.64 154.9399 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 40.64 151.13 0))
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/lm139.pdf" (at 43.18 148.59 0))
    (pin "2")
    (pin "4")
    (pin "5")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "11")
    (pin "13")
    (pin "14")
    (pin "8")
    (pin "9")
    (pin "12")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U5") (unit 5)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 27.94 149.86 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C5" (at 34.29 149.8536 90))
    (property "Value" "1u" (at 31.75 149.8536 90))
    (property "Footprint" "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (at 27.94 149.86 0))
    (property "Datasheet" "~" (at 27.94 149.86 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "C5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 77.47 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0119" (at 77.47 109.22 0))
    (property "Value" "GND" (at 77.47 107.95 0))
    (property "Footprint" "" (at 77.47 102.87 0))
    (property "Datasheet" "" (at 77.47 102.87 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0119") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 152.4 38.1 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "LOAD1" (at 154.94 36.8299 0))
    (property "Value" "LOAD" (at 154.94 39.3699 0))
    (property "Footprint" "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (at 152.4 38.1 0))
    (property "Datasheet" "~" (at 152.4 38.1 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "LOAD1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 39.37 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0124" (at 39.37 86.36 0))
    (property "Value" "GND" (at 39.37 85.09 0))
    (property "Footprint" "" (at 39.37 80.01 0))
    (property "Datasheet" "" (at 39.37 80.01 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0124") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 66.04 64.77 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0118" (at 66.04 68.58 0))
    (property "Value" "+9V" (at 66.04 59.69 0))
    (property "Footprint" "" (at 66.04 64.77 0))
    (property "Datasheet" "" (at 66.04 64.77 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0118") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 77.47 97.79 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "SW2" (at 78.74 96.5199 90))
    (property "Value" "Trip" (at 78.74 99.0599 90))
    (property "Footprint" "Button_Switch_THT:KSA_Tactile_SPST" (at 72.39 97.79 0))
    (property "Datasheet" "~" (at 72.39 97.79 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "SW2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 66.04 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0120" (at 66.04 109.22 0))
    (property "Value" "GND" (at 66.04 107.95 0))
    (property "Footprint" "" (at 66.04 102.87 0))
    (property "Datasheet" "" (at 66.04 102.87 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0120") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 27.94 156.21 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0128" (at 27.94 162.56 0))
    (property "Value" "GND" (at 27.94 161.29 0))
    (property "Footprint" "" (at 27.94 156.21 0))
    (property "Datasheet" "" (at 27.94 156.21 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0128") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Switch:SW_Push") (at 66.04 97.79 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "SW1" (at 67.31 96.5199 90))
    (property "Value" "Close" (at 67.31 99.0599 90))
    (property "Footprint" "Button_Switch_THT:KSA_Tactile_SPST" (at 60.96 97.79 0))
    (property "Datasheet" "~" (at 60.96 97.79 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "SW1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 166.37 113.03 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0114" (at 166.37 119.38 0))
    (property "Value" "GND" (at 166.37 118.11 0))
    (property "Footprint" "" (at 166.37 113.03 0))
    (property "Datasheet" "" (at 166.37 113.03 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0114") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 19.05 99.06 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "TP0" (at 19.05 92.71 0))
    (property "Value" "Ground" (at 19.05 95.25 0))
    (property "Footprint" "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (at 19.05 99.06 0))
    (property "Datasheet" "~" (at 19.05 99.06 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "TP0") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Potentiometer_US") (at 120.65 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "RV2" (at 118.11 153.6699 0))
    (property "Value" "10k" (at 118.11 156.2099 0))
    (property "Footprint" "Potentiometer_THT:Potentiometer_Bourns_3266Y_Vertical" (at 120.65 154.94 0))
    (property "Datasheet" "~" (at 120.65 154.94 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "RV2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 105.41 123.19 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R4" (at 107.95 121.9199 0))
    (property "Value" "10k" (at 107.95 124.4599 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 106.426 123.444 90))
    (property "Datasheet" "~" (at 105.41 123.19 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 212.09 102.87 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0112" (at 212.09 109.22 0))
    (property "Value" "GND" (at 212.09 107.95 0))
    (property "Footprint" "" (at 212.09 102.87 0))
    (property "Datasheet" "" (at 212.09 102.87 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0112") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "LED:CQY99") (at 166.37 95.25 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D4" (at 168.91 95.1229 90))
    (property "Value" "Tripped" (at 168.91 97.6629 90))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (at 161.925 95.25 0))
    (property "Datasheet" "https://www.prtice.info/IMG/pdf/CQY99.pdf" (at 166.37 96.52 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "D4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Small") (at 124.46 62.23 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C4" (at 130.81 62.2236 90))
    (property "Value" "1u" (at 128.27 62.2236 90))
    (property "Footprint" "Capacitor_THT:C_Disc_D7.5mm_W2.5mm_P5.00mm" (at 124.46 62.23 0))
    (property "Datasheet" "~" (at 124.46 62.23 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "C4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 212.09 96.52 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R7" (at 214.63 95.2499 0))
    (property "Value" "10k" (at 214.63 97.7899 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 213.106 96.774 90))
    (property "Datasheet" "~" (at 212.09 96.52 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Regulator_Linear:L7805") (at 39.37 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U4" (at 39.37 64.77 0))
    (property "Value" "L7805" (at 39.37 67.31 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown" (at 40.005 76.2 0))
    (property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf" (at 39.37 73.66 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector_Generic:Conn_01x01") (at 82.55 53.34 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "LINE1" (at 85.09 52.0699 90))
    (property "Value" "LINE" (at 85.09 54.6099 90))
    (property "Footprint" "Connector_Pin:Pin_D1.4mm_L8.5mm_W2.8mm_FlatFork" (at 82.55 53.34 0))
    (property "Datasheet" "~" (at 82.55 53.34 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "LINE1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "4xxx:4011") (at 99.06 90.17 0) (unit 2)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 99.06 81.28 0))
    (property "Value" "4011" (at 99.06 83.82 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 99.06 90.17 0))
    (property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/cd40/cd4011bms-12bms-23bms.pdf" (at 99.06 90.17 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U1") (unit 2)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_US") (at 105.41 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R5" (at 100.33 153.67 0))
    (property "Value" "100k" (at 99.06 156.21 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal" (at 106.426 155.194 90))
    (property "Datasheet" "~" (at 105.41 154.94 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "R5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 166.37 67.31 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0107" (at 166.37 71.12 0))
    (property "Value" "+9V" (at 166.37 62.23 0))
    (property "Footprint" "" (at 166.37 67.31 0))
    (property "Datasheet" "" (at 166.37 67.31 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0107") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 120.65 160.02 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0110" (at 120.65 166.37 0))
    (property "Value" "GND" (at 120.65 165.1 0))
    (property "Footprint" "" (at 120.65 160.02 0))
    (property "Datasheet" "" (at 120.65 160.02 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0110") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Power_MOSFET_FDA59N30:FDA59N30") (at 101.6 35.56 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U3" (at 121.92 24.13 0))
    (property "Value" "FDA59N30" (at 121.92 27.94 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-218-3_Vertical" (at 121.92 29.464 0))
    (property "Datasheet" "" (at 101.6 35.56 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 93.98 45.72 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0123" (at 93.98 52.07 0))
    (property "Value" "GND" (at 93.98 50.8 0))
    (property "Footprint" "" (at 93.98 45.72 0))
    (property "Datasheet" "" (at 93.98 45.72 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0123") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 220.98 99.06 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR0116" (at 220.98 102.87 0))
    (property "Value" "+5V" (at 220.98 93.98 0))
    (property "Footprint" "" (at 220.98 99.06 0))
    (property "Datasheet" "" (at 220.98 99.06 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0116") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+9V") (at 27.94 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "#PWR0122" (at 27.94 76.2 0))
    (property "Value" "+9V" (at 27.94 67.31 0))
    (property "Footprint" "" (at 27.94 72.39 0))
    (property "Datasheet" "" (at 27.94 72.39 0))
    (pin "1")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "#PWR0122") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Comparator:LM339") (at 134.62 163.83 0) (unit 4)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U5" (at 134.62 153.67 0))
    (property "Value" "LM339" (at 134.62 156.21 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 133.35 161.29 0))
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/lm139.pdf" (at 135.89 158.75 0))
    (pin "2")
    (pin "4")
    (pin "5")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "11")
    (pin "13")
    (pin "14")
    (pin "8")
    (pin "9")
    (pin "12")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U5") (unit 4)
        )
      )
    )
  )
  (symbol (lib_id "Power_MOSFET_FDA59N30:FDA59N30") (at 41.91 35.56 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U2" (at 62.23 24.13 0))
    (property "Value" "FDA59N30" (at 62.23 27.94 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-218-3_Vertical" (at 62.23 29.464 0))
    (property "Datasheet" "" (at 41.91 35.56 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Comparator:LM339") (at 78.74 160.02 0) (unit 2)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U5" (at 78.74 148.59 0))
    (property "Value" "LM339" (at 78.74 152.4 0))
    (property "Footprint" "Package_DIP:DIP-14_W7.62mm_Socket" (at 77.47 157.48 0))
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/lm139.pdf" (at 80.01 154.94 0))
    (pin "2")
    (pin "4")
    (pin "5")
    (pin "1")
    (pin "6")
    (pin "7")
    (pin "10")
    (pin "11")
    (pin "13")
    (pin "14")
    (pin "8")
    (pin "9")
    (pin "12")
    (pin "3")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "U5") (unit 2)
        )
      )
    )
  )
  (symbol (lib_id "LED:CQY99") (at 166.37 82.55 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "D3" (at 168.91 82.4229 90))
    (property "Value" "Closed" (at 168.91 84.9629 90))
    (property "Footprint" "LED_THT:LED_D5.0mm_IRGrey" (at 161.925 82.55 0))
    (property "Datasheet" "https://www.prtice.info/IMG/pdf/CQY99.pdf" (at 166.37 83.82 0))
    (pin "1")
    (pin "2")
    (instances
      (project "battgrid_breaker"
        (path
          (reference "D3") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
