EXECUTE LIST
<26,1,30,10> <24,1,30,9>	! ENABLE CRATE + REMOVE INHIBIT
<26,1,6,0>			! ENABLE BUTTONS
<10,1,6,0>			! RESET LAM
MOVE BUFFER TO <16,1,7,0>	! WRITE TO LIGHTS
WAIT
MOVE LIST TO BUFFER	! READ 2 INPUT GATES
<0,1,6,0:1>
STOP
