EXECUTE LIST
<10,1,1,0:1>		! Reset LAM 1+ 2
<9,1,1,1>		! Reset input buffer
<26,1,1,1>		! Enable lam #2
MOVE "1764 TO <16,1,1,0>	! Set up to read 32 values
MOVE <2,1,1,0> TO BUFFER WHENLAM 32 TIMES
