Modified on November 7, 1997 PAGE 1 OF 3

Metro-X 4.1 Enhanced Server Set Quick Installation and Release Notes for Linux Requir ed Softwar e

You must have gzip, cpio, and tar installed on your system to install Metr o-X. Column 1 shows the softwar e requir ed by this package. Column 2 shows the minimum version r equir ed. If you have a later version, that should be fine. If you need to install or upgrade your softwar e, column 3 shows the Internet location fr om which you can get it.

Quick Installation

1. Login to the system console as root. 2. You must have XFr ee86™ alr eady installed on your system. If you need to install or upgrade your softwar e, refer to the Required Software section above.

3. If you haven’t alr eady, please make these symbolic links, as suggested by the Linux Filesystem Standar d. This assumes your filesystem setup is fsstnd-compliant. If not, complain to your Linux vendor , and ask him to comply with the standar d in futur e releases. You will have to find your X binaries, library dir ectories (app-defaults, config, etc.), and include files, and make the appr opriate symbolic links yourself.

ln -s /usr/X11R6/lib/X11 /usr/lib/X11
ln -s /usr/X11R6/bin /usr/bin/X11
ln -s /usr/X11R6/include/X11 /usr/include/X11

4. Insert the first Metr o-X disk into drive A and execute the following command in a temporary directory:

# cd /tmp
# cpio --extract --verbose --block-size=36 -I /dev/fd0

Cpio has now extracted a file called MetroX.tar into /tmp. This file contains all the files necessary to install and r un Metr o-X.

TABLE 1: FTP Sites and Files

ITEM VERSION URL

Linux Kernel 1.1.92 ftp://tsx-11.mit.edu/pub/linux/sources/system/

Linux C Library 5.3.12 ftp://tsx-11.mit.edu/pub/linux/packages/GCC/

Shared Dynamic Linker (ld.so)1.7.14 ftp://tsx-11.mit.edu/pub/linux/packages/GCC/

Linux binutils 2.7 ftp://tsx-11.mit.edu/pub/linux/packages/GCC/

XFree86 3.3 ftp://tsx-11.mit.edu/pub/linux/packages/X11/XFree86-3.3/

GNU tar, zip, cpio any ftp://ftp.uu.net/systems/gnu/

Modified on November 7, 1997 PAGE 2 OF 3

5. Use the following commands to install Metr o-X:

# tar -xvf MetroX.tar
# ./install.metroess

6. When the installation is finished, type “y” at the pr ompt: Run Metr o-X 4.1 configX now? (y/n) 7. Using the graphical configuration scr een, select the Mouse , Keyboar d, Monitor , Graphics Car d, Resolutions . For details r efer to the configuration chapter in the manual.

8. Save and exit from configX. 9. Remove the temporary files:

# rm MetroX.tar install.metroess metroess.tar.gz

10. Run the following command: /usr/bin/X11/X 2>&1 |tee /tmp/errors 11. This will test the server configuration. Y ou should see a gray backgr ound with a small X cursor that tracks the mouse. If this is not what you see, consult the manual for tr ouble-shooting suggestions.

12. Type - - to exit the server . (If you need to make changes to your configuration, type the command: /usr/bin/X11/configX) 13. You ar e now r eady to start xdm or use xinit to start your normal X session.

Release Notes

Graphics Car ds The following chipsets ar e not supported:

P9000 MGA older than the Millennium P9100 Mach 8

Only the following chipsets support DPMS:

S3 864 S3 trio64 STORM S3 964 S3 trio 64V MACH64 S3 trio32 ARK I128

ISA-bus Mach64 car ds which wer e supported in Metr o-X 3.1 are not supported in Metr o-X 4.1 on

systems with mor e than 12 MB RAM.

If line artifacts (chopped pixels or thin r ed and gr een lines) appear at the r esolution you ar e using,

tweak the mode using the T iming Editor in ConfigX.

If the Xerr ors file contains the message “no defined matching dot clock for 1 152x864@70Hz”, your car d

has a fixed fr equency clock chip that does not support that setting. Another r evision of the car d might support it, however .

Some ATI Mach64 car ds have har dwar e limitations which pr event the use of certain modes you may

have selected. The server pr obes the car d and r eports “This mode not valid.” The server automatically deletes modes beyond the safe operating range. If you have questions, check the X err ors file.

Keyboar ds If the keyboar d is a US English keyboar d, then try the English 101 Key keyboar d selection. If the arr ow

keys (and the ones just above them) don’t work, then try the English 101 alternate selection. If the keyboar d is still not fully functional, then it is a keyboar d for which we don’t have a keycode definition. Use the Default / Use Console Mapping selection, as it should disable the keyboar d extensions altogether .

Ctrl Alt Backspace

Modified on November 7, 1997 PAGE 3 OF 3

Special Keys If you ar e using either the fvwm or fvwm95 window manager you may experience pr oblems using

special keys within ConfigX. Use of or - will result in behavior appr opriate to the window manager ’s mapping of those keys rather than what Metr o-X expects. This is most appar ent when using - plus arr ow keys in the timing editor of ConfigX.

Touch Scr eens If you r equir e touch scr een support, contact your dealer to arrange aquisition of a subsequent version

of Metr o-X.

Questions/Comments?

If you have problems with the product, first verify that you have ALL the required software installed. If that doesn’t fix the pr oblem, you can r each Metr o Link’s technical support in the following ways:

E-Mail: tech@metr olink.com Phone: +1 (954) 938-0283, ext. 2 Fax: +1 (954) 938-1982 Please be sur e to include the err or output fr om r unning the server and have the following information available:

1. Error output fr om the server in the file /var/log/Xerrors 2. Linux version ( uname -r) 3. C library version ( ls -l /lib/libc.so.*) 4. Metro-X version ( cat /usr/X11R6/lib/X11/Metro/.version) 5. Description of the pr oblem 6. How to r eproduce the pr oblem 7. Suggested fix (optional)

Ctrl Ctrl Shift

Ctrl Shift