MS-DOS KERMIT Ï Î â U

ďąãs |p âďSS

ASPACpž E-Mail : aspac@beta.wsl.sinica.edu.tw

ÞNø i : 94008

83 ~ 12 ë 15 é Version: 1.0

ASPAC peľv nú

ASPAC] Academia Sinica PACkage^O ď ą ã s | p â ď SS ö ó “né u ã Ï Î ” (Software Tools) Î “ÝDÑ M ” (Problem Solving) žpe C bope UÒ oi ğn éÎ åó čÝ óď ą

ãs |p âď SSÒş C Òş £ą ¡}ğ ql Îąê Æ] ]A néÎ åó ^A bąňU Cn é Îå óÏ Îv Qąú UA čiK Oú oÎÛ ÑÏ ÎC

néÎ åóÏ Îv Qąú pU G 1. né žÏÎ vQ G

Nu Îüê FSF] Free Software Foundation^1991~ 6ëÄ Gľ ž

GNU General Public LicenseC

2. åó žÏÎ vQ G

åó iHÛ Ñþ ľÎ ÞÎA ýč oÇH ÏQ Cč Dšn âò Ožň úC

]@ëž PoorMan LaT_EXďL kÏ Îďå íĺ ź‘W Ù , ÒH żå ďÈH ^å ÓíÜ ź‘ WÙ .

Contents

1 Introduction 1 1.1 What is KERMIT ? : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 1 1.2 Getting Started : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 4 1.3 Starting and Exiting MS-DOS KERMIT : : : : : : : : : : : : : : : : : : : : : : : : : 5 1.3.1 Starting : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 5 1.3.2 Exiting : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 6 1.4 Getting On-Line Help : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 7 1.5 Getting Status : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 9

2 Connection and Hangup 11 2.1 By Modem : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 11 2.1.1 Step-By-Step Connection : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 11 2.1.2 Automatic Connection : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 15 2.1.3 Hangup : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 20 2.2 By TCP/IP Local Area Network : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 21 2.2.1 Step-By-Step Connection : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 21 2.2.2 Automatic Connection : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 23 2.2.3 Hangup : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 24

3 Main Functions of MS-DOS KERMIT 25 3.1 Terminal Emulation : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 25 i

3.1.1 Basic Operations : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 25 3.1.2 Temporarily Switching to MS-DOS KERMIT or MS-DOS : : : : : : : : : : : 28 3.1.3 Build Multiple Sessions in TCP/IP Network : : : : : : : : : : : : : : : : : : : 29 3.1.4 Text v.s. Graphical Terminal : : : : : : : : : : : : : : : : : : : : : : : : : : : 29 3.2 File Transfer : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 30 3.2.1 Using KERMIT Protocol : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 30 3.2.2 Using Server : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 35 3.2.3 Using ZMODEM Protocol : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 38

4 Advanced Usage 41 4.1 Macro Command and Script Programming : : : : : : : : : : : : : : : : : : : : : : : 41 4.2 Useful Commands : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 45 4.2.1 MS-DOS Related Commands : : : : : : : : : : : : : : : : : : : : : : : : : : : 45 4.2.2 Terminal Emulation Related Commands : : : : : : : : : : : : : : : : : : : : : 46 4.2.3 File Transfer Related Commands : : : : : : : : : : : : : : : : : : : : : : : : : 47

A Installing MS-DOS KERMIT 49

B Using Modem and TCP/IP LAN to Connect to Remote Host 53

C Full-Duplex v.s. Half-Duplex Communication Settings 55

D Logging Terminal Emulation Process 57

E Screen Color Table 59

F Improving Speed and Quality of File Transfer 61

G Server Functions 65 G.1 Mainframe Server : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 65 G.2 PC Server : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 69

G.3 Secure PC Server : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 72

H Chinese Environment Settings 75

I MSKERMIT.INI, MSCUSTOM.INI, and USERDEF.INI 77 I.1 MSKERMIT.INI : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 78 I.2 MSCUSTOM.INI : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 92 I.3 USERDEF.INI : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 97

J VT300.INI and VT300X.INI 101 J.1 VT300.INI : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 101 J.2 VT300X.INI : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 107

K References 111

L MS-DOS KERMIT Command List 113

Index 118 iv CONTENTS

Chapter 1

Introduction

1.1 What is KERMIT ?

KERMIT Ob 1981 ~_ Ñ ô Û ñ È j Ç (Columbia Univertsity) pâ ď SS } l o i ž Œ Ý

œÒ À (Terminal Emulation) ÎÉ Œ Ç e (File Transfer) ów n é , äØ ž b Ï PC PU ň gA q č (Minicomputer) ÎD œ (Mainframe) ąş @ G ù i a ğ s u n é . Øe w o i ĺ ř@ ¡ Î n é , Àř MS-DOS KERMIT , C-KERMIT ěľ ż , ib W L | Ê Ø t Î W Ï Î , Uľ ż ď ž R O j P Û P . b Internet ôô W | ş newsgroup – comp.protocols.kermit.misc Î

comp.protocols.kermit.announce @ř æń SSoÎ ÇSS žéa .

KERMIT ř@ RO ÉV æÍ ą (Command-Driven Interactive) né , iţü ÏÎ Ìé JR O

, õæ Œ Ý œ Ò À Î É Œ Ç e ğ D n \ à , Î] w Û ö t Î Ñ Æ È , Ãã ş F ą ž u W š U ą ú (On-Line Help) ÎdSS \à .

MS-DOS KERMIT AÎ ó IBM PC ÎäÛ eœź W , Ü 1993 ~î wo iÜ 3.13 ľ . iä ľ

ÏÎ ÆÚ œ (MODEM) ÎÏìô ô (Local Area Network , Òp : TCP/IP , NOVELL ... ě ) Pů ÝD œ s u , čã Æ Œ Ý œ Ò À Î É Œ Ç e \ à ğ ~ , |ä ľ w q ĺ ř (Macro) RO Î Script

Programming ě\à .

KERMIT {ąiÏ Î anonymous ftp èą ÜU C‘I úo :

ľż ‘IW Ù ÉŒW Ù

MS-KERMIT for DOS, WINDOWS phi.wsl.sinica.edu.tw /pub/msdos/kerm313.zip

nctuccca.edu.tw /Chinese/DOS/kermit/ker3.zip ftp.cc.columbia.edu /kermit/bin/msvibm.zip C-KERMIT for UNIX ftp.cc.columbia.edu /kermit/bin/cku190.tar.z

C-KERMIT for OS/2 ftp.cc.columbia.edu /kermit/bin/ckoker.zip

C-KERMIT for VAX/VMS & Others ftp.cc.columbia.edu /kermit/bin/ckXXXX (XXXX íÜ ľ ż N ź , ÐÑ \

ÓØ ý ď READ.ME ÉŒ ą ú ) KERMIT for IBM Mainframes ( VM/ CMS, MVS, ..)

ftp.cc.columbia.edu /kermit/b/ik*.*

1.1. WHAT IS KERMIT ? 3

MS-DOS KERMIT 3.13 ľ| ãşU CS â :

1. RO ã şö Çö O žS Ê , iÏ ÎY g èą é J , Ããş u Wš Uą ú (On-Line Help) \ à . 2. Çé űè (Media) SÊ :

¿ âą PC iÏ Î Ç C ð ¡ ţ ň s , ÎH Ç C ð s ţ Æ Ú œ , zL ¡ @ q Ü u ô ň s , ÌłÇé tŒ iF 57600 bps.

¿ äľhØ ňą ÆÚœ źĺ ÛÊ ůźu @ .
¿ ibh Ø Ïì ô ôW Ï Î , ]A TCP/IP, Novell, DECnet, NetBIOS .... ě , Çé t Œ

iFÓÏ ìô ôžÌ łt Œ . 3. ŒÝ œÒÀ SÊ :

¿ iÒ À DEC VT tC (]A VT100, VT102, VT220, VT320 ě ) Î Tektronix graphic

4010/4014 ěŒ Ýœ . äď VT220 Î VT320 ãş äľ hrř (Character Set) žàO .

¿ žwxs Ìñ Qűe śž že , iÏ ÎW Uäš ÊÃ õ , |iQ Î Expanded Memory W[Ãõ Buffer jp HW[ xs űÆ .

¿ ib TCP/IP ôô WPÉ ØSS żÓ Sessions .
¿ iwq\ àä .

4. ÉŒ ÇeS Ê :

¿ iÏÎ KERMIT ówÎä L~ ąów (Òp : ZMODEM, XMODEM ě ) źĺ .
¿ ÏÎ ğ Ê ] ø Œ Î Sliding Window ÆØ i Ñ Ï Î Ì ï Ü , Ìł i F 9024(Bytes) *

31(Windows) .

¿ ãşżù Îč ùà O (ÏÎ Checksum Î CRC Error-Correction) , iÑ ÏÎÌ ]w ż ùrÿø Œ .

¿ ãşhr řà ńàO , Ãiäľ ďå ÉŒ Çe .

5. iO ýŒÝ œÒ ÀL {ÎÉ ŒÇ eÛö êT .

6. čÑ øAź (Server) Òą , iäľ ÉŒÇ e , Þzů ÝÉ Œ , Îõæ ůÝR Oě \à . 7. iÏ ÎÒl É (MSKERMIT.INI Î MSCUSTOM.INI) bÒ ÊÉ źĺ‘ ÎÑ ÆÎ ĺř (Macro) RO žwq .

HW SÊ Nó Û öź ‘ ďv @ ąú . żâU À ř| ź : Ä@ź ą ú KERMIT @ë ÏÎ y { , pó ÒÊ Îœ } MS-DOS KERMIT, ÏÎu Wš Uą ú\ à , Îd SSt Îň A . ÄGź ąú Ï ÎÆ Ú œ Î TCP/IP Ïì ô ô P ů Ý D œ s u Î œ u { Ç . ÄT ź ű Ð p ó Ï Î Œ Ý œ Ò À ÎÉŒ Çe âţ Dn \à , Ãą úÏ Îø Aź (Server) Òą Î~ ąó w ZMODEM iæ ÉŒ Ç ežè k . Ä|ź ą ú wq ĺ ř RO Î Ï Î Script Programming žèą , ÃűÐ ä ę‘ Î Ñ Æ ]w RO .

1.2 Getting Started

ÏÎ KERMIT žy{ pU : (AÎóÒ şľ żž KERMIT ď )

1. ÒÊ KERMIT.

2. ÏÎ ÆÚœ ÎÏ ìô ôPů ÝD œsu . 3. ÏÎ KERMIT Dn\ à (ŒÝ œÒ ÀÎ ÉŒÇ e ). 4. Ûů ÝDœ œu . 5. œ} KERMIT.

HW UB JN óUC ź‘ ďv@ Ôz .

1.3. STARTING AND EXITING MS-DOS KERMIT 5

1.3 Starting and Exiting MS-DOS KERMIT

ÒÊ MS-DOS KERMIT ešů ýNÆ Úœ ÎÏ ìôô dţ ť , ÃN MS-DOS KERMIT né w Ë (Install) Ü C:nKERMIT Øý á , ~i }l ÏÎ . wËąú ÐÑ \þ ý A. ż‘ Nąú pó Ò ÊÎ œ} MS-DOS KERMIT.

1.3.1 Starting

b MS-DOS čÜ Å ź (C:n>) áä J kermit , Ki Ò Ê MS-DOS KERMIT. PÉ X { U C T ğ : (Tğe ž 01, 02, ... Ní æź )

01 IBM-PC MS-DOS KERMIT: 3.13 8 JULY 1993
02 Copyright(C) Trustee of Columbia University 1982, 1983

03 Type ? or HELP for help

04 Installing Patches ......
05 MS-DOS Kermit: 3.13 8 July 1993 patch level 17
06 MS-DOS Kermit 3.11/3.12/3.13 initialization file ......
07 Customizations ......

08 Smile !
09 MS-Kermit>

ąú :

¿ Ä 1, 2 æ : MS-DOS KERMIT ľż ąú Tğ , Øe ř 3.13 ľ .
¿ Ä 3 æ : äJ ? Î help , id SSu WšU ąú Tğ , ÐÑ \ 1.3.3. ‘ąú .
¿ Ä 4, 5 æ : Patch Tğ .
¿ Ä 6 æ : õæ MSKERMIT.INI (tÎÒ lÉ ).
¿ Ä 7 æ : õæ MSCUSTOM.INI (ÏÎ ÌÛ wÒl É ).
¿ Ä 9 æ : MS-Kermit> ř MS-DOS KERMIT žtÎ č ÜÅ ź , äá iä J MS-DOS KER-

MIT RO .

YL kű Q Ò Ê MS-DOS KERMIT, BX { Bad Command or File Name Tğ É , ÐÏ Î U Cè ąA ŒÒ Ê :

1. èk @ : ib ôó Øý ďÒÊ MS-DOS KERMIT :

¿ BJ@ : b MS-DOS čÜÅ źá äJ cd n , ^ì ÚØ ý (Root Directory) ď .
¿ BJG : ÏÎå Ñs èné (Òp : vi, emacs, .... ě ) sè AUTOEXEC.BAT ÉŒ , b

PATH= Ôz Ì ¡ Ý [ J :C:nKERMIT (Yz N MS-DOS KERMIT wË ó ä

LØý , Ðü w£T žô |WÙ ) ¿ BJ T : b MS-DOS čÜ Å ź á ä J autoexec , ńsõ æ AUTOEXEC.BAT , N

C:nKERMIT [Jj Mô| (Search Path) ď .

¿ BJ| : b MS-DOS čÜÅ źá äJ kermit , Ki űQ ÒÊ .

2. èk G : Èàb C:nKERMIT Øý ďÒÊ MS-DOS KERMIT :

¿ BJ@ : b MS-DOS čÜÅ źá äJ cd nkermit , NØeÒ bž u@ Øý (Work-

ing Directory) óï Ü C:nKERMIT ď . (Yz N MS-DOS KERMIT wË ó äL Ø ý ,

Ðüw£ Tž ô|W Ù )

¿ BJG : b MS-DOS čÜ Åźá äJ kermit , Kiű QÒÊ .

1.3.2 Exiting

b MS-Kermit> čÜÅ źá äJ quit Î exit (iš gř q Î ex ), Yiœ } MS-DOS KER-

MIT.

YuQ ÈÉÁ ńÜ MS-DOS ďõ æY Çu @ , šôá Kð ^ MS-KERMIT, ib MS-Kermit> čÜ Åź áä J push , KiÈ Éœ} . Ý MS-DOS ďž u@õ æš ôá , ib MS-DOS čÜ Åź áä J exit , Yiń ð MS-KERMIT.

1.4. GETTING ON-LINE HELP 7

1.4 Getting On-Line Help

MS-DOS KERMIT ãşu Wš Uąú (On-Line Help) \à , iý ÏÎÌ Öt ÇSS URO žN q

ÎÏ Îè ą , dSSR Oř ? Î help .

b MS-Kermit> čÜÅ źáä J ? , YX {UC Tğ :

Ask, Askq (read keybd to variable) Open Read/Write/Append file scripts
Bye (logout remote server) Output text (for scripts)
C or Connect (become a terminal) Pause [seconds], Mpause [millisec]
    . .
    . .
    . .

źTğ ąú MS-DOS KERMIT Dn RO ÎäN q .

Yz{ řHW ąú čň , ib MS-Kermit> čÜÅ źáä J help , YX {UC Tğ :

                  Introduction to MS-DOS Kermit

An MS-Kermit command is a line of words seperated by spaces and ending
with a carriage return <the Enter key>. Example:
                        .
                        .
                        .

źTğ HÀþ èą űÐ MS-DOS KERMIT RO , ÃşÉ Rąú , ûÏÎ ? ROóř ÔÉ . čF ÏÎ ? Î help âR O~ , MS-DOS KERMIT |č Ñ t@ Î ą žu W š Uą ú . Îk pU :

éJ ROÉ , ÈÝ bč TwB H ? úN , K| X{š Uą úTğ , ÐÉ zv Bźĺ ź RO , ÐÑ \U Ò .

Ò : dSSt ÎØe ŒÝ œÒ ÀÑÆ ]w ąÎ .

¿ BJ @ : b MS-Kermit> čÜÅź áä J show ?
¿ BJ G : b MS-Kermit>show áäJ terminal

ąú :

¿ BJ @ : È¿ Ï Î show RO i d SS U ţ Ñ Æ ] w ą Î , ýč ¿ ä á ş [ W ó ŋ î r ~ id SSŒÝ œÒ ÀÑ Æ]w ąÎ . ]źb MS-Kermit> čÜÅ źáä J show ? , YX { UC Tğ :

Use one of the following words in this position:
Communications Control-prefixing File Key Logging Macros
Memory Modem Protocol Scripts Server Sessions Statistics
Status Terminal Translation Variables

źÉ åÐ (cursor) |śd b MS-Kermit>show á , ěÝ éJU @Ó ŋîr .

¿ BJ G : ÑHW ąú i¿ : ÏÎ terminal ŋî r id SSŒ Ýœ ÒÀ ÑÆ ] wą Î , ]ź b MS-Kermit>show ğá äJ terminal , YX {U CŒ ÝœÒ ÀÑ Æ]w È :

Terminal type: VT100 Display: Regular, 8-bit
Mode-Line: on Escape character: ^]
Term Tek4010 (auto-entry): enabled Keyboard translation: on
     . .
     . .
     . .

ÑźT ğKi o¿ ØeŒ Ýœ ÒÀ ÑÆ] wą Î .

1.5. GETTING STATUS 9

1.5 Getting Status

bW@ ‘ž dÒ ď £Ï Î show RO , źRO i óU ÚÌ F Ñ MS-DOS KERMIT Øe žÑ Æ ]w ąÎ ÎU ţÎp Tğ . b MS-Kermit> čÜÅ źá äJ show ? , X{U CT ğ :

Use one of the following words in this position:
Communications Control-prefixing File Key Logging Macros
Memory Modem Protocol Scripts Server Sessions Statistics
Status Terminal Translation Variables

b show RO á [W H W ô @ï ţ , Yi dSS MS-DOS KERMIT žUţ ] w ą Î . äď û ń nÌ ]A :

1. show communications : ãÜ qTÛ öÑ Æ] wąÎ . 2. show file , show protocol : ãÜ ÉŒÇ eÛ öÑÆ ]w ąÎ . 3. show key : ãÜY @\ àä ž]w È . 4. show macro : ãÜÒş ĺř RO žwq . 5. show server : ãÜø Aź ÛöÑ Æ] wąÎ . 6. show statistics : ãÜÉ ŒÇ etŒ ÎÉ ąěÎ pÆ r . 7. show status : ãÜU ńn ÑÆ ]wą Î . 8. show terminal : ãÜ ŒÝ œÛö ÑÆ ]wą Î .

ÏÎ show RO o¿ H WU þ ÑÆ ž ]w ą Î á , Ki Q ÎU C ź‘ Ò z žR O ïÜ U Û öÑ ÆÈ , HA şč Pž ôÒ .

Üźz @w| o{ : MS-DOS KERMIT žROÆ ø , čö éJ . řè KÏ ÎÌ _č , MS-DOS

KERMIT čÑ H Y g è ą é J R O ž \ à , çY : éJ R O É È Ý ä J e X Ó r ÿ Y i , ÐÑ

\H UÆ Ò :

show communications iY gř sh com show terminal iY gř sh te

şFY g éJ RO ž óU , zKà D ‘e öa é JR O , At X ? Î help žu Wš Uą ú \ à , XG čÝO Ðô óR OYi ÏÎ MS-DOS KERMIT.

ÏÎ Y g è ą é J R O É š ů ‘ N : Yg R O ž ø Œ š ů ň H Ï À č P R O . H show

terminal RO ř Ò : YÈ é J sh t É , ] show terminal RO P show translation

RO ąi Yg ř sh t , LkÏ Às žřó Ì , |X{ ’?Word ’t’ is ambiguous’ žù~ Tğ .

10 CHAPTER 1. INTRODUCTION

Chapter 2

Connection and Hangup

MS-DOS KERMIT iÏ Î Æ Úœ (Modem) ÎÏì ô ô (Local Area Network , Òp : TCP/IP , NOVELL .... ě ) PůÝ Dœs u , żźN ąú su Îœu {Ç .

2.1 By Modem ż‘ ąú ÏÎ ÆÚœ (Modem) Pů ÝDœ žs uÎ œu{ Ç . suèą iÀ âØ :

1. òż suè ą : ÏÎ MS-DOS KERMIT RO vBź ĺ .

2. ÛÊ suè ą : ÏÎ MSKERMIT.INI (tÎ Òl É ) Î MSCUSTOM.INI (ÏÎÌÛ wÒ l É ) ž\àź ĺ .

œu èą iÀ ěią Îj ćąâ Ø .

2.1.1 Step-By-Step Connection

òż su èą iÀř HU BJ :

1. ]w PÆÚ œs ţž ÇCð (Serial Port) sź . 2. ]w ÆÚœ Çé tv (Speed). 3. sţ ůÝD œ .

ÐÑ \U Ò .

Ò : ÏÎ PC žÇ C ð com2 sţ Æ Ú œ , ůţ ďą ã s |D œ gate.sinica.edu.tw (HU š Ù ř

gate ) , ÆÚœ ňą : HAYES Ûeň , tŒ : 19200bps, ůţè ą : ÆW (Touch Tone) ą , ůţ ź

X : 6513920.

òż su {Ç pU :

¿ BJ @ : b MS-Kermit> čÜÅź áä J set port com2
¿ BJ G : b MS-Kermit> čÜÅ źá äJ set speed 19200
¿ BJ T : b MS-Kermit> čÜÅ źá äJ connect
¿ BJ | : äJ at
¿ BJ ŋ : äJ atdt 6513920
¿ BJ ż : b sluice# login: čÜ Åźá äJ terminal (# ř 1, 2, 3, ... ěÆ r )
¿ BJ C : b sluice#:Top> čÜÅź áä J sessions (# ř 1, 2, 3, ... ěÆ r )
¿ BJ K : b sluice#:Top>Sessions> čÜÅź áä J telnet -8 gate (# ř 1, 2, 3, ... ěÆ

r ) ąú :

¿ BJ @ : set port ROÎ óüw qT ð (Communication Port) , iÀ řUC TØ :

1. ÇCð (Serial Port) : iř COM1 Ü COM4.

2. BIOS : iř BIOS1 Ü BIOS4.

3. Ïìôô (Local Area Network): iř TCP/IP, NOVELL, ....ě.

¿ BJ G : set speed RO Îó ]w RS-232 űś PÆ Úœ ğą ž Çé tŒ , tŒ È id \ ÆÚ œÏ Îâ U . YÆÚ œã Æê Æč Yà O , ź@ ]w tŒ È ij óÆ Úœ PÆ Úœ ğ ąž êÚÇ ét Œ .

¿ BJ T : äJ connect ROá , Yi JŒ ÝœÒ Àe ś , ÐÑ\ 3.1.1. ‘ą ú .
¿ BJ | : at ř HAYES Ûe ňÆ Úœ RO , Îóú ÕÆ Úœ O_ £‘ . ^şT ği Àř U

CT Ø :

1. OK: íÜ ÆÚ œb £‘ň A , i}l ůź .

2. BUSY: íÜØe uô bÖ ¡ňA , ÝyÔA ůź . 3. NO CARRIER: íÜ ÆÚœ ĳ^ şô óTğ . ÝË dUC Æţ :

{ üw ğÇC ðs źO_ £T .

{ sţ ÆÚœ PÇ Cðğ ÆÚ u (Modem Cable) O_ £T .

Yz éJ ù~ r ÿÉ , |o { : öU Backspace Lk øh ýe éJ žr ÿ , źÉ iï ö

Ctrl-h (PÉö U Ctrl Î h), KàF ì Backspace žÄG .

¿ BJ ŋ : atd ř HAYES Ûe ň ÆÚ œ RO , Îó Ï ÆÚ œ i æů ź Ê@ . źR Oá ů [ W t Î p , Hüw ůźè ą . ůźèą iÀ řHU âØ :

{ ÆW (Touch Tone) èą : H atdt íÜ , řÆ ìæ ń œğ ůź è ą , Øe h Hź è ą řD .

{ SSÄ (Pulse) èą : H atdp íÜ , řþ ñæ ńœğ ůź èą , Øe ûÖ ÏÎ .

atdt Î atdp RO žÏ Îèą pU :

atdt Î atdp [ýů ţžq Üź X ]

qÜź X i Î Cì Æ r (#######) Îe T ì Æ r[ á | ì Ær (###-####) ěè ąí Ü . ÆW èą PSS Äèą ůź ğtğ ÐÑ \Æ ÚœÏ Îâ U .

bż Òď Ï ÎÆ Wè ąů ź , äJ atdt 6513920 á , iě čÆ Ú œo X@ sê ůź n , ÝX {@ø ê ’Í ’ ná , śO Wž OH Î CD üÜO| G_ , íÜw ĺ\ sţď ąã s |ž Terminal Server, ÃX{ UC Tğ :

CONNECT 9600 REL ....
=================================
COMPUTING CENTER, ACADEMIA SINICA
     Dial-up : (02)651-3920

           1.SLIP
           2.PPP
           3.TERMINAL

=================================

sluice# login:

# ř 1, 2, 3, ... ěÆ r .

¿ BJ ż : terminal ř Terminal Server ÒÏ Îž RO . ďąã s| Terminal Server ič Ñ

SLIP , PPP , Î Terminal Emulation ěT Ø s u A È , äJ terminal iï Ü Terminal Emulation AÈ . äJ áX {UC Tğ :

sluice#:Top>

# ř 1, 2, 3, ... ěÆ r .

¿ BJ C : sessions ř Terminal Server ÒÏÎ žRO , äJ áii J Sessions lØ ýď , Ï Î TCP/IP ôô sţ gate Dœ .

¿ BJ K : telnet -8 ř Terminal Server ÒÏ Î ž R O , ÏÎ telnet ów P ü w D œ s ţ , ÃH 8-bit èąÇ eê Æ , iäľ ďå êTž yq . telnet -8 ROž ÏÎè ąp U :

telnet -8 [suD œWÙ Î IP ì} ]

żÒ ď i äJ telnet -8 gate Î telnet -8 140.109.14.2 . su ĺ \á X {U C T ğ :

Type ^](decimal 29) <CR> to return to NetBlazer
Trying 140.109.14.2:##
Telnet session # connected to gate

UNIX(r) System V Release 4.0 (gate)

login:

# ř 1, 2, 3, ... ěÆ r . íů Ý D œ gate ž login Tğ X { á , Yi ä J username Î

password, }lu @ .

2.1.2 Automatic Connection

e@‘ ď wą ú ò żs u èą , źB N űÐ t @Ø ó šK ž s uè ą . iÛ Êź ĺ e @‘ B J @Ü ŋž u@ .

ÛÊ su èą DOQ Î MS-DOS KERMIT žU CSÊ źĺ :

1. b MS-DOS KERMIT ďş âÓń nž Òl É , ÀOř :

¿ MSKERMIT.INI (tÎ Òl É )

¿ MSCUSTOM.INI (ÏÎÌ ÛwÒ lÉ )

ÒÊ MS-DOS KERMIT É , |Û Ê õ æH W â Ò l É žž e . YN ‘ Î žt Î Ñ Æ ] w RO [ J H W É Œ ď , Ki b Ò Ê á Û Ê ź ĺ Ñ Æ ] w u @ . MSKERMIT.INI žą ú Ð Ñ\ þý I .

2. MS-DOS KERMIT ãÆw qĺ ř (Macro) RO ž\ à . ÒŒ ĺř , Oü N@ sÛö RO ř

Xb @_ , Hźĺ Y@S w\ à , Ãi Î@ ĺřR ON ío@ sR O . Is ĺř É , os R OK |Ìw qè ąõ æ , ĺřR OžÏ ÎÐ Ñ\ 4.1. ‘ąú .

ÚÚÄ @ţS Ê , iNò żs uèą BJ @Î Gž set port Î set speed RO [J

MSCUSTOM.INI ď , Kà bÒ Ê MS-DOS KERMIT á , ÛÊź ĺÑ Æ]w u@ .

ÚÚ Ä G ţ S Ê , iN ‘ Î R O s H ĺ ř è ą w q , Ã[ J MSKERMIT.INI Î MSCUS-

TOM.INI ď . bÒÊ MS-DOS KERMIT á , KiIs ĺř , õæ ‘ÎR Os , pPÏ Î MS-DOS

KERMIT žØ (Built-in) žR O@ ë .

b MSKERMIT.INI ÉŒ ď w w q@ dial ĺř R O , iÛ Ê ź ĺò ż s u è ąB J T Ü ŋ žů ź u @ . ÏÎ dial RO e , šů ý Ë d DIALUPS.TXT Î HAYES.SCR âÉŒ O _ w s bó C:nKERMIT Øýď (YN MS-DOS KERMIT wË óä LØý É , şË dO _bÓ Øý U ). Yĳo {ź GÉŒ , şNäq MS-DOS KERMIT wËÏ ù copy Ü C:nKERMIT Øýď .

DIALUPS.TXT řq Ü ŕ ê Æ É . HAYES.SCR ř HAYES Ûe ň Æ Ú œ ž Û Ê ů ź É Œ .

YÏÎ žÆ Úœ čO HAYES Ûeň , hş b MS-DOS KERMIT wËÏ ùž , ÌÓ ÏÎ žÆ Ú œň ąM äÛ ïşž .SCR ÉŒ , ÃN ä copy Ü C:nKERMIT Øýď .

gÑ Wz è k , Kib Ò Ê MS-DOS KERMIT á , Is dial ĺř , ÛÊ ź ĺ 2.1.1. ‘B J @Ü ŋž u@ . ÐÑ\ UÒ .

Ò : ÏÎ PC žÇ C ð com2 sţ Æ Ú œ , ůţ ďą ã s |D œ gate.sinica.edu.tw (HU š Ù ř

gate ) , ÆÚœ ňą : HAYES Ûeň , tŒ : 19200bps, ůţè ą : ÆW (Touch Tone) ą , ůţ ź

X : 6513920.

ÛÊ su {Ç pU :

¿ BJ @ : N set port com2 Î set speed 19200 âRO [J MSCUSTOM.INI ÉŒ ď .

¿ BJ G : b AUTOEXEC.BAT ÉŒ ď[J HU Ôz :

set modem = hayes

¿ BJ T : b DIALUPS.TXT ÉŒď [J HU Ôz :

sinica T6513920 19200 = Telephone number for sinica

¿ BJ | : ÒÊ MS-DOS KERMIT.
¿ BJ ŋ : b MS-Kermit> čÜÅź áä J dial sinica
¿ BJ ż : b MS-Kermit> čÜÅź áä J connect
¿ BJ C : b sluice# login: čÜÅź áä J terminal (# ř 1, 2, 3, ... ěÆr )
¿ BJ K : b sluice#:Top> čÜÅź áä J sessions (# ř 1, 2, 3, ... ěÆ r )
¿ BJ E : b sluice#:Top>Sessions> čÜÅź áä J telnet -8 gate (# ř 1, 2, 3, ... ěÆ

r ) BJ@ ÜTÈ ůb ìÿÏ ÎÉ ]w , Há Èů õæB Jŋ ÜEY i .

ąú :

¿ BJ G : set modem = hayes iN MS-DOS ôÒÜ Æ (Environment Variable) modem ğÈ ] w ř HAYES Ûeň , Ï dial ĺř R Oi I s HAYES.SCR ÉŒ Û Ê ů ź . Yz ÏÎ ž Æ Ú œ ř XXXX ň (Òp : T3000, SPORT .... ě ) , hş ý Ü MS-DOS KERMIT wË Ïù W , ÌÓÏ Îž ÆÚ œňą Mä Ûï şž XXXX.SCR ÉŒ , ÃNź ÉŒ copy Ü

C:nKERMIT Øýď , Má N set modem = XXXX Ôz [J AUTOEXEC.BAT

ď , dial ĺř RO KiÏ Î XXXX.SCR ÉŒÛ Êů ź .

¿ BJ T : DIALUPS.TXT ÉŒ ďU æì WÙp U :

[OW ] [qÜź X ] [Çé tŒ ] [PBè ą ] [ùÑ ] Uæ ìąÈ ÝH @Å Õrÿ (Space) ÀjY i , äNq pU : 1. OW (Alias Name): KóOÐ ğW Ù , pźÒ ďž sinica .

2. qÜźX : iÎ CìÆ r (#######) ÎeT ìÆr [á |ì Ær (###-####) íÜ , eś Ý[ ù T Î P , Hùú ůź èą řÆW ą (Touch Tone) ÎSSÄ ą (Pulse) . 3. ÇétŒ : RS-232 űśP ÆÚœ ğą žÇé tŒ . 4. PBèą : ůÝ DœÏ Îğ PBè ą , ją À]w ř NONE. 5. ùÑæ .

ÏÎ @ës èn é (vi, emacs, ...ě) Yi Œï DIALUPS.TXT ÉŒ že . Çé t Œ ÎP B èą æ iÎ ’=’ Åźú N , íÜ ÏÎ MS-DOS KERMIT Øe Ò ]w ž Ç ét ŒÎP Bè ąi æůź .

¿ BJ ŋ : dial ĺřR OžÏ Îè ąÎ u@ì zp U :

1. èą@ : dial [Alias Name]

Ü DIALUPS.TXT ÉŒ ďMä Ó Alias Name ÒNíž qÜ źX , MáI s HAYES.SCR ÉŒÎP ÆÚ œÛï şž XXXX.SCR ÉŒ (XXXX NíÆÚ œň ź ) iæůź . bż Ò ď , äJ dial sinica á , iě č Æ Úœ o X @ sê ů ź n , MáX { U C T ğ :

Looking up "sinica"
From dialing directory : sinica = T6513920
Dialing T6513920, wait .... ATDT6513920

ÝX{@ øê ’Í ’ ná , śOW ž OH Î CD üÜO| G_ , íÜw ĺ\s ţď ą ãs|ž Terminal Server, ÃX {UC Tğ :

CONNECT 9600 REL ....

Máð^ MS-DOS KERMIT ď , X{ MS-Kermit> čÜ Åź . äJ dial ĺřRO É , iào Íž ù~ą Îp U :

(a) Alias Name ĳwq ó DIALUPS.TXT ď : źÉ|X {U Cù ~Tğ :

sinica not found in dialing directory C:\KERMIT\DIALUPS.TXT

Ãś îůź .

(b) ÆÚ œ ĳ } Ò Î q T ð ü w ù ~ : X{ Turn on or connect your modem! žù ~T ğ , źÉş }ÒÆ Úœ q¡ ÎH set port ROń sü wÇC ðs ź .

2. èąG : dial [Telephone No.]

¡ţIs HAYES.SCR ÉŒ ÎP ÆÚœ Ûï şž XXXX.SCR ÉŒ (XXXX NíÆ Ú œňź ) iæů ź , qÜź Xeş [W T Î P Hù úůź èą . bżÒ ď , äJ dial T6513920 á , iěč Æ Úœ o X@ sê ů źn , ÃX{ U C Tğ :

Dialing T6513920, wait .... ATDT6513920

ÝX{@ øê ’Í ’ ná , śOW ž OH Î CD üÜO| G_ , íÜw ĺ\s ţp â ďSSž Terminal Server , ÃX{U CT ğ :

CONNECT 9600 REL ....

Máð^ MS-DOS KERMIT ď , X{ MS-Kermit> čÜ Åź . iàžù ~ą ÎÎB zè ąÐ Ñ\è ą@ Òz .

3. èąT : Èä J dial ĺřRO , äáč[ ôó ÑÆ ÏÎe @ÿ ůź žź X , Is HAYES.SCR ÉŒ ÎP ÆÚ œ Ûï şž XXXX.SCR É Œ (XXXX Ní ÆÚ œňź ) iæ ůź .

bżÒď , Ye @ÿů źÉ ÏÎ źXř 6513920 , hÈ äJ dial ĺř ROá , iě č ÆÚœo X@ sêů źn , ÃX {U CT ğ :

Dialing T6513920, wait .... ATDT6513920

ÝX{@ øê ’Í ’ ná , śOW ž OH Î CD üÜO| G_ , íÜw ĺ\s ţď ą ãs|ž Terminal Server , ÃX{ UC Tğ :

CONNECT 9600 REL ....

Máð^ MS-DOS KERMIT ď , X{ MS-Kermit> čÜ Åź . iàžù ~ą ÎÎB zè ąÐ Ñ\è ą@ .

¿ BJ ż : ÏÎ dial ĺř R O s ţ ď ą ã s | ž Terminal Server á , |ð ^ MS-Kermit> čÜ Åźď , źÉi~ òÏ Î MS-DOS KERMIT žŒ ÝœÒ À\ àPů ÝD œ gate su ; çiÏÎ äL ŒÝœ ÒÀ né PůÝ Dœ gate su .

Y~ ò Ï Î MS-DOS KERMIT, ÈÝ b MS-KERMIT> čÜ Å ź á ä J connect (iY gř c ) , YiJ ŒÝ œÒÀ eś , , ÃX{ UC Tğ :

CONNECT 9600 REL ....
=================================
COMPUTING CENTER, ACADEMIA SINICA
     Dial-up : (02)651-3920

           1.SLIP
           2.PPP
           3.TERMINAL

=================================

sluice# login:

# ř 1, 2, 3, ... ěÆ r .

YÏ ÎäL ŒÝ œÒ Àné Pů ÝDœ gate su , hşä J exit Î quit , œ} MS-DOS

KERMIT áA ÏÎ .

¿ BJ CÜE žą úÐ Ñ\ 2.1.1. ‘ .

2.1.3 Hangup

œu è ą i À ř ě i ą Î j ć ą G Ø , bź ť H s ţ ď ą ã s | D œ gate.sinica.edu.tw (HU šÙ ř gate ) řÒ :

1. ěi ąœu :

¿ BJ@ : bůÝ Dœ gate žčÜÅ ź gate:~> áäJ logout, ð^ Terminal Server.
¿ BJG : b Terminal Server žčÜÅ ź sluice#:Top>Session> áä J top ^ì sluice#:Top>

Øýď . (źBž # íÜ 1, 2, 3, .... ěÆr )

¿ BJT : b Terminal Server žč ÜÅź sluice#:Top> áä J logout , YiÁ _Æ Ú œPůÝ Terminal Server žsţ . (źBž # íÜ 1, 2, 3, .... ěÆ r ) ¿ BJ | : öU Alt-x (PÉ ö U Alt Î x) Î Ctrl-]-c (PÉ öU Ctrl Î ] , Aö U

c ) , Yi ð^ MS-Kermit> čÜ Åź ď , źĺœ u{ Ç .

ąú :

¿ BJ@ : bůÝ Dœ gate ďäJ logout , ^ì Terminal Server á , X{UC Tğ :

    sluice#:Top>Sessions>

# ř 1, 2, 3, ... ěÆr .

źÉÆÚ œť Pů Ý Terminal Server Oùs uňA . iAÿ äJ connect RO , ä áüúý sţ žDœ WÙ Î IP ì} , Hsţ äLD œ ; Î~ òõæ BJ GÜ | , ÏÆ ÚœPů Ý Terminal Server œu .

¿ BJ T : źB ž logout ř Terminal Server RO , Îó Ï Æ Ú œ P ů Ý Terminal

Server œu . œuá X{ NO CARRIER Tğ , BÆÚ œW ž OH Î CD üÜO |ű À ,

íÜwœ u .

2. jć ąœu : iÎ HU âØè ąF ĺ :

¿ èą@ : öU Alt-x (PÉ öU Alt Î x ) Î Ctrl-]-c (PÉö U Ctrl Î ] , Aö U

c ) , ð^ MS-Kermit> čÜ Å ź , Aä J hangup , Yi Ï Æ Ú œ P ů Ý Terminal Server œu . œu áX {UC Tğ :

The Phone or Network Connection should have hang up

źÉÆÚ œW ž OH Î CD üÜ O| űÀ , íÜ wœu .

¿ èą G : öU Ctrl-]-h (PÉ ö U Ctrl Î ] á , Aö U h ) , Yi Ï Æ Ú œ P ů Ý

Terminal Server œu , ^ì MS-Kermit> čÜ Å ź , ÆÚ œ Wž OH Î CD üÜ O ç

|űÀ , íÜ wœu .

jć ąœu èą çA ÎóQ Î TCP/IP Ïì ôô Pů ÝDœ su žąÎ ď .

2.2 By TCP/IP Local Area Network

MS-DOS KERMIT çä ľÏ ÎÏ ìô ô (Local Area Network) PůÝ Dœ su . bşh Ïì ô

ôď , TCP/IP ôô OØ eÌ űM ž@ Ø , ]O |ž ôô ÐÇ , ]źÚ ÌH TCP/IP ôô řű Ð ïH .

ż‘ą úÏÎ TCP/IP ôôs ţů ÝD œžs uÎ œu{ Ç . suè ąiÀ âØ :

1. òż suè ą : ÏÎ MS-DOS KERMIT RO vBź ĺ .

2. ÛÊ suè ą : ÏÎ MSKERMIT.INI (tÎ Òl É ) Î MSCUSTOM.INI (ÏÎÌÛ wÒ l É ) ž\àź ĺ .

œu èą iÀ řěi ąÎ jćą âØ .

2.2.1 Step-By-Step Connection

òż su èą iÀř HU BJ :

1. ]w TCP/IP ôôU ţÑ Æ .

2. üw ýsţ ůÝ Dœ ğ IP WÙ Îì } . 3. sţ ůÝD œ .

ÐÑ \U Ò .

Ò : ÏÎ TCP/IP ôôsţ ďą ãs| Dœ gate.sinica.edu.tw (HUš Ùř gate ) òż su {Ç pU : (HU RO ąb MS-Kermit> čÜ Åź áä J )

¿ BJ @ : äJ set tcp/ip address 140.109.7.163
¿ BJ G : äJ set tcp/ip subnetmask 255.255.255.0
¿ BJ T : äJ set tcp/ip broadcast 140.109.1.255
¿ BJ | : äJ set tcp/ip primary-nameserver 140.109.1.10
¿ BJ ŋ : äJ set tcp/ip gateway 140.109.1.10
¿ BJ ż : äJ set tcp/ip domain sinica.edu.tw
¿ BJ C : äJ set port tcp/ip gate
¿ BJ K : äJ connect ąú :

¿ BJ @ : set tcp/ip address RO Î óü wØ eÏ Î ğ PC ž IP ì} , ÐV ô ôÞ z Ìd SSzÏ Î PC ž IP ì} .

¿ BJ GÜż žU ţÑ ÆÈÐ Vô ôÞz Ìd SS .
¿ BJ C : set port tcp/ip RO Î ó ü wÏ Î TCP/IP ôô s ţ ů Ý Dœ , źR O ž Ï

Îè ąpU :

set port tcp/ip [ýsuž ůÝ Dœ WÙÎ IP ì} ]

bż Òď , iä J set port tcp/ip gate Î set port tcp/ip 140.109.14.2 .

¿ BJ K : äJ connect RO á Yi J Œ Ýœ Ò Àe ś , Pů ÝD œ gate su , ÃX { U CT ğ :

UNIX(r) System V Release 4.0 (gate)

login:

íů ÝDœ gate ž login TğX {á , äJ username Î passwd , Yi} lu@ .

2.2.2 Automatic Connection

P 2.1.2. ‘ÏÎğ ìz ÛP . ÛÊs uèą NW @‘ Òz BJ@ Üż ž TCP/IP ôôÑ Æ] w RO[ J MSCUSTOM.INI (ÏÎ ÌÛ wÒ lÉ ) ď , bCÿ ÒÊ MS-DOS KERMIT É , Ki Û Êź ĺò żs uBJ @Ü żžu @ .

b MSCUSTOM.INI ÉŒ ď ç w q@ telnet ĺř R O , iõ æ ò ż su B J C Î K , ÛÊ sţ ůÝ Dœ .

źĺH Wâ B Já , ib ÒÊ MS-DOS KERMIT ğá , ÏÎ telnet ĺř RO , Yi Pů Ý Dœ su .

Ò : ÏÎ TCP/IP ôôsţ ďą ãs| Dœ gate.sinica.edu.tw (HUš Ùř gate ) ÛÊ su {Ç pU :

¿ BJ @ : NW @‘ ďB J@Ü żž TCP/IP ôôÑ Æ] wRO [J MSCUSTOM.INI ď .
¿ BJ G : ÒÊ MS-DOS KERMIT
¿ BJ T : b MS-Kermit> čÜÅ źá äJ telnet gate

BJ@ Èůb ìÿ ÏÎÉ ]w , Há ÏÎ ÉÈ ůõæ BJ GÎT Yi . ąú :

¿ BJ T : telnet ĺřR Ož ÏÎ èąp U :

1. èą@ : telnet [ůÝDœ WÙ ] 2. èąG : telnet [ůÝD œž IP ì} ] 3. èą T : Èä J telnet ĺř R O , äá č [ ô ó Ñ Æ : ÏÎ e @ ÿ su ž ů Ý D œ WÙÎ IP ì}A ÿsu .

bż Ò ď , äJ telnet gate á , ýõ æ set port tcp/ip gate RO , üw q T ð ř

TCP/IP ôô , Ãü w ý s ţ ž ů Ý Dœ ř gate ; Má õ æ connect RO , iJ Œ Ý œ

ÒÀ eś , Pů ÝDœ gate su , ÃX {U CTğ :

UNIX(r) System V Release 4.0 (gate)

login:

íů ÝDœ gate ž login TğX {á , Yi äJ username Î passwd, }lu @ .

2.2.3 Hangup

œu è ą i À ř ě i ą Î j ć ą G Ø , bź ť H s ţ ď ą ã s | D œ gate.sinica.edu.tw (HU šÙ ř gate ) řÒ :

1. ěi ąœu :

bůÝD œ gate žčÜÅ ź gate:~> áäJ logout , Yið^ MS-DOS KER-

MIT, źĺœ u .

2. jć ąœu : iÎ HU âØè ąF ĺ :

¿ èą@ : öU Alt-x (PÉ öU Alt Î x ) Î Ctrl-]-c (PÉö U Ctrl Î ] , Aö U

c ) , ð^ MS-Kermit> čÜ Å ź , Aä J hangup , Yi P ů Ý Dœ gate œu . œ

uáX{ UC Tğ :

    The Phone or Network Connection should have hang up

¿ èąG : öU Ctrl-]-h (PÉöU Ctrl Î ] á , Aö U h ) , Yi Pů ÝDœ gate œ

u , ð^ MS-Kermit> čÜÅ ź .

jć ąœu èą çA ÎóQ ÎÆ ÚœP ůÝ Dœ suž ąÎ ď .

Yz ž PC WP É Ë ş Æ Ú œ (mkidxModem) Î TCP/IP ôô d , hi Ï Î ä ď @ Ø Ë m PY @ů ÝD œsu á , AÏÎ t@ ËmP t@ ůÝ Dœs u , ÐÑ\ þý B ğą ú .

Chapter 3

Main Functions of MS-DOS KERMIT

MS-DOS KERMIT čÑ ž D n \ à ] A Œ Ý œ Ò À Î É Œ Ç e , żź N ą ú p ó Ï Î ź â ţ

\à .

3.1 Terminal Emulation

b MS-Kermit> čÜ Åźá äJ connect (išg ř c ), KiJ ŒÝ œÒ ÀňA . ż‘ Ną ú

MS-DOS KERMIT čÑ ž Œ Ý œ Ò À \ à , ]A : ŒÝ œ Ò À e ś T ğ Î ä ò ż Þ @ , ÈÉ Á

ńÜ MS-KERMIT Î MS-DOS, ØSShÓ Sessions ,Îå rŒ Ýœ PÏÎ ŒÝ œğÁ ń ....ě .

3.1.1 Basic Operations

b MS-Kermit> čÜÅź áä J connect , Ki JŒ ÝœÒ Àň A , eśÌ Uè ş@æ ÏÕ ž ňA C (Status Line).

YÏÎ ÆÚœ (Modem) Pů ÝDœ su , źň AC Tğ pU :

Esc-chr:^] help:^]? port:2 speed:19200 parity:none echo:rem VT220 ...

YÏÎ TCP/IP ôôP ůÝD œs u , źňA CT ğpU :

Esc-chr:^] help:^]? 1:gate parity:none echo:rem VT220 ...

ňA Cď Uæ ìNq pU :

1. Esc-chr : öU Ctrl-] (PÉ ö U Ctrl Î ] ), Yi J Èœ Ò ą (Escape-Level Mode) ňA ,

iA äJY @r ÿ (Character) , õæü wğ ÈœÒ ąR O .

2. help: öU Ctrl-]-? (PÉ öU Ctrl Î ] ä , Aö U ? ), ÌWèY X{ HÏ Õèą ãÜ ğ

Èœ ÒąR Ou Wš Uąú (On-Line Help) Tğ pU :

? This message F Dump screen to file
C Close the connection P Push to DOS
S Status of the connection Q Quit logging
M Toggle mode line R resume logging
B Send a Break 0 Send a null
L Send a Long 1.8 s Break H Hangup phone
A Send Telnet ’Are You There’ I Send Telnet ’Interrupt Process’
Typing the escape character will send it to the host ....

źT ğ ą ú U È œ Ò ą R O ğ N q , ÌU è Ã ş @ Command> čÜ Å ź , Ñä J È œ Ò ąR OÎ , ‘Î ÈœÒ ąR ON óyá ąú .

3. qT Ñ Æ : iÀ řÏ Î ÆÚ œ su ÎÏ Î TCP/IP ôô s uâ Ø . YÏ ÎÆ Ú œs u , h ãÜ Ç C ð s ź Î RS-232 PÆ Ú œ ğ ą ž Ç é t Œ , bż Ò ď ř port:2 speed:19200 . YÏ Î TCP/IP ôô su , hã Ü Session sźÎ su DœW Ù , bżÒ ďř 1:gate .

4. Parity : ąúsu ÏÎ žPì èą .

5. Echo : ąú su ÏÎž Tğ ^ş èą .

6. ÒÀ ŒÝœ ňą : bż Òďř VT220.

bŒÝ œÒ Àň Aď , MS-DOS KERMIT wÄÏ ži O ýÌ ñQ űž ŒÝ œÒ Àe śž e , öU PgUp Î PgDn ä , Yib W / UQű ždò ąš Ê .

b MS-Kermit> čÜ Å ź á ä J show terminal , id SS Œ Ý œ Ò À ň A Uţ Ñ Æ ] w Tğ pU :

Terminal type: VT100 Display: Regular, 8-bit
Mode-Line: on Escape character: ^]
Term Tek4010 (auto-entry): enabled Keyboard translation: on
     . .
     . .
     . .

ÈœÒ ą R O (Escape-Level Mode Command) žØ žb ó : ÏÎ \ àä N í Y Ç ‘Î R O , Ïz č ů œ } ŒÝ œ Ò À ň A , Ki õ æ PŒ Ý œ Ò À ň Aş ö ž R O . ńn ž È œ Òą R O pU :

¿ Ctrl-]-c : PÉ öU Ctrl Î ] ä , AöU c , iÈÉ æ œ s u ňA , ^ì MS-Kermit> č

ÜÅ źU , ÐÑ \ 3.1.2. ‘ąú .

¿ Ctrl-]-s : PÉ öU Ctrl Î ] ä , AöU s , idSS Øe suň AU ţÑ Æ]w Tğ pU :

    Speed: 19200 Terminal Type: VT220
    Communications Port: TCP/IP Mode-line: on
    Parity: none (8-bit data) Send Packet size (maximun): 9024
    Local echo: off Receive Packet size (maximun): 9024
          . .
          . .
          . .

¿ Ctrl-]-m : PÉ öU Ctrl Î ] ä , Aö U m , iÏňA Cø ćÎX { , ř@ Áń (Toggle)

RO .

¿ Ctrl-]-f : PÉ ö U Ctrl Î ] ä , Aö U f , iN Ø e Ã õ ď ã Ü ž T ğ O ý ó KER-

MIT.SCN ÉŒď , iÎ óO ýŒÝ œÒ ÀL { , ÐÑ\ þý D ąú .

¿ Ctrl-]-p : PÉö U Ctrl Î ] ä , Aö U p , iÈ É æ œs u ň A , ^ì C:n> čÜ Å ź

U , ÐÑ\ 3.1.2. ‘ą ú .

¿ Ctrl-]-q : PÉöU Ctrl Î ] ä , AöU q , iÈś OýŒ Ýœ ÒÀ L{ , ÐÑ\þ ý D

ąú .

¿ Ctrl-]-r : PÉ öU Ctrl Î ] ä , Aö U r , iń sÒ Ê] öU Ctrl-]-q ÒÈ ś žO ý

ŒÝ œÒÀ L{ , ÐÑ \þ ý D ąú .

¿ Ctrl-]-h : PÉöU Ctrl Î ] ä , AöU h , iSSèj ćÁ _ (hangup) Øež su ňA .

HW È œ ň A R O ď , Ctrl-]-c iÑ Alt-x úN ; Ctrl-]-s iÑ Alt-s úN , Ctrl-]-h iÑ Alt-h úN . Ctrl-]-r iÑ Alt-r úN . Ctrl-]-q iÑ Alt-q úN .

3.1.2 Temporarily Switching to MS-DOS KERMIT or MS-DOS

ÛŒ Ýœ ÒÀ ňAÈ ÉÁ ńÜ MS-DOS KERMIT , iÌU CB JÞ@ :

¿ BJ @ : bŒ Ý œ Ò À ň A ď ä J Ctrl-]-c (PÉ ö U Ctrl Î ] , Aö U c ) Î Alt-x (PÉö U Alt Î x ) , YiÈ É ^ì MS-Kermit> čÜÅ źď , źÉ Pů ÝD œ ťO ù s uň A .

¿ BJ G : b MS-Kermit> čÜÅ źá äJ MS-DOS KERMIT RO , õæUţ u@ .
¿ BJ T : b MS-Kermit> čÜÅ źáä J connect (iY gř c ),Yi ^ì ìýž ŒÝ œ

ÒÀ ňA .

ÛŒ Ýœ ÒÀ ňAÈ ÉÁ ńÜ MS-DOS , iÌU CB JÞ@ :

¿ BJ @ : bŒ Ý œÒ Àň A ďä J Ctrl-]-p (PÉö U Ctrl Î ] , Aö U p ) , Yi È É ^ì C:n> čÜÅ źď , PÉ X{ MS-DOS žľżT ğ , źÉP ůÝ Dœ ťOù su ňA .

¿ BJ G : b C:n> čÜÅ źá äJ MS-DOS RO , õæU ţu@ .
¿ BJ T : b C:n> čÜ Å źá ä J exit , YX { Press space to continue... Tğ ,i ^

ìì ýžŒ Ýœ ÒÀ ňA .

3.1.3 Build Multiple Sessions in TCP/IP Network

b MS-DOS KERMIT ď , ÏÎ TCP/IP ôô P ůÝ D œs u É , iPÉ P żą D œs u , ØSS żÓ Session . ØSShÓ Sessions ž{Ç pU : (HÏ ÎÛ Ês uèą řÒ )

¿ BJ @ : Ì 2.2.1. Î 2.2.2. ‘ÒzB JP ůÝD œs u , ØSSÄ @Ó Session .
¿ BJ G : bÄ@ Ó Session ďöU Alt-x (PÉö U Alt Î x ) Î Ctrl-]-c (PÉö U Ctrl

Î ] , Aö U c ), iÈÉ ^ì MS-Kermit> čÜÅ źď .

¿ BJ T : b MS-Kermit> čÜÅ źá äJ telnet [ůÝD œž W ÙÎ IP ì} ] , YiP Ä Gą ůÝD œs u , ØSSÄ GÓ Session .

ÌÓW zBJ , i~òØ SSÄ T , | , ŋ , żÓ Session .

ØSS h Ó Sessions á , şp ó b č P ž Session ąÁ ń O ? un ö U Alt-n (PÉ ö U Alt Î n ) , YiÁ ńÜ U@Ó Session , ÑňA CT ğio ¿Ø ež Session sź Îsu Dœ WÙ .

ýP @ D œ Ø SS h Ó Sessions Session , ťi Ì B J @ Ü T ä J R O , ýb B J T ä J tel-

net [ůÝ Dœ žWÙ Î IP ì} ] á , |X{U CT ğ :

status session hostname
current > 1 gate

Choices R Return to active session
          1..6 Pick a new or existing session
          N Start a new session (default)

Choice>

źÉå Ð|ś db Choice> čÜÅź á , ěÝéJ ïţ : äJ R , ið^ ìÓ wØSS su ž

Session ď ; äJ 1 Ü 6 žÆr , ið^ü w Session ď , ÎØ SSsž Session ; ¡ţ öU Enter

Î N , YiP źDœ ØSS sž Session .

3.1.4 Text v.s. Graphical Terminal

ŒÝ œň ąi Àřå r (Text) ÎÏÎ (Graphic) âj þ , MS-DOS KERMIT iÒ Àźâ þŒ Ý œ . år ŒÝ œD nř VT tCŒ Ýœ , Òp : VT100, VT220 , ... ě . ÏÎ ŒÝ œH Tektronic tC ř D , ýâ Ì L k P É ã Ü . ]ź b Ï Î ÿ Ï n é (Òp : GNUPLOT , MATLAB , ...ě ) É , RO ąÀş bå rÒą Uä J , ÏÎãÜ ąÀ şbÏ ÎÒ ąď iæ , öU Alt- - (PÉö U Alt Î - ) Yib âØ ŒÝœ ąÁ ń .

ÏÎÏ ÎŒÝ œÉ šů ‘N : čibď åt ÎU ÏÎ ÏÎ\ à , _h NX {ÃX ÎL kÞ @ žù ~ą Î .

3.2 File Transfer

ÉŒÇ eO KERMIT Òč Ñž ÄG ţ Dn \à . MS-DOS KERMIT QÎU Cè ąi æ ÉŒ Ç e : 1. ÏÎ KERMIT ów . 2. ÏÎ øAź (Server) \à .

3. ÏÎ ~ąó w (Òp : ZMODEM Protocol ě ).

ż‘ Ną úH WUØ Çe èą .

3.2.1 Using KERMIT Protocol

í PC PůÝ D œ ąË m KERMIT né (MS-DOS KERMIT , C-KERMIT , .... ě ), BP É õ æÉ , KiÏÎ KERMIT ówÇ eÉ Œ . ÐÑ\U âÒ .

Ò@ : Ûď ą ãs | Dœ gate.sinica.edu.tw (HUš Ù ř gate ) Uü (Download) @å rÉ test Ü PC.

Çe {Ç pU :

¿ BJ @ : ÒÊ MS-DOS KERMIT.
¿ BJ G : QÎÄ GźÒ zs uè ą , ÏÎÆ ÚœÎ TCP/IP ôô P gate su .
¿ BJ T : b gate Dœč ÜÅ ź (gate:~>) áäJ kermit, õæ C-KERMIT.
¿ BJ | : b C-Kermit> čÜ Åź áäJ send test
¿ BJ ŋ : öU Alt-x (PÉ ö U Alt Î x ) Î Ctrl-]-c (PÉ ö U Ctrl Î ] , Aö U c ),

^ì MS-Kermit> čÜÅ źU .

¿ BJ ż : b MS-Kermit> čÜÅź áä J receive
¿ BJ C : ÝÇ e š ô á , b MS-Kermit> čÜ Å ź á ä J connect (iY g ř c ), ^ì

gate Dœ .

¿ BJ K : b C-Kermit> čÜÅ źáä J quit Î exit , œ} C-KERMIT.
¿ BJ E : QÎÄ GźÒ zœ uè ą , P gate œu , ^ì MS-Kermit> čÜÅ ź .

ąú :

¿ BJ T : C-KERMIT ř UNIX ľż ž KERMIT, äD n R O P MS-DOS KERMIT ÛP .

b gate Dœ WÒ Ê C-KERMIT á , X{U CT ğ :

C-Kermit 5A(189), 30 June 93, Solaris 2.x
Type ? or HELP for help
C-Kermit>

C-Kermit> ř C-KERMIT žtÎ čÜ Åź , äá iäJ C-KERMIT RO .

¿ BJ | : send RO Î ó N @ Ó Î h Ó É Œ e Ü ů Ý KERMIT Îø A ź (Server) , ÏÎ èą pU :

send [ýÇe žÉŒ WÙ ]

ýÇ ehÓ ÉŒ É , iÏÎ #, *, Î ? ěqÎ rÿ (Wildcard Character) íÜ ÉŒ WÙ , Î kp U :

1. ? : Îó ÀN @rÿ , ýčo ÎóÀ NÉ ŒWÙ žÄ @Ó rÿ . 2. * : Îó ÀN ÆÓr ÿ .

3. # : ÎóÀ N@ rÿ , ýÈ Îó ÀNÉ ŒW ÙžÄ @Ó rÿ .

Ð‘ N : b C-KERMIT ďÈà ÏÎ * qÎ rÿ .

żÒ ď , b C-Kermit> čÜÅ źáä J send test á , |X {UC Tğ :

Return to your local Kermit and give a RECEIVE command

KERMIT READY TO SEND ....

źÉ iöU Alt-x (PÉöU Alt Î x ) Î Ctrl-]-c (PÉö U Ctrl Î ] , AöU c ), ^ ì MS-DOS KERMIT, Hõæ receive RO .

¿ BJ ż : receive RO Îó ţ ňÛ ů Ý KERMIT ÇÓ žÉ Œ . Yů ÝÉ Œ ÉW Pż a É ŒÉ WÛP É , ib receive ROá üw ţňÉ WH QÏÀ .

żÒď , b MS-Kermit> čÜ Å ź á äJ receive á , Y}l Ç e ÉŒ , PÉ X{ U C T ğ :

      MS-DOS Kermit : 3.13 8 July 1993 patch level 21

          File name : test as test
          File type : text, Transparent to CP437
       Current path : C:\KERMIT
 KBytes transferred :
Percent transferred :
                  % :
          Receiving :

  Number of packets :
      Packet length :
  Number of retries :
         Last error :
       Last message :

File name æď , eÌ řůÝ Dœ gate WžÉ ŒÉ W , ář MS-DOS KERMIT žţ ňÉ W . File type ãÜ Ç e ê Æ æ ą (żÒ ď ř å Æ r (text)), ÏÎ r ř W Ù (żÒ ďř CP437),

Î¡ űèą (żÒ ďř Transparent).

Current path ãÜ MS-KERMIT ØeÒb ô| ì} . KBytes transferred ãÜ Øew Çe ÉŒ øŒ . Percent transferred ãÜ ÉŒ Øew Çe ÊÀ ñ . Number of packets ãÜØe wÇ eğÊ ]Æ Ø . Packet length ãÜ Øe Çeğ Ê] øŒ . Number of retries ãÜ ØeÇ eÊ ]žń eÿ Æ .

ÉŒ Ç e šô É , MS-KERMIT |o X@ } Í n ; Receiving æX { Completed Tğ ; Çe tŒ (chars/sec) ÎW eÏ Îv (Channel Utilization) ěÎp Ær |PÉ ãÜ ; Last message æď X{ï źţ ňÉ ŒžB zè ą ; Má^ ì MS-Kermit> čÜ Åź . YÉ ŒÇe ćÑ É , Last error æď| X{ù ~ì ] .

ÒG : Û PC Wü (Upload) @å r É test Üď ą ã s | D œ gate.sinica.edu.tw (HU š Ù ř

gate )

Çe {Ç PÒ @ÛP , ýUCB Jč ~ :

¿ BJ | : b C-Kermit> čÜ Åź áäJ receive
¿ BJ ż : b MS-Kermit> čÜÅź áä J send test

ąú :

¿ BJ | : receive RO ą ú i Ñ \ W @ Ò ď B J ż ą ú . b C-Kermit> čÜ Å ź á ä J

receive , X{ UC Tğ :

Return to your local Kermit and give a SEND command

KERMIT READY TO RECEIVE ....

źÉ iöU Alt-x (PÉöU Alt Î x ) Î Ctrl-]-c (PÉö U Ctrl Î ] , AöU c ), ^ ì MS-DOS KERMIT, õæ send RO .

¿ BJ ż : send ROą ú i Ñ \ W @ Ò ď B J| ą ú . äJ send test áX{ P W @ Ò ďB JżÛ Pž Tğ .

HWâ ÓÒl wï póÏ Î KERMIT ówÇe ÉŒ @@ ąú . ţU ÓÚ ÌN űÐX Ób Ç eL {ď ‘Î žRO :

1. jć ď_É ŒÇ e : ibÇe L{ ďHU Cè ąF ĺ :

¿ öU x : ď_iæ ďž ÉŒÇ e , õæ U@Ó ÉŒ Çe .
¿ öU z : ď_i æď ÎHá žÉ ŒÇe .
¿ öU c : ď_i æď ÎHá žÉ ŒÇe , ÃSSY ^ì MS-Kermit> čÜ Åź .

2. üw É ŒÇ eæ ą : iÎ set file type ROü w . źR Oš ůb send Î receive ě ÉŒ Ç e R O e õ æ . MS-DOS KERMIT Î C-KERMIT bÒ Ê É w N É Œ Ç e æ ą ž wř åÆ r (Text) æą . ]ź : YÇ eå Ær æą ÉŒ , hčů äJ ôó üw ÉŒ Çe æ ąž RO ; YÇ eG iì (Binary) æąÉ Œ , hş ÀOb eX Ýž send ROÎţ ňÝ ž

receive RO eýä J set file type binary , Hü w£T žÉ ŒÇ eæą .

3. üw P W É Œ ž B z è ą : Ye X É Œ É W P ţ ň Ý ì ş É Œ P W É , iÏ Î set file

collision RO üw Bz èą . b MSKERMIT.INI tÎ Òl Éď ]wř : set file collision rename , ]ź MS-DOS KERMIT |Û Ê Nţ ň É Wó ï (rename) řsW Ù . ý

ïÜ źţ] w , ib MS-Kermit> čÜÅź áä JHU RO :

¿ set file collision overwrite : ţň Ý |N ţň ÉŒ Ðg (overwrite) bì şÉ Œ

W , ìÉ Œx sžê Æ| øć .

¿ set file collision discard : ţňÝ |Nţ ňÉ ŒľH SSó , č[ xs .

3.2.2 Using Server

ÏÎ KERMIT ówÇ eÉ Œž B JQ ÀÆ ø , šů č_ b PC Pů ÝD œą Áń . ]ź KER- MIT tč Ñ @ø Aź (Server) \à , iÏ ÉŒ Ç eB J þą b PC Ýźĺ . ÏÎø A ź\ à ž BJ pU :

1. bů ÝDœ Wõ æ KERMIT žø Aź \à . 2. b PC PůÝD œą ÇeÉ Œ . 3. öň ůÝD œW žø Aź\ à .

ÐÑ \U Ò .

Ò : ÏÎøA ź\ à , Nå rÉ test1 Ñ PC Wü (Upload) Üďą ãs |Dœ gate.sinica.edu.tw (HUšÙ ř gate) , ANå rÉ test2 Ñďąã s| Dœ gate Uü (Download) Ü PC. Çe {Ç pU :

¿ BJ @ : ÒÊ MS-DOS KERMIT.
¿ BJ G : QÎÄ GźÒ zs uè ą , ÏÎÆ ÚœÎ TCP/IP ôô P gate su .
¿ BJ T : b gate Dœč ÜÅ ź (gate:~>) áäJ kermit , õæ C-KERMIT.
¿ BJ | : b C-Kermit> čÜ Åź áäJ server
¿ BJ ŋ : öU Alt-x (PÉ ö U Alt Î x ) Î Ctrl-]-c (PÉ ö U Ctrl Î ] , Aö U c ),

^ì MS-Kermit> čÜÅ ź .

¿ BJ ż : b MS-Kermit> čÜÅź áä J send test1
¿ BJ C : b MS-Kermit> čÜÅ źá äJ get test2
¿ BJ K : ÝÇe š ôá , b MS-Kermit> čÜ Åź áä J bye, ÏůÝ D œ gate æœ ø A

źň A , ÃÁ_ PůÝ Dœ gate žsu .

ąú :

¿ BJ | : äJ server á , |X{ UCT ğ :

    Entering server mode. ...... Use SEND and GET for file transfer.
    Use REMOTE HELP for a list of other available services. Use BYE or
    FINISH to end server mode.

    KERMIT READY TO SERVE ....

íÜ gate Dœw iJø Aź ňA , iţ üø AźR O .

¿ BJ ż : send RO Îó N@Ó Îh ÓÉŒ eÜ ůÝ KERMIT ÎøA ź , ÐÑ \ 3.2.1. ‘ Ò@ ďBJ |ž ąú .

¿ BJ C : get RO Î ó n D ů Ý ø A źN @ Ó Î h Ó É Œ Ç e Ü ż a KERMIT , ÏÎ è ąp U :

get [ýţ ňž ÉŒW Ù (@ÎhÓ ) ]

YQ ïÜţ ňÉ ŒÉ WÉ , ÈÝ äJ æ@ get ROY i , źÉ |ýX { Remote Source File: Tğ n D é J ů Ý É Œ W Ù , AX { Local Destination File: Tğ n D é J ż a É Œ WÙ , Yi [H ïÜ .

¿ BJ K : bye ROi źĺU CT BJ :

1. ÏůÝD œæ œøA źň A . 2. ÏůÝD œœ } KERMIT.

3. ÛůÝD œ logout , ÃÁ_P ůÝ Dœ žsu .

Ñż Òď i ¿ : íů ÝD œ Ò Ê KERMIT, Ãi J øA ź \à É , Èů b PC ÝÏ Î send Î get ROY iź ĺÒş ÉŒ Çeu @ , û 3.2.1. ‘Òzè ąó řK ű .

ţUÓ űÐX Ób ÇeL {ď ‘Î žRO :

1. üw É ŒÇ e æą : ÏÎ ø Aź \ àÇ e ÉŒ É , žw ÉŒ æ ąř å Ær æ ą . Yn Ç e Gi ìæą ÉŒ , şb MS-DOS KERMIT Ýž send Î get RO eä J set file type

binary Î remote set file type binary RO , Ï PC ÎůÝ øA źą ïÜř Çe G

iì æąÉ Œ .

2. bye P finish ROž ÏO : bye ROÒ źĺž u@ wÔ zó BJK žą ú . b MS-DOS

KERMIT ďt č Ñ @ finish RO , çi Ï ů Ý D œ æ œ ø A ź ň A . âÌ ž Ï O b ó :

finish RO È Ï ůÝ D œæ œ ø Aź ň A , ýčœ } C-KERMIT , çčõ æ Ûů Ý D œ

logout žu@ .

]ź , YzbÇ eÉ Œá čA PůÝ Dœ Où suÉ , iÏÎ bye RO ; Yz bÇ eÉ Œ áť ÝPů ÝD œs uÉ , şÏ Î finish RO . øAź |čÑ äL ÉŒA È\ à , ÐÑ\ þý G .

3.2.3 Using ZMODEM Protocol

MS-DOS KERMIT çä ľÏÎ ~ą ów ÇeÉ Œ , bźH ZMODEM ówřÒ .

í PC PůÝ Dœ ąËm ZMODEM né (b PC Wř DSZ.COM , b UNIX ôÒ ďř rz Î

sz ), BPÉõ æÉ , Ki ÏÎ ZMODEM ówÇe ÉŒ .

Ð‘N : ZMODEM ówÈ AÎ óÏÎ ÆÚ œPů ÝD œs užą Î , Lk şÎ óH TCP/IP ôô su žą Îď .

ÏÎ ZMODEM ów Çe É Œe š ůý N DSZ.COM {ąw Ë Ü C:n>KERMIT Øý U , Ã Tw RZ Î SZ {ąb UNIX ôÒ žj M ô | (PATH) ž . Má N U C rz Î sz ĺřR O w q [J MSCUSTOM.INI ÏÎ ÌÒl Éď :

define rz run dsz F ha on port 2 G rz -r %1 define sz run dsz F ha bo port 2 G sz %1 %2 %3 %4 %5 %6 %7 %8 %9

YÆ Úœ ÃD Ëmó ÇC ð com2 , ÐN port ğáž ÑÆ ïřÛ ïş žÆr .

źĺW z ] w á , Ðń s Ò Ê MS-DOS KERMIT, Îb MS-Kermit> čÜ Å ź á ä J take

mscustom.ini , Yiü J rz Î sz ĺř ROw q , }lÏ Î . ÐÑ\ HUG Ò .

Ò@ : Ûď ą ãs | Dœ gate.sinica.edu.tw (HUš Ù ř gate ) Uü (Download) @å rÉ test Ü PC.

Çe {Ç pU :

¿ BJ @ : ÒÊ MS-DOS KERMIT.
¿ BJ G : ÏÎ 2.1. ‘Òzè ą , ÏÎÆ Úœ P gate su .
¿ BJ T : b gate Dœč ÜÅ ź (gate:~>) áäJ sz test
¿ BJ | : öU Alt-x (PÉö U Alt Î x )Î Ctrl-]-c (PÉ ö U Ctrl Î ] , Aö U c ),

^ì MS-Kermit> čÜÅ źU .

¿ BJ ŋ : b MS-Kermit> čÜÅź áä J rz
¿ BJ ż : ÝÇ e š ô á , b MS-Kermit> čÜ Å ź á ä J connect (iY g ř c ), ^ì

gate Dœ .

¿ BJ C : QÎ 2.1.3. ‘Òz œuè ą , P gate œu , ^ì MS-Kermit> čÜÅ ź .

ąú :

¿ BJ T : sz RO i Ï Î ZMODEM ów N É Œ e X . żÒ ď ä J sz test áX { U C T ğ :

sz ready. Type ’rz file ....’ to your modem program

źT ğUè ià |X {@C Ñr ÀPÆ rc ĺž ÃX , ř£ ‘{H , Ð~òÞ @ .

¿ BJ ŋ : rz ROi ţň ZMODEM ówÇ Óž ÉŒ . żÒ ďä J rz áX{ UCT ğ : (T ğe ž 01, 02, 03, .... řæ ź )

01 DSZ.COM Copyright 04-26-94 by Omen Technology INC
02 ’The High Reliability Software’

03 DSZ Registration and Documentation: $20 Check/MO
04 Omen Technology Inc, P. O. BOX 4681, Portland OR 97208

05 VISA/MC ZERO PAPERWORK Registration! Data: 503-621-3746
06 VOICE: 503-621-3406

07 COM2 9600 bps Carrier Detect enabled Handshake both S/N 0
08 Command line =’F ha on port 2 G rz -r’
09 total: 3000 bytes Estimated 0.2 Min
10 test: 3000 bytes Estimated 0.1 Min

Ä@ Üż æą ú DSZ.COM {ąž ľż Tğ . ÄC , Kæą ú DSZ.COM {ą žÑ Æň A ÎR O . ÄE , Qæą úw pÇ eÉą . Má }lÇ eÉ Œ , ÃX{ UC Tğ :

1024 ZMODEM CRC-32

íÜ C@Ê ]ø Œř 1024 bytes, ÏÎ CRC-32 żùr ÿ . ÉŒ Çeš ôá X{ UCÇ eÉ ąÎt Œž Îp Tğ :

Closing test 3000 chars 0.06 min 757 ch/sec
Ending ZMODEM session

ÃX { DSZ FINISHED! exit code=0 Tğ , Má^ ì MS-Kermit> čÜ Åź U .

ÒG : Û PC Wü (Upload) @å r É test Üď ą ã s | D œ gate..sinica.edu.tw (HU š Ù ř

gate )

Çe {Ç PÒ @ÛP , ýUCB Jč ~ :

¿ BJ T : b gate Dœč ÜÅ ź (gate:~>) áä J rz
¿ BJ ŋ : b MS-Kermit> čÜ Åź áäJ sz test

ąú :

¿ BJ T : äJ rz áX{ UC Tğ :

    rz ready. Type ’sz file ....’ to your modem program

źT ğUè ià |X {@C Ñr ÀPÆ rc ĺž ÃX , ř£ ‘{H , Ð~òÞ @ .

¿ BJ ŋ : äJ sz test áX{P Ò@ ďB Jŋ ÛPž Tğ , ý Command line áž RO ř :

F ha bo port 2 G sz test

HWâ Ó Ò l w ï p ó ÏÎ ZMODEM ów Çe É Œ @ @ ą ú . ţU Ó Ú Ì N űÐ X Ó b Çe L{ ď‘ ÎžR O :

1. Çe h Ó ÉŒ : ib sz ğá[ W @Ó Î hÓ ý Ç ež É ŒW Ù , Ãi Ï Î ? , * ěq Î rÿ (Wildcard Character).

2. óïţ ň É Œ É W : Yţ ň É Œ P {s É Œ P W É , ib rz ğá [ W ý ţ ňž É W , _ hN oÍÐ g (Overwrite) ž{H .

Chapter 4

Advanced Usage

Ä@ ź Ü Ä T ź w ï MS-DOS KERMIT čÑ ž ò ż R O @ @ š ű , żź N ű Ð p ó i @ B ÏÎ MS-DOS KERMIT . 4.1. ‘ą ú MS-DOS KERMIT čÑ ž ĺ ř R O (Macro) Î Script

Programming \à , 4.2. ‘hą ú@ Ç‘ ÎRO .

4.1 Macro Command and Script Programming

MS-DOS KERMIT čÑ wqĺ řR O (Macro) Î Script Programming ž\à . ĺřRO ON Y

@s R O ř X b @ _ , H@ ĺ ř WÙ N í , Is ź ĺ ř W Ù É , KÌ w q è ą õæ o @ s R O , Fìö ó ÏÎ ž Øž . Script Programming hO HR O ÉŒ (Command File) Îą , BÎÜ Æ Î śî y{ ěè k , Fìş Î{ą žÄ G . HUÀ Oąú ğ .

wqĺ řRO žè kpU :

define [ĺř ROW Ù ] [wq že ]

Is ĺř R O É , ÈÝb MS-Kermit> čÜÅ ź áä J ĺ řR O W Ù , K|Ì w qž e õ æ RO .

H MSCUSTOM.INI ÏÎÌ Ûw Òl Éďw qž ĺřR O tsend řÒ , wq pU :

define tsend set file type text, send n%1 n%2

ĺř R OW Ù ř tsend , Øž b Û Êe X å Æ r (text) ÉŒ . wq ž e ř set file type

text Î send n%1 n%2 âRO , n%1 Ü n%9 Ní Isĺ řR OÉ äáñ Hž ÑÆ , n%0

Ní ĺř RO WÙ . b MS-Kermit> čÜÅ źáä J : tsend [ýÇ ežå Ær ÉŒ WÙ ] , Kõ æ set file type text Î send n%1 n%2 âRO .

MS-DOS KERMIT čÑ HU Æþ Script Programming \à :

1. éJ / éX : Òp ask , input , output ... ě . 2. wq ÜÆ : Òp assign , define ě . 3. âN Bâ : Òp increment Î decrement ě . 4. Þè Bâ : Òp not , if = , if ¡ , if ¿ .... ě . 5. jô śî : Òp goto [label] , count ě . 6. ÉŒ łg : Òp open , read , write , close ě . õæ Script ÉŒž èkp U :

take [Script ÉŒWÙ ]

ÔÓR OÐ Ñ\ C. M. Gianone ÒÛ ’Using MS-DOS KERMIT’ @ÑÎ KERMIT.HLP ÉŒ , źBÈ H@Ò ąú .

Ò : H@ Script ÉŒ autoconn ÛÊźĺ ÏÎ ÆÚœ Î TCP/IP ôôPů ÝD œsu žu @ .

autoconn ÉŒž epU : (01, 02, 03, ... ěř æź )

01 comment Main Menu for AutoConnect Script

02 :choose
03 cls
04 echo { WELCOME TO AUTOMATIC CONNECTION FUNCTION!}
05 echo
06 echo { Connection Method:}
07 echo
08 echo { 1. By MODEM}
09 echo { 2. By TCP/IP Network}
10 echo { 3. Return to MS-DOS KERMIT}
11 echo
12 ask \%a { Please Enter Selection: }
13 echo

14 comment Branch Part

15 if = \%a 1 goto modem
16 if = \%a 2 goto tcp
17 if = \%a 3 end
18 goto choose

4.1. MACRO COMMAND AND SCRIPT PROGRAMMING 43

19 comment MODEM Connection

20 :modem
21 echo
22 ask \%b { Please Enter Alias Name or Telephone No.: }
23 if equal \%b " " goto modem
24 echo
25 dial \%b
26 connect
27 goto choose

28 comment TCP/IP connection

29 :tcp
30 echo
31 ask \%c { Please Enter Host Name or Host IP Address: }
32 if equal \%c " " goto tcp
33 echo
34 telnet \%c
35 goto choose

ýõæ ź Script ÉŒ , ÈÝb MS-Kermit> čÜÅź áä J take autoconn Yi .

ąú :

¿ Ä 1 æ : comment řùÑR O , Îóy ž , íÜż æ@ řù ÑÎ , äž ečľ õæ .
¿ Ä 2 æ : _ź : Îó ù ú Ð O (label) , äá ř Ð O W Ù . P goto RO X Î É , iź ĺ

Unconditional Jump .

¿ Ä 4 æ : echo RO iN üwr êÎ ÜÆ žeã Ü (display) óÃõW . ÎkpU :

echo frê že gÎ ÜÆW Ù

rê e áş H Aů f Î g]ò , ÜÆ Nó HU ž eą ú . Èş @ Ó echo É , íÜL X @ CÅ Õæ .

¿ Ä 12 æ : ask ROÎ óæ Íą (Interactive) éJ . Îkp U :

ask [ÜÆW Ù ] fčÜrê že g

MS-DOS KERMIT žÜÆ iÀ řHU |þ :

1. n%a Ü n%z : Script ÉŒ žw (Built-in) žþì (Global) ÜÆ .

2. nm(Var Name) : řÏ ÎÌ Ûw (User-Defined) ÜÆ . iQ Î assign Î define

RONY @Æ rÎr êÈ üw ÜźÜ Æď . nm(Var Name) řÞÎ ÏÎÌ Ûw Ü Æžèk , Aůžř ÜÆ WÙ .

3. nv(Var Name) : MS-DOS KERMIT tÎž wÜ Æ , ]A éÁ (date), Éą (time),

ÒbØý (working directory), .... ě .

4. n$(Var Name) : MS-DOS ôÒÜ Æ (Environment Variable).

¿ Ä 15 æ : if řÞè BâR O , iÀř HU Tþ :

1. PÆrş ö : ]A if = , if ¡ , if ¿ ... ě . 2. Pårş ö : ]A if equal , if llt , if lgt ě .

3. ňpP_ : ]A if success , if failure , if inpath , if exist .... ě . if ROÏ Îèą pU :

if [ÞèBâ ą ] [RO (@ ÎhÓ )]

Þè Bâą ąH prefix èąíÜ , æąpU :

[ÞèB âl (Operator)] [Bâ ÿ (Operand)] [Bâÿ ] YÞ èBâ Èř u (True), hõ æä ážR O . tÝ ‘N : MS-DOS KERMIT ÈčÑ not Bâ , čč Ñ and P or Bâ .

¿ Ä 17 æ : end Î stop ROi œ} Script ÉŒ , ð^ MS-DOS KERMIT. ÏO pU :

1. end RO : ^ìI sź ĺřÎ Script ÉŒž W@ hĺ řÎ Script ÉŒ ď ; YL , h^

ì MS-Kermit> čÜÅź .

2. stop RO : ¡ţ^ì MS-Kermit> čÜÅ ź .

4.2 Useful Commands

MS-DOS KERMIT čÑ \h] wt ÎÑ ÆžR O , bźN äÏ Àř Tjþ :

1. P MS-DOS şö žR O . 2. PŒ ÝœÒ Àň Aş öžR O . 3. PÉ ŒÇe şö žR O .

HU NU þR O , QÎ FAQ Îąą úÏ ÎÉœ ÎÏ Îè k .

4.2.1 MS-DOS Related Commands

MS-DOS KERMIT čÑ U C MS-DOS RO , ]A : cd , cls , delete , dir , type ěŋ Ó ; MSKERMIT.INI tÎ Òl Éď çş more , copy , rename ěT Óĺř RO wq ; HWR O

ąi óÒ Ê MS-DOS KERMIT á , ó MS-Kermit> čÜÅ źá äJ ÏÎ .

YÝÏ ÎHW RO ğ~ž MS-DOS RO , iÎ UCâ Øè ąFĺ : 1. b MS-Kermit> čÜ Åź áäJ run [ýõæž MS-DOS ROÎ ÑÆ ] 2. b MS-Kermit> čÜ Åź áäJ push , ð^ MS-DOS čÜÅ ź (C:n>) ď , ÏÎ MS-DOS RO , Má äJ exit , ^ì MS-Kermit> čÜ Åźď .

4.2.2 Terminal Emulation Related Commands

PŒ Ý œ Ò À ň A ş ö ž R O ] A : śî Ã õ , śî ä L , Îś î L í œ ě T j þ , Àz p U . (Ð‘N : HU ROą b MS-Kermit> čÜ Åź áäJ )

1. ïÜ č ÜÅ ź : bÉ ŒÇ e L{ ď , MS-DOS KERMIT Pů ÝD œ KERMIT žčÜ Å ź ąř Kermit> , čö Ï À , źÉ i N MS-DOS KERMIT žč Ü Å ź ï Ü , Òp : ïÜ ř

Local> , HQÏ À . ïÜ čÜ Åź ROp U :

set prompt [čÜÅ źrê ]

Ki N MS-DOS KERMIT čÜÅ źÑ MS-Kermit> ïÜř sč Ürê .

2. ïÜÃ õ C â : ýï ÜÃ õ G Œ , ež (Foreground Color), ÎI ž (Background Color) ž Câ , iÎ UC ROï Ü :

set terminal color [0Î1] [ež Câ ] [IžC â ]

Ä@ ÓÆr íÜ @ë GŒ (H 0 íÜ ) ÎłG Œ (H 1 íÜ ) , ež PI žC âíÐ Ñ\ þ ý E .

3. ]w ŒÝœ ňą : íiJ ŒÝ œÒÀ ňA á , o{ : ÏÎ cls RO Lk MčÃ õ , ÏÎ more RO L k v ű ã Ü ž e , ÎÏ Î vi ěs è n é L k £ T s è É Œ É , şË d Œ Ý œ ň ą O_ £T , Ãń s]w ŒÝ œň ą . ]w ŒÝ œňą žR Op U :

set terminal type [ŒÝ œňą ]

Yč¿ MS-DOS KERMIT äľ žÇ Œ Ý œ ňą , iäJ set terminal type ? , YX {Ò şŒÝ œň ą , Aïú äď @Øä JY i .

4. ]w ^ š (Rollback) űÆ : bŒ Ý œ ÒÀ ň Aď č _ö U PgUp É , Ìhi ^ šÜ e Q űž že . Yžw žQ ű^š \à čÅÏ ÎÉ , iÎ UC RO W[ :

set rollback [^š űÆ ]

íÆ Ø j ó 20 É , ]O Ð é Å ą č ň , ià o Í ]w L Ä ž ą Î , źÉ Ý Q Î set ter-

minal expanded-memory RO Î Expanded Memory Manager (Òp : EMM386 ,

QEMM ě ) žóU , ÐÑ\ KERMIT.HLP ÉŒąú .

5. ]w WøC år žB zèą : YYC år žeW L@ æ , WLąÀ år žB zèą iÎ U CR Oüw :

set terminal wrap [onÎ off]

]w ř on É , íÜN W X ą À å rÁ Î ĺ ř s ž @ æ ; ]w ř off É , hN W Xą À å rø h .

6. ]w äL : ýN Y@ä (ÎÕ Xä ) ]wř Hot Key, iÎ UC RO ]w :

set key [scancodeÈ ] [wqÈ ]

scancode řöUÓ äá , BIOS žłú È . wqÈ iřY @r ÿ (Character), rê (String), KERMIT RO , Keyboard Verb , Îĺ řw q , iÑ \ Using MS-DOS KERMIT @Ñ ď þ

ý I žą ú . ÏÎ źR O w q \à ä á , bŒ Ý œÒ À ň Aď ö U ź ä , qT ð| N w q Èe ÜůÝ Dœ .

Yč ¿Y@ äž scancode Èř ó , çiý äJ :

set key

Má äJý üw ř Hot Key žä , AäJ wq È . H@ Òąú pU :

set key n315 nkdos

äJ WzR Oá , öU F1 ä , Yi¡ţ Èœ Ü MS-DOS ď .

7. ]w L í œ : žw Lí œ ř PRN, YQ NC L š G redirect ÜY @ ÉŒ , iÎ U CR O ] w : set printer [ÉŒ WÙ ]

Ki NCL šG redirect ÜÉ Œď .

4.2.3 File Transfer Related Commands

PÉ ŒÇ eş öžR Op U : (HUR Oą b MS-Kermit> čÜ Åźá äJ )

1. Nţ ň É Œ redirect Üä L device: Nţ ň ž É Œ redirect ÜL í œ Î Ã õ , Óč s J É ŒÉ , iÎ UC ROü w :

set destination [disk Î printer Î screen]

žw Èř disk.

2. xs ĳ Ç e ź ę ž É Œ : bÉ Œ ø Œ j , Çe É ą û ø ž ą Î U , Yď ~ o Í ù ~ , Ýń sÇe É , ià | Ó Oó h É ą . Yà Nw ţ ň ąÀ x s , hi î Ö ńs Ç e ÒÝ ž ê Æ q . iÎUC RO ]w :

set incomplete [discard Î keep]

žw Èř discard , čxs . ]w ř keep É , h[ Hxs .

48 CHAPTER 4. ADVANCED USAGE

Appendix A

Installing MS-DOS KERMIT

ýõ æ MS-DOS KERMIT, šůã şUC ]Æ :

1. IBM PC Ûeqč .

2. MS-DOS Î PC-DOS 2.0 HW ľż .

3. ÜÖ ş 360K ÏÐx sÅą . 4. iÎ OÐé b 220K HW .

5. qT Ëm : MS-DOS KERMIT čÑUC TØ P~ Ésţ žè ą :

¿ âą PC ¡ţs ţ : Nâą PC žÇ Cð (Serial Port) Hql u¡ ţs ţ . ÇCð @ ëř RS-232-C űś d , Ìţ } Æ i À ř 9-pin Î 25-pin âØ , ÌÇ ź i À ř com1 ,

com2, com3 , com4 ě .

¿ ÏÎÆÚ œ (Modem): QÎq Üuô Çe êÆ , iÀ řU CâØ :

{ žm ą (Internal) ÆÚ œ : ¡ţą b PC žX RÑ ď .

{ ~ţ ą (External) ÆÚ œ : Ëm ó PC Pq Üu ôğ ą , řØ e‘ Îž sţ èą .

¿ ÏÎÏì ôô (Local Area Network): gÑÏì ôô Çe êÆ , iÀ ř TCP/IP , NOV-

ELL, ... ě , ş]t Aí žXÊ {ą (Driver Software).

6. ql u (Cable) : iř UC| Øğ @ :

¿ êÀÆÚ u (Null Modem Cable): Îó ¡ţ sţ âą PC žÇC ð .
¿ ÆÚu (Modem Cable) : Îó sţ ÇCð P~ ţą ÆÚœ .
¿ qÜu (Telephone Cable) : sţÆÚ œP ¡@ qÜu ô .
¿ ôôu (Network Cable) : sţÏì ôô dP Ïìô ô .

7. ÏÎ űśd : iř CGA, EGA, Î VGA .... ě .

ãÆ HW wé ]Æá , Ki}l N PC P~És ţ , sţè ąi ÀřU CT Ø :

1. âą PC ¡ţs ţ : iÑUC âØ èąź ĺ :

¿ ÏÎêÀ ÆÚ u (Null Modem Cable) ¡ţ sţâ ą PC žÇCð .
¿ NÄ@ ą PC žÇC ðP Æ Úu s ţ , źÆ Úu ž t@ ÝP ê ÀÆ Ú œà ţź (Null

Modem Adapter) Î Modem Eliminator sţá , AÎÄ Gø Æ Úu sţ Ü ÄG ą PC

žÇCð .

2. ÏÎÆ Ú œ P ~É s ţ , iÀř U C â Ø ąÎ : (Ð‘ N : LINE P PHONE žą Õ W Ù b Uň ÆÚœ Wi àč P ! ) (a) ÏÎžm ąÆ ÚœP ~É sţ , BJ pU :

¿ BJ @ : Nž mą ÆÚœ ąb PC žXR ÑW .
¿ BJ G : ÏÎq Üus ţž mą ÆÚœ ž LINE ąÕP¡ @q Üu ô .
¿ BJ T : ÏÎq Üus ţž mą ÆÚœ ž PHONE ąÕ Pq Üœ .

(b) ÏÎ~ţ ąÆ ÚœP ~É sţ , BJ pU :

¿ BJ @ : ÏÎ ÆÚ usţ PC žÇ CðP ~ţ ąÆ Úœ .
¿ BJ G : ÏÎq Üus ţ~ ţą ÆÚœ ž LINE ąÕP¡ @q Üu ô .
¿ BJ T : ÏÎq Üus ţ~ ţą ÆÚœ ž PHONE ąÕ Pq Üœ .

3. ÏÎ Ïìô ôd P~ Ésţ , BJpU :

¿ BJ@ : NÏì ôôd ąb PC žXR ÑW .
¿ BJG : ÏÎ ôôu sţ Ïìô ôd P~ ÉÏì ôô .
¿ BJT : wË ôôX Ê{ ą .

ÏÎè k@ ÎGP ~É sţ É , šů Oý Òs ţžÇ Cð sź řó , H@ř set port RO ÏÎ žÑ Æ . HØ e PC ‘Î žs ţè ąÓ ě , ÇC ð com1 q‘ PÆ ń (Mouse) sţ , ]ź Æ Úœ q‘ ţó ÇCð com2 .

wé] ÆwË źĺ á , ţUÓ ÝÝ MS-DOS KERMIT né]t žÇ DnÉ Œ :

¿ READ.ME : MS-DOS KERMIT ąúÉ , ]t wË BJÎ UÉ Œšű .

¿ KERMIT.EXE: MS-DOS KERMIT iõæÉ .

¿ þ[ ÉWř .INI Ì : UØ ÒlÉ , Àř MSKERMIT.INI (tÎÒl É ) Î MSCUSTOM.INI

(ÏÎ ÌÛ wÒl É ) ě .

¿ þ[ ÉWř .PCH Ì : PATCH {ą , ]A MSKERMIT.PCH Î MSR313.PCH .
¿ þ[ ÉWř .SCR Ì : Uň ÆÚ œÏ ÎžÛ Êů źÉ , Òp HAYES.SCR ě .

¿ DIALUPS.TXT : dial ĺřÏ Îž OWÎ qÜ ŕê ÆÉ .

¿ þ[ ÉWř .TXT Ì : Uňr ř (Character Set) ÏÎ žrř É .

N MS-DOS KERMIT néw ËÜ PC žBJ pU : (Hw ËÜ C:nKERMIT řÒ )

¿ BJ @ : ÒÊ PC, Ëdw Ð C: ďO_ş 360K HW ži ÎÅ ą (Free Space) .
¿ BJ G : ØSS nKERMIT Øý .
¿ BJ T : N MS-DOS KERMIT ÏùW Òş ÉŒ Copy Ü C:nKERMIT Øý ď .
¿ BJ | : ÏÎ å Ñ s è n é (Òp : vi, emacs, pe2, .... ě ) sè AUTOEXEC.BAT É , b

jM ô | (PATH=) Ôz Ì ¡ Ý [ J C:nKERMIT , HK b ô ó Ø ý U ą i Ò Ê

MS-DOS KERMIT.

Üź zK ź ĺÒ ş wË B J , i} l ÏÎ MS-DOS KERMIT. ÃÐ Ë dU C U ţê Æ , HQ ÏÎ :

1. ÏÎ ÆÚœ su É :

Ëd ţØ êTÓ¡ O_ ř HAYES Ûe ň ÆÚœÏ Îâ U sţ ÆÚœ žÇ Cðs ź @ë com1 ř 9-pin ž D ň¡ ţY (D-

type Male Connector), com2 ř 25-pin

ž D ň¡ ţY (Yz ž PC čř źň , ÐÑ\ ÏÎ âUÎ űś dW žÐÜ ) ÆÚ œtŒ ÆÚœÏ Îâ U

MSKERMIT.INI Î MSCUSTOM.INI

O_ b C:nKERMIT ď iÑ MS-DOS KERMIT Distribution

Disk ďúo MSKERMIT.INI ďO _ w q dial ĺ

řR O

ÏÎ show macro ROd SS

HAYES.SCR Î DIALUPS.TXT O_

b C:nKERMIT ď iÑ MS-DOS KERMIT Distribution

Disk ďúo

2. ÏÎ TCP/IP ôôs uÉ :

Ëd ţØ êTÓ¡ PC ž IP ì} VôôÞ zÌ dSS

Name Server ž IP ì} PW Gateway ž IP ì} PW Domain Name WÙ PW Broadcast dò PW Subnetmask ÆØ PW MSKERMIT.INI Î MSCUSTOM.INI

O_ b C:nKERMIT ď iÑ MS-DOS KERMIT Distribution

Disk ďúo MSCUSTOM.INI ď O _ w q telnet

ĺř RO

ÏÎ show macro ROd SS

Appendix B

Using Modem and TCP/IP LAN to Connect to Remote Host

Yzž PC PÉ Ë mÆ Ú œÎ TCP/IP ôô d , hiæ À ÏÎ ź âØ è ąP ů ÝD œ su . B

Jp U :
  ¿ BJ @ : ž ý N Æ Ú œ Î TCP/IP ôô Ò Ý ž U ţ q T Ñ Æ ] w R O [ J MSCUS-

TOM.INI ÉŒď . ]A UCâ þ :

1. PÆÚœ şö žqT ÑÆ ]w RO :

{ set port { set speed

2. P TCP/IP ôôş öžq TÑ Æ] wRO , ]A :

{ set tcp/ip address { set tcp/ip subnetmask { set tcp/ip broadcast { set tcp/ip primary-nameserver { set tcp/ip gateway { set tcp/ip domain

¿ BJ G : b AUTOEXEC.BAT ÉŒď [J set modem =hayes Ôz . YÏÎž ÆÚ œ čO HAYES Ûe ň , hş b MS-DOS KERMIT žw Ë Ïù ď Mä Û ïş ž .SCR ÉŒ , ÃN ä copy Ü C:nKERMIT Øý ď . Má AN set modem=XXXX (XXXX NíÆ Úœ ň ą ) Ôz[J AUTOEXEC.BAT ÉŒď .

54 APPENDIX B. USING MODEM AND TCP/IP LAN TO CONNECT TO REMOTE HOST

ÑÏÎ ÆÚœ sţ ůÝD œÁ ńÜ ÏÎ TCP/IP ôôsţ É , iÎ UCâ Øè ąźĺ :

1. òż suè ą : (HURO ąb MS-Kermit> čÜÅ źá äJ )

¿ BJ@ : äJ set port tcp/ip RO , äáüú ůÝ Dœ WÙÎ IP ì} . çiý ä J set port tcp/ip , Nq T ð ü w ř TCP/IP ğá , AÏ Î set tcp/ip host üwýs už ůÝD œ IP WÙÎì } .

¿ BJG : äJ connect

Yi PůÝ Dœ su , Þ@ L{ ğÔÓ Tğ ÐÑ\ 2.2.1. ‘ .

2. ÛÊs u è ą : ÈÝ b MS-Kermit> čÜ Å ź á ä J telnet RO , äá üú ů Ý D œ W ÙÎ IP ì} , Yi PůÝ Dœ su , Þ@ L{ ğÔÓ Tğ ÐÑ\ 2.2.2. ‘ .

ÑÏÎ TCP/IP ôôs ţůÝ Dœ Áń ÜÏÎ ÆÚ œsţ É , BJ pU :

¿ BJ @ : b MS-Kermit> čÜ Åź á äJ set port RO , äá ü úP Æ Úœ s ţž Ç C ðs ź (com1, com2 , com3 , com4 ě ).

¿ BJ G : b MS-Kermit> čÜÅ źá äJ set speed RO , äáü úÆ Úœ ÆÚœ tŒ .

¿ BJ T : PůÝ Dœs u . iÏÎ UCâ Øè ąźĺ :

1. òżsu èą :

{ BJ @ : b MS-Kermit> čÜ Åź áä J connect { BJ G : äJ at { BJ T : äJ atdt RO , äá üú qÜ źX .

{ BJ | : b sluice# login: čÜ Åźá äJ terminal (# íÜ 1, 2, 3, ... ěÆr ) { BJ ŋ : b sluice#:Top> čÜ Åźá äJ sessions (# íÜ 1, 2, 3, ... ěÆr ) { BJ ż : b sluice#:Top>Sessions> čÜÅ źá ä J telnet -8 RO , äá üú ů ÝD œWÙ Î IP ì} . (# íÜ 1, 2, 3, ... ěÆr ) YiPů ÝD œsu , Þ@L{ ğÔ ÓT ğÐÑ \ 2.1.1. ‘ .

2. ÛÊsu èą :

{ BJ@ : b MS-Kermit> čÜ Å ź áä J dial RO , äá ü ú Alias Name Îq Üź X (eś ů[ W T Î P).

{ BJ G : b MS-Kermit> čÜÅ źá äJ connect { BJ T : b sluice# login: čÜÅ źáä J terminal (# íÜ 1, 2, 3, ... ěÆr ) { BJ | : b sluice#:Top> čÜ Åźá äJ sessions (# íÜ 1, 2, 3, ... ěÆr ) { BJ ŋ : b sluice#:Top>Sessions> čÜÅ źá ä J telnet -8 RO , äá üú ů ÝD œWÙ Î IP ì} . (# íÜ 1, 2, 3, ... ěÆr ) YiPů ÝD œsu , Þ@L{ ğÔ ÓT ğÐÑ \ 2.1.2. ‘ .

Appendix C

Full-Duplex v.s. Half-Duplex Communication Settings

bją Àą ÎU , MS-DOS KERMIT Pů ÝD œą ąH þù u (Full-Duplex) èą qT . ýb Y ÇąÎ ďi àÝ Hb ùu (Half-Duplex) èą qT , źÉ ůN YÇ ÑÆ Èń s] w , HÅ Xê Ú ÝD .

PqT ÑÆ] wş öžR O] AH UÆØ :

1. set duplex : Îó ü w q T è ą , iÀ ř þ ù u (Full-Duplex) Îb ù u (Half-Duplex)

âØ . q‘ř þù uè ą .

2. set parity : Îóü wP ìè ą (Parity), iÀř NONE, ODD, EVEN, MARK ě . q‘

ř NONE.

3. set flow-control : ÈAÎ ó þù uq T ď , Îó üw y qś îè ą (Flow Control), i

Àř NONE, XON/XOFF, RTS/CTS ě . bb ùuq Tď ]w ř None.

4. set handshake : ÈA Î ób ù u q Tď , Îó ü w Line Turnaround Character , iÀ

ř None, XON, CR, LF ě . bþ ùuq Tď ]wř None.

56 APPENDIX C. FULL-DUPLEX V.S. HALF-DUPLEX COMMUNICATION SETTINGS

HUÎ íCè ąN ‘čž su qT ÑÆ] wą ÎCX :

su ôÒ qTèą Pìèą y q ś î è ą^{Handshake} èą žw su ôÒ FULL NONE XON/XOFF NONE P UNIX Dœs u FULL NONE XON/XOFF NONE P VAX/VMS Dœ s u^{FULL NONE XON/XOFF NONE} P IBM Dœ Hþ Ãõ èą (Fullscreen) su^{FULL EVEN XON/XOFF NONE}

P IBM Dœ Hæ Cè ą (Linemode) su^{HALF MARK NONE XON} PC P PC ąHê ÀÆ Úu (Null Modem Ca-

ble) èą su

HALF NONE XON/XOFF NONE

HÏ ìô ô (LAN) s u^{FULL NONE XON/XOFF NONE} Hł t Æ Ú œ (Ç é t Œ j ó 38400bps) su FULL øąÎÓ w RTS/CTS NONE

Appendix D

Logging Terminal Emulation Process

ÏÎ ŒÝ œ Ò À \ àP ů Ý D œ su É , ià ] ôô u z Z Î ůÝ D œ č £ ‘ś œ , ÉP s è ďžÉ Œø ć . ř¿î ź Øą Îo Í , MS-DOS KERMIT SO čÑ Oý ŒÝ œÒ À L{ ž\ à . OýŒ ÝœÒ ÀL {iÎ UC âØ èąF ĺ :

1. ÏÎ log session P close session RO . Þ@ BJ pU :

¿ BJ@ : ÌÄG źÒz BJ PůÝ Dœ su , Ãn J (login) Þ@ .
¿ BJG : býO ý žŒ Ý œÒ À L{ } lğ e , öU Alt-x Î Ctrl-]-c , ð^ MS-

Kermit> čÜ Åź .

¿ BJT : b MS-Kermit> čÜ Åźá äJ log session
¿ BJ| : b MS-Kermit> čÜ Åź áä J connect , ð^Œ Ýœ ÒÀ ňA , ~òÞ @

. ¿ BJ ŋ : ýO ý ž Œ Ý œ Ò À L { š ô á , öU Alt-x Î Ctrl-]-c , ð^ MS-

Kermit> čÜ Åź .

¿ BJż : b MS-Kermit> čÜÅ źá äJ close session
¿ BJC : b MS-Kermit> čÜ Åź áä J connect , ð^ ŒÝ œÒÀ ňA , ~òÞ @

. 2. ÏÎ È œÒ ąR O (Escape-Level Mode Command) Ctrl-]-f źĺ : öU Ctrl-]-f Èà O ýØ eãÜ ŒÝ œÒ Àeś žž e .

58 APPENDIX D. LOGGING TERMINAL EMULATION PROCESS

ÏÎ log session Î close session RO O ý Œ Ý œ Ò À L { É , žw ž x s É Œ ř

SESSION.LOG . YÝ x s ó ä L É Œ É , ib log session RO á ü w x s É Œ W Ù .

Yä J log session prn , iN ŒÝ œÒÀ L{ ńÉ (Redirect) ÜLí œWL X . Yč QO ý Y@q ŒÝ œÒ À L{ É , iäJ È œÒ ąR O Ctrl-]-q Î Alt-q Èś Oý ; ýì _ Oý É , iäJ ÈœÒ ąR O Ctrl-]-r Î Alt-rńs }lO ý .

ÏÎÈ œÒą RO Ctrl-]-f Oý ŒÝœ ÒÀ L{ É , žwž xs ÉŒ ř KERMIT.SCN . Cÿ öU Ctrl-]-f É , |Hs òè ąO ýe śž e . YtX ÏÎ PgUp Î PgDn ä , Cÿ iO ýÌ ñQ űžŒ Ýœ ÒÀL { .

gÑH WâØ èą , Ki Oý ńnž ŒÝ œÒ ÀL{ , HŒKð M_ už ąÎ .

ýs ýw O ýž Œ Ý œÒ À L{ , ib MS-Kermit> čÜ Å źá ä J replay RO , áś ţ Wx sÉ ŒW Ù (iř SESSION.LOG, KERMIT.SCN, ÎäL Ûæ wq žxs ÉŒ W Ù ), Yi NO ýUÓ žŒ Ýœ ÒÀL {ń sãÜ .

HW â Ø è ą È A Î ó O ý å r ň Œ Ý œ ž Ò À L { . Yn O ý Ï Î Œ Ý œ ž e ś ž e , iä J Ctrl-End , Yi N Ø e Ï Î Œ Ý œ ž e ś ž e O ý ó TEKPLT##.TIF ... ď . (## ř 01, 02, 03 ... ěÆr )

Appendix E

Screen Color Table

set terminal color ROÒ ÏÎ žÃõ Câ ]w ÑÆp Uí ÒC :

Câ ež (Foreground)ÑÆ È Iž (Background)ÑÆÈ Â 30 40 õ 31 41 ñ 32 42 í 33 43 Å 34 44 ţ 35 45 Åñ 36 46 Õ 37 47

60 APPENDIX E. SCREEN COLOR TABLE

Appendix F

Improving Speed and Quality of File Transfer

ÉŒ Çe t Œ O ü ÉŒ b Ç e É , æì É ą ž êÆ ž Ç e q ; Çe ~è O ü É Œ Çe ž £ T v (ia Œ ), źG ţ Ê è ü Ç é ű è (Òp : qÜ u , Ïì ô ô u .... ě ) žv T ě j . MS-DOS

KERMIT čÑ ÆÓ Ñ Æ] w RO , ýÏ Î Ìi HÇ é űè ž SÊ Õã , Húo Ì Aí žt Œ P

~è .

PÉŒ Çe tŒ ş öž ÑÆ ]A Ê] øŒ (Packet Length) Î Sliding Window žjp . Ê] øŒ Vj , ÒÝ Ç e ÿÆ V Ö , tŒi H ğ č ł ; Sliding Window Vj , C@ É ą ži e X ž Ê ]Æ ØV h , ičł Çe tŒ .

Ê] ø Œ À ř e X Ê ] ø Œ Î ţ ň Ê ] ø Œ â Ø , ÀO N í Ç e É Ò à e X Î ţ ň Ê ] øŒ ž Ì j È . eX Î ţ ň â Ý Ò ] w ž Ê ] ø Œ È č @ w n Û P , iÀ O Ï Î set send

packet-length Î set receive packet-length RO Õã . HWâ RO žÏÎ èą pU :

set send packet-length [üw øŒ (H byte řæ ì ) ]

set receive packet-length [üw øŒ (H byte řæì ) ]

Ê]ø Œ ÈÌ Cř 1 byte , Ìł i Ü 9024 bytes , eX Ê] øŒ È žw řÌ j È 9024 bytes , ţň Ê] øŒÈ žw ř 94 bytes . YzÏ Îž Çé űèW e (Bandwidth) dò j , čö üø T zZ , ~è}n (Òp : úÖu , Pbq lu .... ě ) , hiW jÊ ]øŒ È .

WjÊ ]øŒ ÈÉ Ý‘N UC Æţ :

1. êÚ Ç e É Ï Î ž Ê ] ø Œ H e X Î ţ ň â Ý ] w ž Ê ] ø Œ È ď û p Ì ř Ç : eX Ê ]ø Œ Î ţ ň Ê ] ø Œ À O N í e XÎ ţ ň Ê ] ž Ì j È . Ye X Î ţ ň â Ý Ò ] w ž Ê] øŒÈ čP É , hÌU CW hMw êÚ ÇeÉ ÏÎ žÊ ]øŒ :

¿ Y (eX Ý ]w ž e X Ê] ø Œ È ) > (ţňÝ ] w ž ţň Ê ] ø ŒÈ ) , hH ţ ň Ý ž]wÈ řê ÚÇe žÊ ]ø Œ .

¿ Y (eX Ý ]w ž e X Ê] ø Œ È ) < (ţňÝ ] w ž ţň Ê ] ø ŒÈ ) , hH e X Ý ž]wÈ řê ÚÇe žÊ ]ø Œ .

q‘b Ò Ê MS-DOS KERMIT Î C-KERMIT É , eX Ê ] øŒ È | ž w řÌ j È 9024

bytes , ţňÊ ]ø ŒÈ |žw ř 94 bytes , ]źÈ Ý] wţ ňÊ ]ø ŒÈ , Yiï Üê Ú

Çe ÉÏÎ žÊ ]ø Œ .

2. Çé ű è ø T [ j , Î MS-DOS KERMIT iÏ Î ž w Ä Ï (Buffer) îp É , ąi à Ï ø Œj žÊ] čö Çe . ]źY Çe tŒč WÏ řÉ , ş] wû pžÊ ]ø ŒÈ .

3. [j Ê] øŒ Èo oÍ Çe ù~ É , i] wû øž żù (Error-Checking) rÿ øŒ Hï ¡ . iäJ set block-check 2 Î set block-check 3 RON żù rÿø ŒW [Ü 2 Î

3 bytes.

4. bÇ é ű è ø T ě j ž ą Î U , čÈ č ş W [ Ê ] ø Œ È , ÏÓ ş î Ö Ê ] ø Œ È Ü 94

bytes HU .

Sliding Window ÆØi ÏÎ set window ROÕ ã , ÏÎè ąp U :

set window [üw Sliding Window ÆØ ]

Sliding Window ÆØ ÌC ř 1 , Ìł iÜ 31 , žw Èř 1 É , íÜ ÏÎ Stop-And-Wait èą

Çe Ê] . ïÜ Sliding Window ÆØÉ Ý‘ NUC Æţ :

1. ]w ž Sliding Window ÈřÌ jÏ Îŋ Œ , bêÚÇ eÉ , ià ÏÎ ûpž Window ÆØ . 2. PÉ W[Ê ]ø ŒP Sliding Window ÆØ , oo ÍÇ etŒ Uř {H É , şýîp Ê] ø Œ , AřC Sliding Window ÆØ .

3. Sliding Window ž\ àš ůbÇ eÝ Îţň Ýž KERMIT ąčÑ žą ÎU~ iÏ Î .

řF Ñ Ê ] ø Œ È P Sliding Window ÆØ ï É Œ Ç e t Œ ž v T , ÚÌ w ï č P Sliding

Window ÆØ U , ïÜ Ê ] ø Œ ï ó É Œ Ç e t Œ ž v T @ @ ú Õ , úÕ š G Ð Ñ \ ż ď SS Þ

Nø i 94022 . ÚÚ Ó ø iž š G , kÇ X č P Sliding Window ÆØÉ , i] w žÌ j Ê ] ø ŒÈ íC pU :

Sliding Window Æ ÌjÊ ]ø ŒÈ (Bytes) 1 9024 2 4523 4 2257 8 1124 16 557 31 283

PÉŒ Ç e ~ è ş ö ž ÑÆ ] A ż ù (Block-Check) rÿø Œ Î ń e (Retry Number) žÿ Æ . żù rÿ ø Œ W[ , ičł ż ù àO , HT O ê Æ£ T Ê . ńeÿ Æ V h , he ÔÇ e ć Ñ žà OV j . MS-DOS KERMIT žž wż ùøŒ ř 1 byte, ńeÿ Æř 5.

żùr ÿøŒ iÏ Î set block-check RO Õã , ÏÎ èąp U :

set block-check [üwrÿ øŒ (H byte řæì ) ]

żù rÿ ø ŒÌ C ř 1 byte , Ìł ř 3 bytes , žw Èř 1 byte . Yz Ï Îž Ç é űè ö ü øTz Z (Òp : qÜu .... ě ), hşW [ż ù rÿ øŒ , HTO êÆ ž£ T Ê . ýÝ ‘ NU C Æţ :

1. UØ øŒğ żù rÿ ÒÏÎ žż ùèą pU :

¿ 1 byte : single-character checksum
¿ 2 bytes: 2-character checksum
¿ 3 bytes: 3-character 16-bit CRC

2. żù rÿø ŒV j , ÒÝB zÉ ąVø , ÇetŒ VC . ńeÿ ÆiÎ set retry ROÕ ã , ÏÎè ąpU :

set retry [üw ńe ÿÆ ]

źRO Î óü w : íe X Y@ Ê] ć ÑÉ , ńÆe X źÊ ]ž Ì łÿ Æ . bÇ éű èö ü ø Tz Z (Òp : qÜ u .... ě ) É , şčł ńe ÿÆ È , Hč łÉ ŒÇ eĺ\ žœ | , ńe ÿÆ L Ìł ŋî .

HW |Ø R O ÝÌ ê Ú ąÎ ] w , Bĳ źą i à şň ÿ {H . Òp : W[ Ê] ø ŒÈ i Ï É ŒÇ e t Œ W [ ; ýź É ż ù r ÿ ø Œ ç ş W [ , HT O ê Æ ž £ T Ê , Óá Ì S | Ï t Œ ř C . Ñp źþą ÎÆ h , ÝÌê Úą Î@@ vÅ , Hú oÌ ÎÕ X .

b ASPAC pžž ÑÒÒ lÉ USERDEF.INI ď , NH WUţ ÑÆ ]w pU :

¿ eX Ê]ø Œ : 9024 bytes
¿ ţň Ê]ø Œ : 1024 bytes

¿ Sliding Window ÆØ : 1

¿ żù rÿø Œ : 1 byte

ÑÒ Òl É USERDEF.INI žąú ÐÑ \þý I .

Appendix G

Server Functions

b 3.2.2. ‘ď wą úpó N KERMIT čÑž øA ź\à Îó ÉŒ Çe . čF ÉŒ Çe~ , øA ź\ à| şä LÎ~ , Nóżþ ýď Ôz .

KERMIT čÑ ø A ź \ à ž D n Î ~ b ó : Ï@ ą œ ź ĺ ř č Ñ A È ž ň A , ýÏ Î Ì i

Ñů Ýœ źs úøA źW žê¡ . bUľ ż KERMIT {ąž óUU , Dœ Î PC ąiĺ řø A ź , HU NÀz ğ .

G.1 Mainframe Server

ż‘ H ď ą ã s | D œ gate.sinica.edu.tw (HU š Ù ř gate ) @ø A ź ř d Ò , ąú Ï Î D œ @ř øA źž ąÎ . NůÝ Dœ gate ÒÊĺř øA źž BJp U :

¿ BJ @ : ÏÎÆ ÚœÎ TCP/IP Ïì ôô , Ñ\Ä GźÒ zs uè ą , PůÝ Dœ gate s ţ . ¿ BJ G : bů ÝD œ gate žčÜ Åź gate:~> áä J kermit , õæ C-KERMIT (Ys ţ äL Dœ , ià řäL ľż ž KERMIT)

¿ BJ T : b C-KERMIT čÜ Å ź c-kermit> áä J server , Ki Ï ů Ý D œ gate iJ

KERMIT øA źňA .

źĺ Wz B J á , öU Alt-x Î Ctrl-]-c , Yi ð ^ PC , b MS-Kermit> čÜ Å ź U Ï Îů ÝD œ gate čÑ žø AźA È .

žýä J remote help , iòo ůÝ Dœ gate žø Aź AÈu Wš Uą ú (On-Line Help) Tğ pU :

GET files REMOTE CD [dir] REMOTE DIRECTORY files
SEND files REMOTE SPACE [dir] REMOTE HOST command
MAIL files REMOTE DELETE files REMOTE WHO [user]
BYE REMOTE PRINT files REMOTE TYPE files
FINISH REMOTE HELP REMOTE SET parameter value

HW Yř ůÝ Dœ gate ÒčÑž Òş øAź AÈ .

ůÝD œ gate Òč ÑøA źA ÈÔz pU :

1. PÉ ŒÇe şö žR O , ]A get Î send ě , ÐÑ \ 3.2.2. ‘ąú .

2. MAIL RO : ib MS-Kermit> čÜÅ źáä J :

mail [ÉŒW Ù ] [ňHHW Ù @‘ Iì } ]

źR Ožu @y {p U :

ýN É Œ Ç e Ü ů Ý D œ gate , Ñø A ź x s ó u @ Ø ý ď ; Má Ò Ê ů Ý D œ gate Wž mailer {ą , NÓ É Œ H E-mail èą e Ü ü w ‘ I ğ ň H H ; í

mailer {ą wţ ň Ò şÉ Œ á (ýč@ w ź ĺe X E-mail žu @ ), ìý x só

u@Øý ďž ÉŒK QR č .

mail ROi PÉ eX @ÓÎ hÓ ÉŒ , ÈůÏ Î ? Î * ěqÎ rÿ (Wildcard Character)

íÜ . YňH Hç bP ůÝD œ gate W , h‘ Iì} iÙ ď . 3. Ïů ÝDœ gate æœø Aź ňA žRO , ]A :

¿ bye : źR O i Ï ů Ý D œ gate õæ H U T Ó R O : 1. œ} ø A ź ň A , 2. õæ quit RO œ} C-KERMIT , 3. õæ logout RO , œ}ů ÝD œ gate .

¿ finish : źR O È Ï ůÝ D œ gate œ}ø A ź ň A , ýčõ æ quit Î logout R

O , ]ź ů ÝD œ gate ťś d b C-KERMIT ď . b PC Ýž MS-Kermit> čÜ Å ź áäJ connect , ťi iJ ŒÝœ ÒÀ ňA , ~ò PůÝ Dœ gate Oùs u .

G.1. MAINFRAME SERVER 67

4. PÉ ŒÞz şö žR O , ]A :

¿ remote cd : ïÜbů Ýø Aź gate Wžu @Øý (Working Directory) ìm .
¿ remote space : dSS ůÝ øAź gate WØ ež iQÎ Åą (Available Space) jp

.

¿ remote delete : Rčů ÝøA ź gate Wž ÉŒ .
¿ remote print : QÎůÝ øA ź gate žL íœC Ls óů ÝDœ gate žÉŒ .
¿ remote help : dSSů Ýø Aź gate ÒčÑž øA źA È .
¿ remote dir : CX ůÝø Aź gate WY@ Øý žžÒ şÉ ŒêÆ .
¿ remote type : sýůÝ øA ź gate WY @É Œžž e .

5. Pů ÝDœ şö žR O , ]A :

¿ remote who : CX ůÝD œ gate WØ ež ÏÎ Ìňp .
¿ remote host : õæůÝ Dœ gate WžR OÎ {ą .

Òp : äJ remote host finger john iõ æůÝ Dœ Wž finger ¡Î {ą , dSS ÏÎÌ john žêÆ .

¿ remote set : Îó ï Ü ů Ý D œ gate ž C-KERMIT tÎ Ñ Æ ] w È , iä J remote set ? dSSi ïÜ þÇÑ ÆÈ .

Òp : äJ remote set file type binary iN ůÝD œ gate žÉ ŒÇ eæ ąïÜ řG iìæ ą .

HW Yř ů ÝD œ gate @ř KERMIT øAź Ï Îž ą Î . YQ b Y@ D œW õ æø A ź , }ñ ÑL HÏ ÎÉ , Nś {H UÝ D : póN YÇ øA źA È\à úø (Ò : Rč (delete) ÉŒ , óï u@ Øý (cd) .... ě ), HŒK ÏÎ Ì}a zŕ WØSS žê Æ ?

řÑM źÝD , ib ůÝ Dœ gate õæ server ROğ e , ýäJ disable RO , NąÀ ø Aź AÈ \à öň , ¿î ÏÎÌ õæ oÇR O . disable RO žÎk pU :

disable [ÉŒA È\ àWÙ ]

Òp : ýŋ îÏÎ ÌÏ Î remote delete RORč øA źW žŒŒ É , iÌU CB Jõ æ :

¿ BJ @ : ÏÎÆ ÚœÎ TCP/IP Ïì ôô , Ñ\Ä GźÒ zs uè ą , PůÝ Dœ gate s ţ .

¿ BJ G : bůÝ Dœ gate žčÜ Åź gate:~> áäJ kermit , õæ C-KERMIT
¿ BJ T : bů ÝD œ gate ž c-kermit> čÜ Åź áä J disable delete , öň remote

delete RO .

¿ BJ | : bů ÝDœ gate ž c-kermit> čÜÅ źá äJ server , Ï gate iJøA źň A . źÉ ÏÎ ÌK LkÏ Î remote delete ROR čsb øA źWž ŒŒ .

ýdSS iöň þÇ \à , ib ůÝD œ gate ž c-kermit> čÜ Åź áäJ disable ? , úo uW šU ąú Tğ (On-Line Help) pU :

all directory get set
delete type send
host bye who
space finish cd

Yä J disable all , hi öňÒ şA È\ à .

ýńs }ñY @ý eQö ňž \à É , iä J enable RO}Ò . enable ROžÎ kp U : enable [ÉŒA È\à WÙ ]

çi ÏÎ enable ? , Hú op disable ROÒ Cž uWš Uą úTğ (On-Line Help) .

G.2 PC Server

@ë PC bÒÊ MS-DOS KERMIT ğá , çi äJ server RO , čÑ øA ź AÈ . ż‘ N ą úp óN PC ÒÊĺ řø Aź , Î PC øAźč Ñž AÈ .

N PC ÒÊĺ řø Aź žBJ pU :

¿ BJ @ : b MS-Kermit> čÜÅ źáä J set port com2Î set speed 19200 RO ] wq T ð s ź Î Æ Ú œ t Œ . (YÏ Î č P ž q T ð s ź ÎÆ Ú œ t Œ É , ÐH ê Ú È @ řÑ Æ )

¿ BJ G : b MS-Kermit> čÜÅ źá äJ connect , iJ ŒÝ œÒÀ ňA .
¿ BJ T : bŒ Ýœ Ò Àe śď ä J ats0 =1 (Ær 0 , Dr À O ) , ÏÆ Ú œi Jţ ě Ò

ą (Answering Mode) , źÉÆ ÚœW ž AA , OH Î CD üÜO| G_ .

¿ BJ | : öU Alt-x Î Ctrl-]-c , ð^ MS-Kermit> čÜ Åź U .
¿ BJ ŋ : b MS-Kermit> čÜÅź áä J server .

źĺ Wz BJ á , eśW |X{ UC Tğ :

     MS-DOS Kermit : 3.13 8 July 1993 patch level 21
       Server mode : type Ctrl-c to exit
         File name :
         File type :
      Current path : C:\KERMIT\
KBytes transferred :

 Number of packets :
     Packet length :
 Number of retries : 0
        Last error :
      Last message :

íÜ w PC wiJø Aź ňA .

wÒÊ PC øAź á , np óN äL PC Üĺ Client (Îá ) , HzL ÆÚ œs ú PC øA ź čÑ žA ÈO ? N PC ÒÊĺ ř Client žBJp U :

¿ BJ @ : b MS-Kermit> čÜÅ źáä J set port com2Î set speed 19200 RO ] wq T ð s ź Î Æ Ú œ t Œ . Ð‘ N : Client PC žÆ Ú œ t Œ P PC øA ź š ů ] w ř ÛP È .

¿ BJ G : b MS-Kermit> čÜÅ źá äJ connect , iJ ŒÝ œÒÀ ňA .
¿ BJ T : bŒ ÝœÒ Àe śďä J atdt 7654321 , Hsţ PC øAź . (atdt ROá ř

øA źžq Üź X )

¿ BJ | : źÉ i ě ì @ s ê ů ź n Î ţ q n , Ý CONNECT Tğ X { á , öU Alt-x Î

Ctrl-]-c , ð^ MS-Kermit> čÜ Åź .

źĺ Wz BJ á , Kĺř ůÝ PC øA źž Client , ib MS-Kermit> čÜ Åź UÏ ÎůÝ PC čÑ žø Aź AÈ .

žýä J remote help , iò o ů Ý PC øAź ž u W š U ą ú (On-Line Help) Tğ p U :

GET filespec REMOTE DIRECTORY filespec REMOTE PRINT filespec
SEND filespec REMOTE HELP this text REMOTE SET command
BYE,FINISH,REMOTE LOGOUT REMOTE HOST command REMOTE SPACE drive-letter
REMOTE CD/CWD directory REMOTE LOGIN name password REMOTE TYPE filespec
REMOTE DELETE filespec REMOTE MESSAGE 1-line msg REMOTE WHO

HW Yř ůÝ PC øAź ÒčÑ žA È .

ÚÌi o { : ůÝ PC øAź Òč Ñ žA Èj ą ÀP W@ ‘ ďÑ ůÝ D œ gate øAź Ò č Ñž AÈ ÛP , ]ź ÈN âÌč Pğ BÔz pU :

1. finish , bye , Î remote logout TÌ ąiś îs úůÝ PC øAźÒ čÑ žA È , ý

tO pU :

¿ finish : źROi Ïů Ý PC øAźœ }ø Aźň A , ^ì MS-Kermit> čÜÅ źU ,

ýčÁ_ Client PC P PC øAź ąwţ qž qÜ uô , ]źÆ ÚœW ž AA , OH Î CD üÜ O ť M G Û . un ů Ý PC Aÿ ä J server RO , Yi A ÿ ^ ì PC øAźň A .

¿ bye : źR O i Ï ů Ý PC øA ź õ æ H U T Ó R O : 1. œ} ø A ź ň A , 2. õæ

quit RO œ} MS-DOS KERMIT , ð^ MS-DOS ď , 3. Á_ Client PC P PC øA

źąwţ qž qÜu ô , ]źÆ Úœ Wž OH Î CD üÜO |ű À .

¿ remote logout : P bye RO ž@ ÎÛP .

2. remote message : iN @æ Tğe Üů Ý PC øA ź , ãÜ óøA źÝ ž Last Message:

ğá .

3. remote who : @ë PC ÈÑ@H ÏÎ , ]ź bä Jź ROá io

Message: Just this server žTğ .

bê ÚÞ @É i o{ : Òş Tğ ą HÉ ŒÇ e èą Ñ PC øAź e Ü Client PC , ]ź b ä J remote dir , remote type ěRO É , b PC øA źÝ |X {P ÉŒ ÇeÉ ÛP že ś , b Last Message: ğá ç|X { remote name is CON žTğ .

PC øAź çčÑ disable Î enable RO , Höň Îń s}Ò YÇ AÈ \à , äÎ kP e @‘ Òz ÛP .

Üźz wï PC øAź ž\à ş@ šæ {Ñ . bêÚÏ Îá ià |čÍ HU ÃÝ : Y PC ø Aźž q Üź X ř \h H Ò¿ , pó ¿ îĳ g Âv ž Ï ÎÌ s ú PC øAź W ž AÈ O ? źI iÑ set server login Î remote login âRO źĺ , ÐÑ \U@ ‘ą ú .

G.3 Secure PC Server

MS-DOS KERMIT řÏ PC øAź ã ş ¿ î D ks ú ž à O , čÏ Î disable RO öň Y Ç

AÈ \à ~ , |iÏ Î set server login RO jœ ĳgÂ vž ÏÎ ÌiJ PC øA ź .

b PC øAź ÝÏ Î set server login RO žB JpU :

¿ BJ @ : b MS-Kermit> čÜÅ źáä J set port com2Î set speed 19200 RO ] wq T ð s ź Î Æ Ú œ t Œ . (YÏ Î č P ž q T ð s ź ÎÆ Ú œ t Œ É , ÐH ê Ú È @ řÑ Æ )

¿ BJ G : b MS-Kermit> čÜÅ źá äJ connect , iJ ŒÝ œÒÀ ňA .
¿ BJ T : bŒ Ýœ Ò Àe śď ä J ats0 =1 (Ær 0 , Dr À O ) , ÏÆ Ú œi Jţ ě Ò

ą (Answering Mode) , źÉÆ ÚœW ž AA , OH Î CD üÜO| G_ .

¿ BJ | : öU Alt-x Î Ctrl-]-c , ð^ MS-Kermit> čÜ Åź U .
¿ BJ ŋ : b MS-Kermit> čÜ Å ź á ä J set server login bar foo (set server

login RO žÄ @ÓÑ Æř username , ÄG ÓÑÆ ř password )

¿ BJ ż : b MS-Kermit> čÜÅź áä J server .

źĺ Wz BJ á , PC øAź Kij œĳ gÂ vžÏ ÎÌ iJ .

wÒÊ PC øAź á , ANt @ą PC ÌUC BJ ÒÊĺ ř Client PC :

¿ BJ @ : b MS-Kermit> čÜÅ źáä J set port com2Î set speed 19200 RO ] wq T ð s ź Î Æ Ú œ t Œ . Ð‘ N : Client PC žÆ Ú œ t Œ P PC øA ź š ů ] w ř ÛP È .

¿ BJ G : b MS-Kermit> čÜÅ źá äJ connect , iJ ŒÝ œÒÀ ňA .
¿ BJ T : bŒ ÝœÒ Àe śďä J atdt 7654321 , Hsţ PC øAź . (atdt ROá ř

øA źžq Üź X )

¿ BJ | : źÉ i ě ì @ s ê ů ź n Î ţ q n , Ý CONNECT Tğ X { á , öU Alt-x Î

Ctrl-]-c , ð^ MS-Kermit> čÜ Åź .

G.3. SECURE PC SERVER 73

źĺW zBJ á , ib MS-Kermit> čÜ Åź áä J remote help , ýźÉ oX {

Error: REMOTE LOGIN required Tğ , íÜš ůý ÏÎ remote login ROéJ username Î password á , ~isú PC øAź Òč Ñž AÈ . remote login RO žæą pU :

remote login username password

w¿ PC øA ź ž username ř foo , password ř bar , ]ź b MS-Kermit> čÜ Å ź á ä J

remote login foo bar , KX { MS-Kermit Server Ready žTğ , íÜ w ĺ \ i J PC ø

Aź . źÉ A ä J remote help , Ki ò o ů Ý PC øA źž u W š Uą ú (On-Line Help) Tğ pU :

GET filespec REMOTE DIRECTORY filespec REMOTE PRINT filespec
SEND filespec REMOTE HELP this text REMOTE SET command
BYE,FINISH,REMOTE LOGOUT REMOTE HOST command REMOTE SPACE drive-letter
REMOTE CD/CWD directory REMOTE LOGIN name password REMOTE TYPE filespec
REMOTE DELETE filespec REMOTE MESSAGE 1-line msg REMOTE WHO

Üź Ki ÏÎ PC øAź ÒčÑ žU ţA È , URO žąú ÐÑ \e @‘ .

b PC øA źď Èà] w@ Õ username Î password . Y] whÕ username Î password É , |HÌ á]w ž@ ÕÈ řÇ .

b PC øAź ď iN set server login RO P disable ROX Î , HP É Fĺ Lo Ï Î ÌÎ ŋî sú Ê@ž Øž .

74 APPENDIX G. SERVER FUNCTIONS

Appendix H

Chinese Environment Settings

í MS-DOS KERMIT bď åô Òď ÏÎÉ , Ý[J @Ç ÑÆ ]wR O , Hã ÜÎ Çeď åÉ Œ . iN H UX { ž R O [J MSKERMIT.INI (tÎÒ l É ) ď , Ki b Ò Ê MS-DOS KERMIT ÉÛ Êź ĺ] wÑÆ u@ , ãş äľ ďåô Òž àO .

žýÝ ‘N : CÓď år Hâ Ó 8 bits žì ÿÕ (byte) Ní , ]ź ÝN Pì èą (Parity) ï ĺ NONE, ~ňH eÇ 8 bits žê Æ , äJ set parity none Yiź ĺ] w .

řF Ï Œ Ý œ Ò À \ à ã ş ã Ü ď å r ž à O , ÝN Œ Ý œ Ã õ ã Ü Ò Ï Î ž ì ÿ Õ ø Œ Ñž w ž 7 bits ïř 8 bits , äJ set terminal display 8 Yi ź ĺ ] w . tÝ N Œ Ý œ ÏÎ ž r ř (Character Set) ]w ř č Ï Î ô ór ř , iä J set terminal character-set

transparent źĺ]w .

ţUÓ ÝB zďå ÉŒ Çe ÝD . @ëÏ ÎåÆ r (text) æąÇ eÉŒ É , ţň Ý| ñû Ç eÝ Ò Ï Î ž r ř (Character Set) O_ Û P , Y_ , hi æ r ř à ń ž u @ . ]ď å | č Ý ó ôór ř , Gi N ź \à ö ň , äJ set transfer character-set transparent Ki ö ň rř àń \à . źĺź ţ] wá , Ki ÏÎå Ær æą Çeď åÉ Œ .

76 APPENDIX H. CHINESE ENVIRONMENT SETTINGS

Appendix I

MSKERMIT.INI, MSCUSTOM.INI, and USERDEF.INI

żþ ý N ą ú Ð Ç t Î Ò l É (MSKERMIT.INI) ÎÏ Î Ì Û w Ò l É (MSCUSTOM.INI) ž že , Ãű Ð ASPAC pžč Ñž ÑÒÒ lÉ (USERDEF.INI). Ææ zb\ łż þýá , àÌ Ú ÒB žô ÒS Ê , ÛæŒ ïUÒ lÉ žže , Ï MS-DOS KERMIT óÅX zžÝ D .

MSKERMIT.INI ÐÇ t Î Ò l É ř ô Û ñ È j Ç Ò s @ , bÒ Ê MS-DOS KERMIT áÑ KERMIT.EXE łJ õ æ . MSKERMIT.INI ďw q j ą À t Î Ñ Æ È Î ‘ Î ĺ ř R O , äž e

|H MS-DOS KERMIT sľż žÀX Óó s , ]ź MS-DOS KERMIT Xľ ÌÆ æzĺ qč Œ ïź ÉŒ , HK sľ żÀ XÉ àSS Yó ń . ýz @w şÓ ÃÝ : Y MSKERMIT.INI žž eč i Œï , žòÛæ wq žt ÎÑÆ ÈÎ ĺřR Oş bó Bwq ? łŒ Nb MSCUSTOM.INI ď .

MSCUSTOM.INI řÏ ÎÌÛ wÒ lÉ , b MSKERMIT.INI õæ źę ÉQł Jõ æ . MSCUS- TOM.INI Oý Ï ÎÌ Û æw q ž tÎ Ñ ÆÈ Î ĺř R O , zi b äď Œ ï MSKERMIT.INI w

qž tÎ ÑÆ È , çi [Js žĺ řRO , äže čH MS-DOS KERMIT sľż ÀXÓ Qï Ü , ]źz iñSS aN ÒÝ \à[ Jź ÉŒď .

USERDEF.INI ř ASPAC pž Ò čÑ ž Ñ Ò Ò lÉ , źÉ Œ ď ï U tÎ Ñ Æ È ž wq ą H

żå UÛ öź ‘žž eř Ç , i@ř zÛæ Œï MSCUSTOM.INI ÉžÑ Ò .

HUN ÀOą úW zTÓ Òl Éž že .

I.1 MSKERMIT.INI

MSKERMIT.INI řÐ Ç t Î Ò l ÉŒ , |b Ò Ê MS-DOS KERMIT áÑ KERMIT.EXE łJ

õæ , źÉŒ ď w q j ą À t Î ÑÆ È Î ‘ Î ĺ ř R O . Ð‘ N : żÒ l É È A Î ó 3.11 ľğ áž MS-DOS KERMIT {ąď .

MSKERMIT.INI ÐÇ t Î Ò l É í C p U . řK ó ą ú _ č , Äú É Œ P ą ú æ ù è ą i æ . Ä@ą À :

; FILE MSKERMIT.INI
;
; Standard initialization file for MS-DOS Kermit 3.11 or later. Kermit should
; execute the commands in this file automatically when it starts. Kermit
; looks for MSKERMIT.INI first in the current disk and directory, and if it is
; not found there, then in the disks and directories listed in your DOS PATH
; variable (if any). You can override Kermit’s initialization file search by
; specifying a different filename on the command line, preceded by the -F
; switch, for example "kermit -f monday.ini" or "kermit -f nul".
;
; Author: Christine M. Gianone, February 1990 (for MS-DOS Kermit version 3.0)
; Revised for version 3.11 September 1991.
; Revised for version 3.12 September 1992.
; Revised for version 3.13 June 1993 (corrected August & September 1993)

źą Àï MSKERMIT.INI ÐÇt ÎÒl É@ @š ű , źÉ Œ| bÒÊ MS-DOS KERMIT áÑ

KERMIT.EXE łJ õ æ . źÉ Œ ş m ó C:n>KERMIT ØýU . ÏÎ Ìi Û æ ű gä L Ò l É

Hú Nż É Œ , ÈÝ b ÒÊ MS-DOS KERMIT Éä J kermit -F [äL Ò l É ŒW Ù ] Yi . YÉ ŒW Ùř nul, hčõæ ôó tÎ ÒlÉ .

ÄGą À :

; CUSTOMIZATIONS
;
; It is recommended that you not modify this file. Instead, you should adapt
; the sample MSCUSTOM.INI file to make your customizations: key settings,
; macro definitions, SET commands to override the ones in this file, and so
; on. The MSCUSTOM.INI file should go in the same directory as this file.
; This file will execute MSCUSTOM.INI if it can be found.

źą À ą ú MSCUSTOM.INI ÏÎ Ì Û w Ò l É ž Î ~ . MS-DOS KERMIT Xľ Ì Ø ş Ï Î ÌÉ q č ó ï MSKERMIT.INI ÉŒ ž ž e , ÓN w ï č P Ï Î ô Ò Ò [ J ž S í ] w R O mó ź É Œ ď . í MS-DOS KERMIT QÒ Ê É , |ý õ æ MSKERMIT.INI ÉŒ ž ž e , M áA õ æ MSCUSTOM.INI ÉŒ , Ki N U t Î Ñ Æ È Ñ ž w È ï Ü ř Ï Î Ì ž S í ] w È .

MSCUSTOM.INI şP MSKERMIT.INI móP @Ø ýď .

ÄTą À :

; COMPATIBILITY
;
; This initialization file works for versions 3.11 and later of MS-DOS Kermit.
; The IF INPATH command is new to version 3.12; it tests whether a given file
; can be found in your DOS PATH or your current directory. The IF INPATH
; command is not used if your MS-DOS Kermit version is earlier than 3.12.

źą Àą ú MSKERMIT.INI ÈAÎó 3.11 ľğ áž MS-DOS KERMIT ď , Ãąú sWR O if

inpath ž\à Îä AÎľ ż (ÈAÎó 3.12 ľğá ž MS-DOS KERMIT {ąď ).

Ä|ą À :

; PATCHES
;
; The MSKERMIT.PCH file contains "patches" (corrections) to MS-DOS Kermit.
; If the MSKERMIT.PCH file can be found, and it agrees with your Kermit
; version, the patches are applied at this time. The MSKERMIT.PCH file
; is included on your MS-DOS Kermit distribution diskette. Updated patch
; files can be obtained from Columbia University.
;
if > \v(version) 312 if inpath MSR\v(version).PCH goto patch
if > \v(version) 311 if not inpath MSKERMIT.PCH goto begin

:PATCH
echo Installing patches...
echo
patch

:BEGIN
echo MS-DOS Kermit 3.11 / 3.12 / 3.13 initialization file...

patch {ąÎ óï MS-DOS KERMIT @ run-time correction . 3.13 ľž MS-DOS KERMIT ÏÎ MSR313.PCH @ř patch {ą ; Yř 3.12 ľ , hÏ Î MSKERMIT.PCH .

Äŋą À :

COMMENT - Variable definitions...

; Reserved variables. If you define new macros, don’t use these names:
;
; _editor - DOS command that runs my preferred editor, for EDIT macro.
; _editfile - Last EDIT command filename, defined by EDIT macro.
; _dialfile - Pathname of dialing directory file, for DIAL macro.
; _dialnum - Last DIAL command phone number, defined by DIAL macro.
; _modem - Modem type for DIAL command. Used to run the appropriate
; dialing script, e.g. HAYES.SCR.
;
; You can override the default _editor, _dialfile, and _modem definitions
; by setting environment variables in your AUTOEXEC.BAT file, for example:
;
; SET EDITOR=EDIT
; SET MODEM=MICROCOM
; SET DIALFILE=C:\PHONES\DIALING.DIR
;
; or you can redefine these variables in your MSCUSTOM.INI file.

; Editor...
;
define _editor edlin ; EDLIN is the default editor.
if not eq "\$(EDITOR)" "" -
  define _editor \$(EDITOR)

; Dialing directory file...
;
define _dialfile C:\KERMIT\DIALUPS.TXT ; Default dialing directory file.
if not eq "\$(DIALFILE)" "" -
  define _dialfile \$(DIALFILE)
if > \v(version) 311 if not inpath \m(_dialfile) -
  echo Dialing directory \m(_dialfile) not found.

; The type of modem you have. You also need a corresponding <name>.SCR
; file to dial the modem. For example, if the value of _modem is HAYES,
; you must have a HAYES.SCR file stored somewhere in your DOS PATH or in
; your current directory.
;
define _modem HAYES ; Default is modem type is HAYES.
if not eq "\$(MODEM)" "" -

  define _modem \$(MODEM)
if > \v(version) 311 if not inpath \m(_modem).SCR -
  echo WARNING: Dialing script file \m(_modem).SCR not found!

źą À ą ú MS-DOS KERMIT ÒÏ Î ž ž w Ü Æ , ]A : editor, editfile, dialfile, dialnum, Î

modem ě , äNíN qp WÒ z . äď editor, modem, Î dialfile ěžwÜ ÆÈ ÀO ]wř :

¿ editor = edlin (Line Editor)
¿ modem = hayes (HAYES Ûeň ÆÚ œ )
¿ dialfile = C:nKERMITnDIALUPS.TXT (qÜŕ ÉŒ )

Yz Ï Î ž s è ź , ÆÚ œ ň ą , Îq Ü ŕ É Œ č ř W C È É , ib AUTOEXEC.BAT ÉŒ ď ÀO [J UC Ôz :

¿ set editor = [sè néW Ù ]
¿ set modem = [ÆÚœ ňą ]
¿ set dialfile = [qÜŕ ÉŒ WÙ ]

Yió ï žw Ü Æ È . Ð‘N : ïÜ modem žw Ü Æ É , Ùš ů ‘ NÛ ï şž .SCR ÉŒ O _ sb .

Äżą À :

COMMENT - Macro definitions section...

; Macros for communicating with UNIX, VAX/VMS, and similar systems:
;
def 8bit set parity none, set term bytesize 8, set term controls 8
def 7bit set term bytesize 7, set term controls 7

def vax set par non, set flo x, set hand no, set dupl ful, set key \270 \127

def vms do vax, do 8bit ; Assumes 8-bit no-parity connection.
def unix do vax, do 7bit ; Most UNIX systems are still 7-bit.

; Macro for communicating with IBM mainframes in linemode:
;
def ibm set par mark, set flo no, set hand xon, set dup ha, set key \270 \8

; Macro for communicating with IBM mainframes in fullscreen mode,
; through 3270 protocol converter like IBM 7171:
;
def fullscreen set par ev,set flo x,set hand no,set dupl ful,set key \270 \8

źąÀ w qP UNIX , VAX/VMS, IBM (]t æ CÒ ą Pþ Ã õÒ ą ) ěD œ su É ÒÏ Î ž qT ÑÆ ÎŒ ÝœÑ ÆÈ . qTÑ Æ] A :

1. Pì èą (Parity) 2. yq śîè ą (Flow-Control)

3. Handshake èą

4. æu Îùu (Duplex)

ŒÝ œÑ Æ] A :

1. ŒÝ œãÜ rÿ Õø Œ (Terminal Bytesize) 2. ŒÝ œśî rÿ Õø Œ (Terminal Controls)

PÉ wq ąÀ Hot Key žN q .

ÄCą À :

; Macro to use Internet host names with Novell’s LWP/DOS TELAPI and TSU.
; Assumes TSU is in the PATH and current directory is writable.
; Usage: "telapi <host-name>".
;
def telapi run tsu -o \%1 k1,run tsu -a k1 1,set port bios1,connect

źą Àw qÏ Î NOVELL ôôPů ÝD œsu ÉÒ ÏÎ žĺř RO telapi.

ÄKą À :

; Additional DOS commands available directly from the MS-Kermit> prompt.

; DOS MORE command... (no "<" needed)
def more if < argc 2 fatal {More what?},-
run more < \%1

; DOS REN(ame) command...
def rename if < argc 2 fatal {Rename what?},-
  if < argc 3 fatal {Rename \%1 to what?},-
  run ren \%1 \%2

; DOS COPY command...
def copy if < argc 2 fatal {Copy what?},-
  if < argc 3 fatal {Copy \%1 to what?},-
  run copy \%1 \%2

; DOS CHCP command to examine or change code page...
def chcp run chcp \%1

; EDIT command...
def edit if = argc 2 assign _editfile \%1,-
  if not def _editfile fatal {Edit what?},-
  run \m(_editor) \m(_editfile)

źąÀ H ĺř R Ow q ‘Î ž MS-DOS RO , ]A : more , rename , copy , chcp , edit ě .

ÄEą À :

; CAPTURE command - Easy downloading of a file from the host, with no error
; checking. Unlike the LOG SESSION command, CAPTURE always creates a new
; file. It overwrites file of same name if it already exists. Usage: at the
; MS-Kermit> prompt, type "capture xxx" where xxx is the name of the file you
; want to create on the PC. Once you are connected to the host, TYPE the
; desired file. Escape back when done. The captured file will be on your
; disk (with a TYPE command at the beginning & a prompt at the end).
;
def capture if = \v(argc) 1 fatal {Capture into what file?},-
  if exist \%1 del \%1,-
  log session \%1,-
  connect,close session,log sess session.log,close sess

źą Àw q capture ĺř RO , źRO QÎ log session NÃ õWX {ž Òş žeO ýU Ó , FìP ÉŒÇ eÛ P\ à . Îk pU :

¿ BJ @ : ÏÎ ÄG źÒ zèą Pů ÝDœ su .
¿ BJ G : öU Alt-x Î Ctrl-]-c , ^ì MS-DOS KERMIT ď .
¿ BJ T : b MS-Kermit> čÜÅ źá äJ capture [OýÉ ŒWÙ ] .
¿ BJ | : b MS-Kermit> čÜÅź áä J connect , ńss ţů ÝDœ .
¿ BJ ŋ : bů ÝD œč Ü Åź áä J cat [ÉŒ WÙ ] , sý ÉŒ ž e (Yz sţ ž ůÝ D

œč ř UNIX tÎ , ÐäJ äLR O )

źÉÓ ÉŒ že Kw s óÉ Œď . ýů‘ NU CT I : @ . capture ĺřR OÈ àÎ ó Oý å Ær (text) æąž ÉŒ , G . Oý ÉŒž Ä@ æř cat RO , T . Lżù àO .

ÄQą À :

; NORMAL, NOISY and CLEAN macros, modify to suit your environment...
def normal set rec pac 94, set ret 5, set block 1, set window 1
def noisy set rec pac 40, set ret 20, set block 3, set window 8
def clean set rec pac 1000, set ret 4, set block 2, set window 2

źąÀ H ĺř è ąw q Ç éu ô b£ ‘ (normal) , şøT (noisy) , ÎLø T (clean) ąÎ ď Ò ÏÎ žÊ ]ø Œ (Packet Length) , ńe ÿÆ (Retry Number) , żùr ÿø Œ (Error-Checking) , Î Sliding Window ěÑÆ È . ÀO pU :

1. £‘ ąÎU : Ê]ø Œ = 94 Bytes, ńeÿÆ = 5, żùr ÿø Œ = 1 Bytes, Sliding Window = 1 2. şø T ą Î U : Ê] ø Œ = 40 Bytes, ńe ÿ Æ = 20, żù r ÿ ø Œ = 3 Bytes, Sliding

Window = 8

3. Lø T ą Î U : Ê] ø Œ = 1000 Bytes, ńe ÿ Æ = 4, żù r ÿ ø Œ = 2 Bytes, Sliding

Window = 2

ÄQ@ ąÀ :

; Define a FATAL error macro. Print message, go back to prompt.
def fatal echo \%1, stop

; ERRSTP macro, for use in scripts that want to hang up a dialed
; or network connection if there is any error.
def errstp echo \%1,hangup,stop

źą À H fatal Î errstp ĺř w q o Í ù ~ É ž B z è ą . fatal ĺř R O b L X ù ~ T ğ á , SSY ð ^ MS-Kermitgt čÜ Å ź U ; errstp ĺř R O b L X ù ~ T ğ á , |õ æ Á _ s u ž u @ , Að ^ MS-Kermitgt čÜ ÅźU .

ÄQG ąÀ :

; LOOKUP macro for use with DIAL command.
; Requires MS-DOS Kermit 3.11 or later.
; Uses \m(_dialfile) for the dialing directory filename, defined above.
; Edit that file to contain the entries you will actually want to use.
;
if < version 311 goto nolook
def split assign \%x \%1,-
  assign \%y \%2,-
  assign \%s \%3,-
  assign \%p \%4

def lookup if < \v(argc) 2 end 0,-
  if not def _dialfile end 0,-
  if not exist \m(_dialfile) end 0,-
  open read \m(_dialfile),-
  if failure fatal {Can’t open dialing directory file \m(_dialfile)},-
  assign \%5 \%x, assi \%6 \%y, assi \%7 \%s, assi \%8 \%p,-
  echo Looking up "\%1",-
:loop,-
  read \%9,-
  if fail goto eof,-
  split \%9,-
  if def \%x if not equal {\%x} {\%1} goto loop,-
  echo From dialing directory: \%x = \%y,-
  assign _dialnum \%y,-
  if def \%s if not eq \%s = set speed \%s,-
  if def \%p if not eq \%p = set parity \%p,-
  goto done,-
:eof,-
  echo "\%1" not found in dialing directory \m(_dialfile),-
:done,-
  assign \%x \%5, assi \%y \%6, assi \%s \%7, assi \%p \%8,-
  close read

; LIST macro to list dialing directory.
; Assumes pathname of dialing directory is in \m(_dialfile).
define list -
  if not def _dialfile fatal {_DIALFILE not defined},-
  if not exist \m(_dialfile) -
    fatal {Can’t find dialing directory file \m(_dialfile)},-
  if < argc 2 run more < \m(_dialfile),-

  if > argc 1 run find "\%1" \m(_dialfile) | more

; DIAL and REDIAL commands...
;
; Requires the file \m(_modem).SCR to be on current disk or in DOS PATH,
; e.g., HAYES.SCR. Uses LOOKUP macro to access your dialing directory, if any.
; If argument omitted, uses previous phone number, if any.
; If multiple arguments are given, they are concatenated together
; with the separating spaces preserved, so you can "dial 800 765 4321".
;
def dial if < \v(argc) 2 if not def _dialnum fatal {Dial what?},-
  if > \v(argc) 2 assign \%1 \%1 \%2 \%3 \%4 \%5 \%6 \%7 \%8 \%9,-
  if > \v(argc) 1 assign _dialnum \%1,-
  if not < \v(argc) 2 lookup {\m(_dialnum)},-
  assign \%1 \m(_dialnum),-
  take \m(_modem).scr,-
  if fail end 1, end 0

define redial if not def _dialnum fatal {No number to redial}, dial

goto common ; Skip over old-version warning

:NOLOOK
version
echo WARNING: This Kermit initialization file is for use with MS-DOS Kermit
echo version 3.11 or later. The LOOKUP macro will not be defined, and DIAL
echo will not work. Use an earlier version of MSKERMIT.INI or a later
echo version of MS-DOS Kermit.
define lookup echo The LOOKUP macro is not defined, stop
define dial echo The DIAL macro is not defined, stop

źą Àw q dial Î list âĺř RO . dial RO IsP ÆÚ œň ąÛï şž .SCR ÉŒ iæ Û Êů źž u@ , list RO iCX DIALUPS.TXT ÉŒď wqž Òş êÆ .

ÄQT ąÀ :

:COMMON

COMMENT - File transfer settings

set file collision rename ; Don’t overwrite existing files
set transfer character-set transparent ; For compatibility with old versions
set receive packet-length 94 ; Regular-size packets
set attributes on ; Use file-attribute packets
set window 1 ; Don’t use sliding windows

COMMENT - Script defaults

set input timeout proceed ; Allow IF SUCCESS/FAILURE to work
set input echo on ; Display port input on screen
set input case ignore ; Ignore alphabet case for input matching

źą Àw qÉ ŒÇe Î Script Programming žÛ öÑÆ È . ÉŒÇe žÑ ÆÈ ]A :

¿ PW ÉŒž Bz èą (File Collision) : ńs RW (Rename)
¿ ÉŒ ÇeÏ Îž àń rř (Transfer Character-Set) : čÏÎô ór ř (Transparent)
¿ ţň Ýžţ ňÊ ]ø Œ (Receive Packet-Length) : 94 Bytes
¿ ÉŒ ÝÊy zÊ ] (Packet Attributes) : }Ò (On)

¿ Sliding Window ÆØ : 1

Script Programming žÑ ÆÈ] A :

¿ ěÔ é J É ą W L ] w È ž B z è ą (Input Timeout) : õÜ U @ Ó R O ~ ò õ æ (Pro-

ceed)

¿ éJ TğO _^ şÜ ÃõW (Input Echo) : O (On)
¿ éJ ROj pg Bz èą (Input Case) : Nj pg øř ÛP (Ignore)

ÄQ| ąÀ :

; The following setups are IBM-PC specific...

if not eq "\v(platform)" "IBM-PC" goto fin

COMMENT - Terminal emulation settings. Modify to suit your environment.

set terminal display 7 ; In the 7-bit environment (use 8 for VMS)
set terminal vt320 ; Emulate DEC VT320
set terminal roll off ; Keep rolled-back screens where they are
set terminal wrap on ; Tell Kermit to do line wrap
set terminal tabs at 1:8 ; Set tabs at every 8 spaces
set terminal cursor underline ; Underline cursor (rather than block)
;
; The following accounts for the new scan code generated by Space bar
; on the LK250 keyboard under version 3.13.
;
if eq \v(keyboard) 250 if > \v(version) 312 set key \313 \32

źą Àw q PC WÏ Îž ŒÝœ ÒÀ Ûö ÑÆÈ . ]A :

¿ ŒÝ œãÜ rÿ Õø Œ (Terminal Display) : 7 Bits
¿ ŒÝ œňą (Terminal Type) : VT320
¿ sr ÿìF Éž ãÜ èą (Terminal Roll-Back) : ãÜó åÐØ eì m (Off)
¿ Tğø Œ WL Ã õ ď@ C e śi ã Ür Æ (Ò : 80 Î 132) ÉBz è ą (Terminal Wrap) :

NW LąÀ ¿Ü U@ æãÜ (On)

¿ õæ ä (Tab) žśd ìm (Terminal Tabstops) : 1:8 (śdó 1, 9, 17, 25, 33, 41, ... ěì m ) ¿ åÐ Îň (Cursor Style) : şu Î (Underline)

Ãw q LK250 ňŒÝ œž Sí\ àä .

ÄQŋ ąÀ :

COMMENT - Personalized initialization file
;
if > \v(version) 311 if not inpath MSCUSTOM.INI goto fin
take mscustom.ini

:FIN
echo Smile!

õæ MSCUSTOM.INI (ÏÎÌÛ wÒ lÉ ) , Üź MSKERMIT.INI wõæź ę .

I.2 MSCUSTOM.INI

MSCUSTOM.INI řÏ ÎÌÛ wÒ lÉ , |b MSKERMIT.INI ÐÇtÎ Òl Éõ æźę áQ ł

Jõ æ . źÉŒO ýÏ ÎÌ Ûæw qž tÎÑ ÆÈ Îĺ řRO .

ôÛñ ÈjÇ H MS-DOS KERMIT 3.13 ľč Ñž MSCUSTOM.INI ÏÎ ÌÛ wÒl Éí C pU . řKó ąú _č , Äú ÉŒ P ąú æù èą i æ . Ð‘ N : żÉŒ ď\ hą Àą H ùÑ Å ź (;) íÜ , RčźÅ źá YiÏ Î .

Ä@ą À :

; FILE MSCUSTOM.INI.
;
; Sample individual customization file for MS-DOS Kermit 3.11 or 3.12.
; Make any desired changes, and then store this file in the same directory
; as your MSKERMIT.INI initialization file.
;
; Author: Christine M. Gianone, Septermber 1992.
; Revised: June 1993.
;
echo Customizations...

źąÀ ï MSCUSTOM.INI ÏÎ Ì Ûw Ò lÉ @@ š ű . Ð‘ N : żÒl É ÈA Î ó 3.11 ľğ áž MS-DOS KERMIT ď .

ÄGą À :

COMMENT - Serial communication settings

set port 1 ; Use COM1 (this is the default anyway)
do vax ; Set parameters for talking to a VAX
                                ; (these are Kermit’s defaults anyway)

; The following commands are commented out, shown as samples only.
; Replace with settings appropriate for your connection.
;
; set speed 9600 ; Transmission speed
; set parity even ; Even parity, 7 data bits
;
; If the remote host or service does NOT use parity, you should use the
; following two settings:
;
; set parity none
; set terminal display 8

źą ÀÎ óH ÆÚœ Pů ÝDœ su É] wÑÆ , ]A : qT ðs ź (Comm. Port No.) , RS-232 űś žÇ ét Œ , Pìè ą (Parity) , ÎŒ Ýœã Ür ÿø Œ ě .

ÄTą À :

COMMENT - Printing
;
; Uncomment the following command if you don’t have a printer. That is,
; remove the semicolon from the left margin. This command prevents
; host-initiated printing operations from hanging your PC. If desired, you
; can also have print operations directed to a file (replace "nul" by a file
; name, for example "set printer c:\logs\printer.log").
;
; set printer nul

źą ÀÎ óń É (Redirect) Lí œéX šG ÜÉ ŒÎä L Device É .

Ä|ą À :

COMMENT - TCP/IP network configuration.
;
; To use TCP/IP connections, replace the dummy values below with appropriate
; values for your network (consult your network manager) and uncomment the SET
; TCP/IP commands. Better yet, just SET TCP/IP ADDRESS BOOTP, period.
;
; SET TCP/IP ADDRESS 123.123.123.123 ; My PC’s numeric IP address
; SET TCP/IP SUBNETMASK 255.255.255.0 ; My physical network’s subnet mask
; SET TCP/IP DOMAIN FOO.BAR.EDU ; My network’s domain name
; SET TCP/IP GATEWAY 123.123.123.1 ; My network gateway’s IP address
; SET TCP/IP PRIMARY-NAMESERVER 123.123.123.2 ; Primary nameserver’s address
; SET TCP/IP SECONDARY-NAMESERVER 123.123.123.3 ; fallback nameserver address
; SET TCP/IP BROADCAST 255.255.255.255 ; My network’s broadcast address

; TELNET macro for making TCP/IP connections.
; "TELNET <ip-host-name-or-address>" makes a new TCP/IP connection.
; "TELNET" (by itelf) resumes the current TCP/IP connection.
; \%1 = IP host name or address
; \%2 = TCP port
; \%3 = terminal type (optional)
;
define telnet -
  set flow none,-
  set port tcp \%1 \%2,-
  if def \%3 set term type \%3,-
  pause 0, if succ c

źą À Î ó H TCP/IP Ïì ô ô P ů Ý D œ s u É ] w Ñ Æ , ]A : PC ž IP Address, sub-

netmask, domain WÙ , gateway Î nameserver ž IP Address, HÎ broadcast žd ò , Ãw q

telnet ĺřR O .

Äŋą À :

COMMENT - Key definitions. Uncomment these if desired, and/or add your own.
;
; set key \96 \27 ; Exchange ESC and
; set key \27 \96 ; accent-grave keys during terminal emulation.

źą ÀÎ ó] wSí \à ä .

Äżą À :

COMMENT - Default terminal emulation screen color is blue on white.
;
; Uncomment and change to suit your tastes.
; See pages 81-82 of "Using MS-DOS Kermit" for color information.
;
; set terminal color 0 34 47 ; Terminal color is blue on white.

źą ÀÎ ó] wÃõ Câ .

ÄCą À :

COMMENT - File transfer preferences.
;
;;; Uncomment and/or change to suit your needs.
;
; set block 3 ; Block check 3 = 16-bit CRC.
; set window 2 ; 2 Window slots.
; set receive packet-length 1000 ; Packet length is governed by receiver.

; Macros for transferring files in text and binary mode...
;
define bsend set file type binary, send \%1 \%2 ; SEND in binary mode
define tsend set file type text, send \%1 \%2 ; SEND in text mode
define bget remote set file type binary, get \%1 ; GET in binary mode
define tget remote set file type text, get \%1 ; GET in text mode

źą ÀÎ ó ] w É ŒÇ e Û ö Ñ Æ , ]A : żù rÿ ø Œ , Sliding Window ÆØ , ţň Ê ] ø Œ ě . Ãwq Ç e åÆ r æ ąÉ ž ĺ řR O tsend Î tget , PÇe G i ìæ ą É žĺ ř R O

bsend Î bget .

ÄKą À :

COMMENT - Character set preferences. Change to suit your needs.
;
; set terminal character-set latin1 ; Remote host’s character set
; set transfer character-set latin1 ; File transfer character set
; set file character-set cp850 ; PC’s local character set

źą ÀÎ ó] wŒÝ œÒ ÀÎÉ ŒÇ eÒ ÏÎž rř (Character Set) .

ÄEą À :

; user-defined initialization
take userdef.ini

echo

õæ USERDEF.INI (ÑÒÒ lÉ ) , Üź MSCUSTOM.INI wõæ źę .

I.3 USERDEF.INI

USERDEF.INI ř ASPAC pž Ò č Ñ ž Ñ Ò Ò l É , źÉ Œ ď ï U t Î Ñ Æ È ž w q ą H ż

åU Ûö ź‘ žž eř Ç , i@ř zÛ æŒ ï MSCUSTOM.INI Éž ÑÒ . USERDEF.INI íC pU , řKóą ú_ č , ÄúÉ ŒP ąúæ ùè ąiæ .

šűą À :

;; Project ASPAC
;; MS Kermit User-defined initialization demo file
;; Academia Sinica Computing Center, Taiwan, ROC
;; 12/05/94

źą Àï USERDEF.INI ÑÒ Òl É@ @šű .

Ä@ą À :

;; Part 1 : Modem Connection Settings

set port 2
set speed 19200

źąÀ Îó HÆ Úœ Pů ÝD œs uÉ ]w ÑÆ , NPÆ Úœ sţ žq Tð sź (Comm. Port

No.) ]w ř Com2 , RS-232 űś žÇ étŒ ]w ř 19200 bps .

ÄGą À :

;; Part 2 : TCP/IP Connection Settings

set tcp/ip address 140.109.1.254 ;; local host ip address
set tcp/ip subnetmask 255.255.255.0 ;; default setting
set tcp/ip broadcast 140.109.1.255 ;; broadcast range
set tcp/ip primary-nameserver 140.109.1.10 ;; nameserver ip address
set tcp/ip gateway 140.109.1.10 ;; gateway ip address
set tcp/ip domain sinica.edu.tw ;; domain name
set tcp/ip host gate.sinica.edu.tw ;; set default host

źą À Î ó H TCI/IP Ïì ô ô P ů Ý D œ s u É ] w Ñ Æ , äď Subnetmask, Broadcast,

Nameserver, Gateway, Domain ě] w È ą H þ | ř æ ì , PC ž IP Address şÑ z ž t Î Þ

zÌ áP , ÐV zž tÎ ÞzÌ SSÝ ÛöÑ ÆÈ áA ÏÎ , _h NoÍ Yń ù~ .

ÄTą À :

;; Part 3 : ZMODEM Program Macro Definition

define rz run dsz F ha on port 2 G rz -r \%1
define sz run dsz F ha bo port 2 G sz \%1 \%2 \%3 \%4 \%5 \%6 \%7 \%8 \%9

źą Àw q rz Î sz âĺřR O , Yz L DSZ.COM ÉŒ , ÐH anonymous ftp èą Ü gate.sinica.edu.tw ďž /aspac/msdos-tools/zmodem Øý Uú o .

Ä|ą À :

;; Part 4 : Terminal Emulation Settings

set terminal type vt220

źą ÀN ŒÝ œňą ïÜ ř VT220 .

Äŋą À :

;; Part 5 : File Transfer Settings

set send packet-length 9024
; set receive packet-length 9024 ; maximun length = 9024 bytes
set receive packet-length 1024
set window 1
set block-check 1

źą À] wP ÉŒÇ eş öžÑ ÆÈ , ]A :

1. eX Ê]ø Œ : ]wř 9024 Bytes (ějÈ ) 2. ţň Ê]ø Œ : ]wř 1024 Bytes (Ìji Ü 9024 Bytes)

3. Sliding Window ÆØ : 1

4. żù rÿø Œ : 1 Bytes

Äżą À :

;; Part 6 : Chinese Environment Settings

set parity none
set terminal character-set transparent
set terminal bytesize 8
set transfer character-set transparent
define trans set term char trans

źą À] wP ďåô Òş öžÑ Æ , ]A :

1. Pì èą (Parity) : None (He\ 8-bit êÆÇ e ) 2. ŒÝœ Ï Î žr ř (Terminal Character Set) : Transparent (čÏ Î ôó r ř , č@ ô ó r řà ń ) 3. ŒÝ œãÜ rÿ Õø Œ (Terminal Bytesize) : 8 Bits (He\ 8-bit êÆÇ e ) 4. ÉŒ Ç e Ï Î ž r ř (Transfer Character Set) : Transparent (čÏ Î ô ó r ř , č@ ô ó rř àń )

Ãwq trans ĺř RO , Hõ æ set terminal character-set transparent . trans R OA Îó õ æ ä L né á A Ï Î ďå É , oX { ÃX ž ą Î , HN ŒÝ œ Ï Î r řń s ] w ř

Transparent .

ÄCą À :

;; Part 7 : Keyboard Mapping

take vt300x.ini ; take enhanced keyborad mapping initialization file
set key \5493 \Kdump ; Ctrl-End key for dump graphic screen to TEKPLTxx.TIF

;; end of user-defined initialization file

źąÀ õæ VT300X.INI žž e , Ï 101 äž PC @ř VT tC ŒÝ œ É , Ærä (Keypad) à şâØ č P \à , VT300X.INI žąú Ð Ñ \þ ý J . tw q Ctrl-End HOý Ã õW X { ž ÏÎ , Üź USERDEF.INI wõæ źę .

100 APPENDIX I. MSKERMIT.INI, MSCUSTOM.INI, AND USERDEF.INI

Appendix J

VT300.INI and VT300X.INI

żþ ýN ąú VT300.INI ÒlÉÎ ASPAC pžŒ ïğ VT300X.INI žtğ .

J.1 VT300.INI

VT300.INI ÒlÉž Øž ř : N PC žąÀ äL ]wř VT220 Î VT320 ŒÝœ ž\ àä , bs

ţä LD œÉ , iÏÎ VT220 Î VT320 ŒÝ œW žSí \à ä , Ïzóş Äv aź ĺu@ . ż Òl É q ‘ b MSCUSTOM.INI ÏÎ Ì Û w Ò l É õ æ š ô e , ÏÎ take RO õ æ ; bż å ďhb USERDEF.INI ÑÒÒ lÉ õ æš ôe ÏÎ take ROõ æ . VT300.INI AÎ ó 3.10 ľ ğá ž MS-DOS KERMIT ď .

@ë PC ÏÎž äL jhř 88 äÎ 101 äâØ , źâØ äL b VT300.INI Òl Éď ą[ H wq , ýØeÏ Îž äL H 101 äÌ řh , ]ź ÈN 101 äąÀ ąú ğ .

VT300.INI ÒlÉž ež íCp U , řKó ąú _č , Äú ÉŒ Pąú æù èą iæ .

Ä@ą À :

; VT300.INI - MS-DOS Kermit keyboard setup for DEC VT200-300 series terminals.
; Originally contributed by Kevin Lowey, University of Saskatchewan Computing
; Services. For use only with MS-DOS Kermit 3.10 or later. Adapted for new
; features of version 3.10 at Columbia University. Further modified by Kevin
; Lowey to correct some problems in the original keyboard layouts.
;
; Two different setups are provided, one for the 101-key extended PC keyboard,
; one for the 88-key original keyboard. This file (when used with MS-DOS
; Kermit 3.10 or later) automatically determines which kind of keyboard you
; have. See the comments in the file to learn the key assignments.
;
; NOTE: The key assignments made by this file comprise just one of an infinite
; number of possible arrangements. No two people agree about how best to map
; DEC keyboard keys to IBM PC keys. If the mappings done by this file do not
; suit your taste, feel free to make modifications.

źą Àą ú VT300.INI žAÎ ľ ż (AÎ ó 3.10 ľğ á ž MS-DOS KERMIT ď ) ÎA Î w é (AÎó 88 äÎ 101 äâØ äL ) , Ãi ÑÏÎ ÌÛ æó ï , HÅX zžÝ D .

ÄGą À :

; Usage: TAKE VT300.INI (or put this command in your MSKERMIT.INI file).
; If you will be emulating a VT220 or VT320 terminal on a DEC VAX computer
; VMS 5.0 or later, and you have an 8-bit (no-parity) connection to it,
; also uncomment the following command:
;
;;; SET TERMINAL DISPLAY 8

; If you need to use the ISO Latin-1 character set in the 7-bit environment
; with the host sending Shift-In/Shift-Out (Ctrl-N/Ctrl-O) to switch between
; ASCII and special characters, uncomment the following command:
;
;;; set terminal character-set latin1 G1

źą À ą ú õ æ VT300.INI žè ą : ib MSKERMIT.INI , MSCUSTOM.INI žš ô B [ J

take VT300.INI Ôz Y i . Y@ ř DEC VAX Î VMS 5.0 ž VT220 Î VT320 ÏÎÉ , ş

NŒÝ œ ãÜ r ÿ (Terminal Display) øŒ ] wř 8 Bits . YÏÎ ISO Latin-1 rř , şN Œ Ý œÏ Îr ř] wř latin1 .

ÄTą À :

; Standard VT terminal settings
;
set term tabs at 1:8

źą À] wõ æä (Tab Key) žśdì mř 1, 9, 17, 25, 33, ... ěìm .

Ä|ą À :

; Version test
;
if not < version 310 goto systest
echo VT300.INI requires MS-DOS Kermit Version 3.10 or later.
pop

; System check
;
:systest
if eq "\v(platform)" "IBM-PC" goto kbtest
echo VT300.INI is only for IBM PCs, PS/2s, and compatibles.
pop

; Automatic keyboard test
;
:kbtest
if equal "\v(keyboard)" "88" goto kb88
if equal "\v(keyboard)" "101" goto kb101
echo Keyboard type "\v(keyboard)" not supported by VT300.INI.
pop

źą ÀÎ óú ÕUC õæ øó : @ . MS-DOS KERMIT O_ ř 3.10 ğáž ľż ? G . wéŋ x O_ ř IBM PC Ûeq č ? T . äL ř 88 äÎ 101 ä ? HMw O_A Î VT300.INI .

Äŋą À :

:kb101
echo VT300.INI: IBM-101 Extended Keyboard Setup...
;
; ***************** IBM-101 Extended Keyboard Definitions ******************
; IBM KEY DEC KEY
; Numeric Keypad
; There are two definitions for each of the numeric keypad keys,
; one for when <NUM-LOCK> is pressed, and one when it isn’t.
set key \850 \kkp0 ; Keypad 0 (Numlock) Keypad 0
set key \338 \kkp0 ; Keypad 0 (Normal) Keypad 0
set key \847 \kkp1 ; Keypad 1 (Numlock) Keypad 1
set key \335 \kkp1 ; Keypad 1 (Normal) Keypad 1
set key \848 \kkp2 ; Keypad 2 (Numlock) Keypad 2
set key \336 \kkp2 ; Keypad 2 (Normal) Keypad 2
set key \849 \kkp3 ; Keypad 3 (Numlock) Keypad 3
set key \337 \kkp3 ; Keypad 3 (Normal) Keypad 3
set key \843 \kkp4 ; Keypad 4 (Numlock) Keypad 4
set key \331 \kkp4 ; Keypad 4 (Normal) Keypad 4
set key \844 \kkp5 ; Keypad 5 (Numlock) Keypad 5
set key \332 \kkp5 ; Keypad 5 (Normal) Keypad 5
set key \845 \kkp6 ; Keypad 6 (Numlock) Keypad 6
set key \333 \kkp6 ; Keypad 6 (Normal) Keypad 6
set key \839 \kkp7 ; Keypad 7 (Numlock) Keypad 7
set key \327 \kkp7 ; Keypad 7 (Normal) Keypad 7
set key \840 \kkp8 ; Keypad 8 (Numlock) Keypad 8
set key \328 \kkp8 ; Keypad 8 (normal) Keypad 8
set key \841 \kkp9 ; Keypad 9 (Numlock) Keypad 9
set key \329 \kkp9 ; Keypad 9 (Normal) Keypad 9

set key \334 \kkpminus ; Keypad + Keypad -
set key \2382 \kkpcoma ; ALT Keypad + Keypad ,
set key \851 \kkpdot ; Keypad . (Numlock) Keypad .
set key \339 \kkpdot ; Keypad . (normal) Keypad .
set key \4365 \Kkpenter ; Keypad Enter Keypad Enter

                          ; F1 PF1 (default Kermit)
                          ; Use GOLD.COM to make Num Lock work as F1/PF1/Gold.
set key \4399 \kPF2 ; Keypad / PF2
set key \311 \kPF3 ; Keypad * PF3
set key \330 \kPF4 ; Keypad - PF4 Key

źą À } l ž set key RO ą Î ó ] w 101 äž ä L ď , US í ä ž \ à . žý Ñ Ì k è žÆ r ä (KeyPad) }l ] w . Èo ‘ N ž O : VT300.INI N . Î 0 Ü 9 äw q ř : čŒ ö U

NumLock P_ , ąï şÜ VT220 Î VT320 ŒÝ œW Ær äž . Î 0 Ü 9 ä .

Äżą À :

; F1 thru F20 keys IBM DEC
set key \1374 \kholdscrn ; Control-F1 F1
set key \1375 \kprtscn ; Control-F2 F2
set key \1376 \khelp ; Control-F3 Setup
; No Definition ; Control-F4 F4

; Default mapping ; F1 Gold (PF1)
; Default Mapping ; F2 PF2
; Default Mapping ; F3 PF3
; Default Mapping ; F4 PF4
set key \319 \kbreak ; F5 Break
set key \320 \Kdecf6 ; F6 DEC F6
set key \321 \Kdecf7 ; F7 DEC F7
set key \322 \KdecF8 ; F8 DEC F8
set key \323 \KdecF9 ; F9 DEC F9
set key \324 \KdecF10 ; F10 DEC F10
set key \389 \kdechelp ; F11 DEC Help
set key \390 \kdecdo ; F12 DEC Do
set key \2408 \kdecF11 ; Alt-F1 F11
set key \2409 \kdecF12 ; Alt-F2 F12
set key \2410 \kdecF13 ; Alt-F3 F13
set key \2411 \kdecF14 ; Alt-F4 F14
set key \2412 \kdechelp ; Alt-F5 Help (F15)
set key \2413 \kdecdo ; Alt-F6 Do (F16)
set key \2414 \kdecF17 ; Alt-F7 F17
set key \2415 \kdecF18 ; Alt-F8 F18
set key \2416 \kdecF19 ; Alt-F9 F19
set key \2417 \kdecF20 ; Alt-F10 F20

źą À N F1 Ü F12 \à ä P Ctrl Î Alt XÎ , ÀO w qř VT220 Î VT320 ŒÝœ W ž F1 Ü F20 \à ä .

ÄCą À :

; Cursor Keypad
set key \4434 \kdecinsert ; Gray Insert DEC Insert Here
set key \4435 \kdecRemove ; Gray Delete DEC Remove
set key \4423 \kdecFind ; Gray Home DEC Find
set key \4431 \KdecSelect ; Gray End DEC Select
set key \4425 \KDecPrev ; Gray Page Up DEC Prev Screen
set key \4433 \KDecNext ; Gray Page Down DEC Next Screen
pop

źą Àw qr ÀäP Ær ä (KeyPad) ğąž żÓ GrayKey ž\à . Üźw źĺ wq 101 äž äL ď , USí äž \à .

íÚÌ ÏÎ VT300.INI Ò] wž \à É , |o{ UCâ ÓÝ D :

1. ìż b PC žÆ r ä (KeyPad) ď , |ĳ öU NumLock äÉ , 7 Î 1 äiÀ O @ ř Home Î End \àä ; 9 Î 3 äiÀ O@ ř PgUp Î PgDn \àä ; 8 , 2 , 4 , 6 äiÀ O@ řW , U , ł , k|Ó èV ä ; 0 Î . äi ÀO @ř Ins Î Del \àä . gL VT300.INI žńs ] wá , oÇ \à čàć F , ï PC ÏÎ ÌÓ ěD ‘čK .

2. öU GrayKey ďž PgUp Î PgDn ä , Lkõ æš ű (Scroll Up/Down) ž\ à .

òó H W â I ì ] , ASPAC pž ï VT300.INI Òl É ď @ Œ £ , Ææ ì _ o Ç ä ì ş ž \ à , óO čÍ F VT300X.INI oÓ sž ÒlÉ .

J.2 VT300X.INI

VT300X.INI ÒlÉ ž Dn \ à bó : ì_Æ r ä (KeyPad) b|ĳ ö U NumLock äÉì ş ž

\à , ÎÏ GrayKey ďž PgUp Î PgDn äãş WUš ű (Scroll Up/Down) ž\ à .

nźĺ Wz\ à , ÈÝŒ ïU Câą ÀY i :

1. Nì VT300.INI ÒlÉ ď , ï KeyPad ď . äÎ 0 Ü 9 äb| ĳ öU NumLock ä (Ðù ş Normal žą À ) žwqğ e[ W ; ÅźÏä ĺř ùÑ Óčõ æ .

2. Nì VT300.INI ÒlÉ ď , ï GrayKey ď PgUp Î PgDn äžwq ğe [W ; Åź Ïä ĺ řùÑ Ó č õæ . t~[ W set key n4425 nkupscn Î set key n4433 nkdnscn âR OHÀ Oõ æ PgUp Î PgDn .

gLW z Œï L {á , PC WÆ rä (KeyPad) b|ĳ öU NumLock äÉ : 7 Î 1 äi À O @ř Home Î End \à ä , ¡ţõ Ü ÌW ű ÎÌ Uű ; 9 Î 3 äi À O@ ř PgUp Î PgDn \ àä , bW @ űÎ U @ű ą šÊ ; 8 , 2 , 4 , 6 äi À O@ ř W , U , ł , k| Ó èV ä ; 0 Î . ä iÀ O@ ř Ins Î Del \àä . B GrayKey ďž PgUp Î PgDn äçi bW @ű ÎU@ űą š Ê .

VT300.INI ÒlÉž Äŋ ąÀb VT300X.INI Œï řpU ÒC :

:kb101
echo VT300.INI: IBM-101 Extended Keyboard Setup...
;
; ***************** IBM-101 Extended Keyboard Definitions ******************
; IBM KEY DEC KEY
; Numeric Keypad
; There are two definitions for each of the numeric keypad keys,
; one for when <NUM-LOCK> is pressed, and one when it isn’t.
set key \850 \kkp0 ; Keypad 0 (Numlock) Keypad 0
; set key \338 \kkp0 ; Keypad 0 (Normal) Keypad 0
set key \847 \kkp1 ; Keypad 1 (Numlock) Keypad 1
; set key \335 \kkp1 ; Keypad 1 (Normal) Keypad 1
set key \848 \kkp2 ; Keypad 2 (Numlock) Keypad 2
; set key \336 \kkp2 ; Keypad 2 (Normal) Keypad 2
set key \849 \kkp3 ; Keypad 3 (Numlock) Keypad 3
; set key \337 \kkp3 ; Keypad 3 (Normal) Keypad 3
set key \843 \kkp4 ; Keypad 4 (Numlock) Keypad 4
; set key \331 \kkp4 ; Keypad 4 (Normal) Keypad 4
set key \844 \kkp5 ; Keypad 5 (Numlock) Keypad 5
; set key \332 \kkp5 ; Keypad 5 (Normal) Keypad 5
set key \845 \kkp6 ; Keypad 6 (Numlock) Keypad 6
; set key \333 \kkp6 ; Keypad 6 (Normal) Keypad 6
set key \839 \kkp7 ; Keypad 7 (Numlock) Keypad 7
; set key \327 \kkp7 ; Keypad 7 (Normal) Keypad 7
set key \840 \kkp8 ; Keypad 8 (Numlock) Keypad 8
; set key \328 \kkp8 ; Keypad 8 (normal) Keypad 8
set key \841 \kkp9 ; Keypad 9 (Numlock) Keypad 9
; set key \329 \kkp9 ; Keypad 9 (Normal) Keypad 9

set key \334 \kkpminus ; Keypad + Keypad -
; set key \2382 \kkpcoma ; ALT Keypad + Keypad ,
set key \851 \kkpdot ; Keypad . (Numlock) Keypad .
; set key \339 \kkpdot ; Keypad . (normal) Keypad .
set key \4365 \Kkpenter ; Keypad Enter Keypad Enter

                          ; F1 PF1 (default Kermit)
                          ; Use GOLD.COM to make Num Lock work as F1/PF1/Gold.
set key \4399 \kPF2 ; Keypad / PF2
set key \311 \kPF3 ; Keypad * PF3
set key \330 \kPF4 ; Keypad - PF4 Key

VT300.INI ÒlÉž ÄC ąÀb VT300X.INI Œï řpU ÒC :

; Cursor Keypad
set key \4434 \kdecinsert ; Gray Insert DEC Insert Here
set key \4435 \kdecRemove ; Gray Delete DEC Remove
set key \4423 \kdecFind ; Gray Home DEC Find
set key \4431 \KdecSelect ; Gray End DEC Select
; set key \4425 \KDecPrev ; Gray Page Up DEC Prev Screen
; set key \4433 \KDecNext ; Gray Page Down DEC Next Screen
set key \4425 \kupscn ; Page Up
set key \4433 \kdnscn ; Page Down
pop

VT300X.INI ÒlÉ ÈŒï ÏÎ 101 äž ąÎ , Yz ÏÎ 88 äž äL , ÐÑÒż þý žą ú

Ûæ Œï .

110 APPENDIX J. VT300.INI AND VT300X.INI

Appendix K

References

1. Tutorial Guide :

Using MS-DOS KERMIT , 2nd edition, by Christine M. Gianone, published by Digital Press, Bedford, MA(1992), or Prentice Hall International, 1992.

2. Files:

¿ KERMIT.HLP : Guide to MS-DOS KERMIT 3.13
¿ KERMIT.UPD : Update file
¿ KERMIT.BWR : Beware File

112 APPENDIX K. REFERENCES

Appendix L

MS-DOS KERMIT Command List

żþý N MS-DOS KERMIT ž‘Î R OC X , Ãš æą úC @ RO ž Nq , HKÖ tÏ Î . ‘ ÎR OÌ \à Àþą úp U : (ÈCX UR OWÙ , ibRO á[ W ? , úo On-Line Help ) 1. œ} MS-DOS KERMIT :

¿ exit Î quit : œ} MS-DOS KERMIT
¿ push : ÈÉœ } MS-DOS KERMIT, ^ì MS-DOS

2. P MS-DOS şö žR O :

¿ cd : ïÜu @Ø ý
¿ cls : Mče ś
¿ delete : Rč ÉŒ
¿ dir : CX Y@Ø ýď žÉ Œ
¿ type : dÝÉ Œž e
¿ space : dÝ Øe ÒB ÏÐW iÎ Åąj p
¿ more : vű ãÜ Tğ
¿ copy : Æs ÉŒ
¿ rename : óïÉ ŒW Ù
¿ run : õæü wž MS-DOS RO

3. dSS uWš Uą ú (On-Line Help) ÎtÎ ÑÆ] wą Î :

¿ help Î ? : dSSu WšU ąú Tğ (þąž e )
¿ show ? : dSS MS-DOS KERMIT ÑÆØ þ
¿ show status : dSS MS-DOS KERMIT ńnÑÆ ]w ąÎ
¿ show communications : dSS qTÛ öÑ Æ]w ąÎ
¿ show terminal : dSSŒÝ œÒ ÀÛö ÑÆ ]w ąÎ
¿ show protocol : dSSÉ ŒÇ eÛ öÑÆ ]w ąÎ
¿ show file : dSS ÉŒÇ eÛ öÑ Æ]w ąÎ
¿ show statistics : dSSÉ ŒÇ eÛ öÎp ÆÚ
¿ show server : dSSø AźÛ öÑ Æ]w ąÎ
¿ show macro : dSSĺ řw q

4. ]w qTÑ Æ :

¿ set port : ]wqT ðs ź
¿ set speed : ]wÆ ÚœÇ et Œ
¿ set parity : ]wPì èą
¿ set duplex : ]w huè ą
¿ set handshake : ]w Handshake èą
¿ set flow-control : ]w yq śî èą

5. TCP/IP Ïì ôôÑ Æ] w :

¿ set port tcp/ip : ]w q Tô ô ř TCP/IP Ïì ô ô , Ãüw ý s ţ ů Ý D œW Ù Î

IP ì}

¿ set tcp/ip address : ]w PC ž IP ì}
¿ set tcp/ip host : ]w ůÝ Dœž IP ì}
¿ set tcp/ip primary-nameserver : ]w NameServer ž IP ì}
¿ set tcp/ip gateway : ]w Gateway ž IP ì}
¿ set tcp/ip domain : ]w Domain WÙ
¿ set tcp/ip subnetmask : ]w Subnetmask ÆØ
¿ set tcp/ip broadcast : ]w Broadcast dò

6. Pů ÝDœ su Îœ u :

¿ connect : iJŒ ÝœÒ Àe ś , ÇÆP ůÝD œs u
¿ hangup : b MS-DOS KERMIT ďÁ _Pů ÝD œžs u

7. ŒÝ œÒÀ :

¿ set prompt : ïÜ MS-DOS KERMIT čÜ Åź
¿ set terminal : ]w ŒÝ œň ą
¿ set display (set terminal bytesize) : ]wŒÝ œã Üìÿ Õ (byte) øŒ
¿ set terminal display : ]w ŒÝ œãÜ ìÿ Õ (byte) øŒ
¿ set terminal color : ]wŒ Ýœ ÒÀ ÃõC â
¿ set rollback : ]w ŒÝœ ^š (Scrollback) űÆ
¿ set terminal rollback : }Ò / öňÏ ÎXR OÐ é (EMS) äľ^ šű Æ\à
¿ set terminal expanded-memory : }Ò / öňÏ ÎX ROÐ é (EMS) \à
¿ set terminal wrap : ]w Wø Cår ÁÎ èą
¿ set key : ]w Hot Key
¿ log session : }l OýŒ Ýœ ÒÀL {
¿ close session : śîOý ŒÝ œÒ ÀL{
¿ replay : ńÐ ¡ñw Oý ğŒÝ œÒ ÀL {
¿ Ctrl-]-? Î Alt-h : dSS Èœ ňA RO (Escape-Level Mode Cmd) ąú
¿ Ctrl-]-c Î Alt-x : ÛŒÝœ ÒÀ ňAÈ œÜ MS-DOS KERMIT
¿ Ctrl-]-f Î Ctrl-End : Oý ŒÝ œÒÀ eś že
¿ Ctrl-]-h : Á_Pů ÝD œsu
¿ Ctrl-]-m : }Ò / öň ňA C
¿ Ctrl-]-p : ÛŒÝœ ÒÀ ňAÈ œÜ MS-DOS
¿ Ctrl-]-r Î Alt-r : }lO ýŒÝ œÒ ÀL{
¿ Ctrl-]-q Î Alt-q : śîO ýŒ Ýœ ÒÀL {
¿ Ctrl-]-s Î Alt-s : dSSŒ Ýœ ÒÀÎ su ňA žUÛ öÑ Æ]w È
¿ Alt-n : bčP Session ąÁń (ÈAÎ ó TCP/IP ôô ď )
¿ Alt- - : bårŒ Ýœ PÏ ÎŒÝ œğ ąÁń
¿ Alt-= : Reset ŒÝœ

8. Cí œśî :

¿ set printer : RedirectCíœé XÜ äL ]Æ

9. ÉŒ Çe :

¿ send : eX @Ó ÎhÓ ÉŒ
¿ receive : ţň@ ÓÎh ÓÉ Œ
¿ Ctrl-x Î x : śîi æď žÉŒ Çe , õæU@ ÓÉ ŒÇe
¿ Ctrl-z Î z : śîi æď ÎH ážÉ ŒÇ e
¿ Ctrl-c Î c : śîi æď ÎH ážÉ ŒÇ e , Ã^ì MS-DOS KERMIT
¿ set file type : ]wÉŒ Çe æą
¿ set file collision : ]wÉW ÛP ÉBz èą
¿ set incomplete : ]w ÉŒÇ eć ÑÉB zè ą
¿ set destination : RedirectÉŒÇ eš GÜä L] Æ
¿ set transfer character-set : ]w rřà ń\ à
¿ set block-check : ]wż ùrÿ øŒ
¿ set retry : ]w ÉŒÇ eć ÑÉń eÿ Æ
¿ set receive packet-length : ]wţň Ê] žø Œ (Byte)
¿ set send packet-length : ]w eXÊ ]ž øŒ (Byte)
¿ set window : ]w Sliding Window jp

10. øA ź :

¿ server : ÒÊø Aź \à
¿ send : eX @Ó ÎhÓ ÉŒ ÜůÝ KERMIT øAź
¿ get : ÛůÝ KERMIT øAź WúU @Ó ÎhÓ ÉŒ
¿ mail : NÉŒ H E-Mail Îąe Üů ÝÏ ÎÌ
¿ bye : öň ůÝ Dœ ž KERMIT øA ź , ÃÁ_ su
¿ finish : öň ůÝ Dœ ž KERMIT øA ź , ^ì KERMIT
¿ remote help : dSSů ÝD œž KERMIT øAź\ àą ú
¿ remote cd : ïÜ bů Ýžu @Ø ý
¿ remote delete : Rčů Ýž ÉŒ
¿ remote dir : CXů ÝY@ Øý ďžÉ Œ
¿ remote host : õæ ůÝt ÎR O
¿ remote message : Çe@T ğÜ ůÝD œ
¿ remote print : bůÝ Cíœ CL üwž e
¿ remote set : ]wů Ý KERMIT øA źÑÆ È
¿ remote space : dSSů ÝÏ Ðži ÎÅ ą (Free Space) jp
¿ remote type : dÝ ůÝ ÉŒž e
¿ remote who : dSSůÝ Dœ Øe nJž ÏÎ ÌêÆ
¿ enable : }ÒůÝ KERMIT øA ź\à
¿ disable : öň ůÝ KERMIT øAź\ à

11. ĺř Î Script Programming:

¿ define : wq ĺř Îü wÜÆ È
¿ assign : üw ÜÆÈ
¿ take : õæ Script ÉŒ
¿ echo : Nrê ãÜ óÃõ W
¿ comment : ùÑ æ
¿ ask, askq, getok : æÍą (Interactive) éJ ÜÆÈ
¿ input, output : ÑqT ðéJ / éX
¿ increment, decrement : W[ , îÖÜÆ È
¿ if not : YÔ zř D , h ....
¿ if =, if <, if > : Yě ó / pó / jó YÆ , h ....(Ær ñû )
¿ if equal, if lgt, if llt : Yěó / pó / jóY rê , h .... (år ñû )
¿ if success, if failure : YÔzĺ SS / čĺ SS , h ....
¿ goto, :<label> : jćõ D (Unconditional Jump) ÜÐO (Label) B
¿ open, read, write, close : }Ò / ł / g / öňÉ Œ
¿ pause, mpause, wait : Èś Script ÉŒ žõ æ
¿ stop, end : šô Script ÉŒžõ æ

118 APPENDIX L. MS-DOS KERMIT COMMAND LIST

Index

*, 31, 40, 66 :, 44 ?, 5, 7, 9, 31, 40, 66, 113 #, 31

AA, 69, 71, 72 Abridged Command, 9 Alias Name, 17, 54 Alt- -, 29 Alt-h, 27 Alt-n, 29 Alt-q, 27, 58 Alt-r, 27, 58 Alt-s, 27 Alt-x, 20, 24, 27–31, 33, 35, 38, 57, 65, 69, 70, 72, 85 ask, 42, 44 assign, 42, 44 at, 12, 54 atd, 13 atdp, 13 atdt, 12, 13, 54, 70, 72 ats0, 69, 72 AUTOEXEC.BAT, 82 Automatic Connection, 11, 15, 16, 21, 23, 29, 54 Background Color, 46, 59 bget, 95 Binary File, 34 BIOS, 12 Block-Check, 64 Broadcast, 52 bsend, 95 bye, 35–37, 66, 71

C-KERMIT, 1, 2, 30, 31, 35, 65, 68

C-Kermit>, 31 capture, 85 cat, 85 CD, 69, 71, 72 cd, 45 Character Set, 75 chcp, 84 Chinese Environment, 75 close, 42 close session, 57, 58 cls, 45 com1, 49, 50, 52, 54 com2, 12, 16, 38, 49, 50, 52, 54 com3, 49, 54 com4, 49, 54 comment, 17, 44 Communication Device, 49 Communication Port, 12 connect, 12, 16, 19–23, 25, 28, 30, 38, 54, 57, 66, 69, 70, 72, 85 copy, 45, 84 count, 42 CRC-32, 39 Ctrl-], 26 Ctrl-]-?, 26 Ctrl-]-c, 20, 24, 27–31, 33, 35, 38, 57, 65, 69, 70, 72, 85 Ctrl-]-f, 27, 57, 58 Ctrl-]-h, 20, 24, 27 Ctrl-]-m, 27 Ctrl-]-p, 27, 28 Ctrl-]-q, 27, 58 Ctrl-]-r, 27, 58 Ctrl-]-s, 27 Ctrl-End, 58, 99 Ctrl-h, 12 decrement, 42 define, 41, 42, 44 delete, 45 dial, 15–19, 51, 52, 54, 88 dialfile, 82 dialnum, 82 DIALUPS.TXT, 15–17, 51, 52, 82, 88 dir, 45 disable, 68, 71–73 Domain Name, 52 Download, 30, 38 DSZ.COM, 38, 39, 98

echo, 26, 44 edit, 84 editfile, 82 editor, 82 EMM386, 46 enable, 68, 71 end, 44 Environment Variable, 16, 44 Error-Checking, 62, 64, 86 errstp, 86 Escape-Level Mode, 26 Escape-Level Mode Command, 26, 27, 57 exit, 6, 19, 28, 30, 45 Expression, 44 External Modem, 49, 50

F1, 105 F12, 105 fatal, 86 File Transfer, 30, 47 File Transfer Message, 32 File Transfer Quality, 64 File Transfer Speed, 61 finish, 37, 66, 71 Flow Control, 55 Foreground Color, 46, 59 FTP site, 2 Full-Duplex, 55, 56

Gateway, 52 get, 35–37, 66

GNUPLOT, 29 goto, 42, 44 Graphic Terminal, 29 GrayKey, 106, 107

Half-Duplex, 55, 56 Hangup, 11, 20, 21, 24 hangup, 20, 24, 27 Hangup Abruptly, 20, 24 Hangup Gradually, 20, 24 HAYES, 12, 13, 15, 16, 52, 53, 82 HAYES.SCR, 15–18, 51, 52 help, 5, 7, 9

IBM Fullscreen Mode, 56, 83 IBM Linemode, 56, 83 if, 44 if =, 42, 44 if equal, 44 if exist, 44 if failure, 44 if inpath, 44, 79 if lgt, 44 if llt, 44 if success, 44 if <, 42, 44 if >, 42, 44 increment, 42 input, 42 Install MS-DOS KERMIT, 49 Internal Modem, 49, 50 Interrupt File Transfer, 34 ISO Latin-1, 102

KERMIT, 1 kermit, 5, 6, 30, 35, 65, 68 kermit -F, 78 KERMIT Protocol, 30 KERMIT.BWR, 111 KERMIT.EXE, 51 KERMIT.HLP, 46, 111 KERMIT.SCN, 27, 58 KERMIT.UPD, 111 KeyPad, 105–107 label, 42, 44 list, 88 Local Area Network, 11, 12, 21, 49, 50, 56 log session, 57, 58, 85 log session prn, 58 Log Terminal Emulation Session, 27, 57 logout, 20, 24, 36, 37, 66

Macro, 15, 41 mail, 66 MATLAB, 29 Modem, 11, 25, 26, 30, 35, 38, 42, 49, 50, 52– 54 modem, 16, 82 Modem Cable, 49 Modem Eliminator, 50 more, 45, 84 MS-DOS Command, 45, 84 MS-DOS KERMIT, 1, 2, 30 MS-DOS KERMIT Command, 113 MS-Kermit>, 5 MSCUSTOM.INI, 5, 11, 15, 16, 21, 23, 38, 41, 51–53, 77, 79, 91, 92, 101, 102 MSKERMIT.INI, 5, 11, 15, 21, 34, 45, 51, 52, 75, 77–79, 102 MSKERMIT.PCH, 51, 80 MSR313.PCH, 51, 80

Name Server, 52 Network Cable, 49, 50 not, 42, 44 Null Modem Adapter, 50 Null Modem Cable, 49, 50, 56 NumLock, 105–107

OH, 69, 71, 72 On-Line Help, 7, 26, 113 open, 42 output, 42

Packet Length, 61, 86 Parity, 17, 26, 55, 75 PATH=, 51 PPP, 13 Pulse, 13, 17 push, 6, 45

QEMM, 46 quit, 6, 19, 30, 66, 71

read, 42 READ.ME, 51 receive, 30–34 remote cd, 67 remote delete, 67, 68 remote dir, 67, 71 remote help, 66, 67, 70, 73 remote host, 67 remote host finger, 67 remote login, 71, 73 remote logout, 71 remote message, 71 remote print, 67 remote set, 67 remote set file type, 37, 67 remote space, 67 remote type, 67, 71 remote who, 67, 71 rename, 45, 84 replay, 58 Retry Number, 64, 86 RS-232-C, 49 RTS/CTS, 55, 56 run, 45 RZ, 38 rz, 38–40, 98

Screen Color Table, 46, 59 Script File, 42 Script Programming, 41, 42 send, 30, 31, 33–37, 41, 66 Serial Port, 12, 49, 50, 52, 54 Server, 30, 31, 35, 37, 65 server, 35, 36, 65, 68, 69, 71, 72 Session, 26, 29 SESSION.LOG, 58 sessions, 12, 13, 16, 54 set attributes, 89 set block-check, 62, 64, 95, 98 set destination, 47 set dialfile, 82 set duplex, 55, 83 set editor, 82 set file collision, 34, 89 set file type, 34, 37, 41 set flow-control, 55, 83 set handshake, 55, 83 set incomplete, 47 set input case, 89 set input echo, 89 set input timeout, 89 set key, 47, 83, 105, 107 set modem, 16, 53, 82 set parity, 55, 75, 83, 93, 99 set port, 12, 15–17, 50, 53, 54, 69, 70, 72, 93, 97 set port tcp/ip, 21–23, 54 set printer, 47 set prompt, 46 set receive packet-length, 61, 89, 95, 98 set retry, 64 set rollback, 46 set send packet-length, 61, 98 set server login, 71–73 set speed, 12, 15, 16, 53, 54, 69, 70, 72, 93, 97 set tcp/ip address, 21, 22, 53, 94, 97 set tcp/ip broadcast, 21, 53, 94, 97 set tcp/ip domain, 21, 53, 94, 97 set tcp/ip gateway, 21, 53, 94, 97 set tcp/ip host, 54, 97 set tcp/ip primary-nameserver, 21, 53, 94, 97 set tcp/ip secondary-nameserver, 94 set tcp/ip subnetmask, 21, 53, 94, 97 set terminal, 90 set terminal bytesize, 83, 99 set terminal character-set, 75, 99, 102 set terminal color, 46, 59 set terminal control, 83 set terminal cursor, 90 set terminal display, 75, 90, 93, 102 set terminal expanded-memory, 46 set terminal rollback, 90 set terminal tabstops at, 90 set terminal type, 46, 98 set terminal wrap, 46, 90 set transfer character-set, 75, 89, 99 set window, 63, 89, 95, 98 sh com, 9 sh te, 9 show, 8, 9 show ?, 9 show communications, 9 show file, 9 show key, 9 show macro, 9, 52 show protocol, 9 show server, 9 show statistics, 9 show status, 9 show terminal, 9, 26 show translation, 9 Sliding Window, 61, 63, 86 SLIP, 13 Start MS-DOS KERMIT, 5 Status Line, 25–27 Step-By-Step Connection, 11, 12, 21, 54 stop, 44 Stop-And-Wait, 63 Subnetmask, 52 Switch to MS-DOS, 28 Switch to MS-DOS KERMIT, 28 SZ, 38 sz, 38–40, 98

take, 38, 42, 43, 101, 102 TCP/IP, 11, 12, 21, 23–26, 29, 30, 35, 38, 42, 49, 52–54 TEKPLT##.TIF, 58 Tektronic, 29 telapi, 84 telnet, 23, 29, 52, 54, 94 telnet -8, 12, 14, 16, 54 terminal, 12, 13, 16, 54 Terminal Emulation, 12, 13, 19, 22, 23, 25, 46 Terminal Server, 13, 14, 17–20 Terminal Type, 26, 29

Text File, 34, 75, 85 Text Terminal, 29 tget, 95 top, 20 Touch Tone, 12, 13, 16, 17 trans, 99 tsend, 95 type, 45

Unconditional Jump, 44 UNIX, 56, 83 Upload, 33, 40 Usage Flow of KERMIT, 4 USERDEF.INI, 64, 77, 96, 97, 101

Variable, 44 VAX/VMS, 56, 83 VT100, 29 VT220, 29, 101, 102, 105 VT300.INI, 101–103, 105–109 VT300X.INI, 99, 107–109 VT320, 101, 102, 105

write, 42

XON/XOFF, 55, 56

ZMODEM Protocol, 30, 38, 40