EXECUTE LIST
<26,1,30,10>				!ENABLE CRATE
<24,1,30,9>				!REMOVE INHIBIT
<26,1,20,0>				!ALLOW DISPLAY LAM
MOVE BUFFER TO <16,1,20,0> WHENLAM	!WRITE ADDRESS
! ADDRESS = IX + IY*'100
DO					!INFINITE DO LOOP
MOVE BUFFER TO <16,1,20,1> WHENLAM	!WRITE A CHAR STRING
ENDDO					!STOP WHEN BUFFER EXHAUSTED
